(footprint "L_FNR6045S" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Inductor, _FNR6045S (https://atta.szlcsc.com/upload/public/pdf/source/20190327/C168103_C4D77756DA9C915521E5EFF252700EB5.pdf)")
  (tags "Inductor 6.0x6.0x4.5mm")
  (attr smd)
  (fp_text reference "REF**" (at 0 -4.4) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 9ffbd17c-f244-42ba-b69e-5b5ed65b1fb5)
  )
  (fp_text value "L_FNR6045S" (at 0 4.5) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6f937bdd-036f-40fd-aced-cdac7ebf4e00)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp bc9510f0-452c-4464-bfb7-b4fabe67b091)
  )
  (fp_line (start -3.3 -3) (end -3.3 -2.04)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 690df306-c9dc-458f-badf-541faa8d9853))
  (fp_line (start -3.3 1.95) (end -3.3 3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6a040469-627f-4b4d-ac49-817dff71ebd7))
  (fp_line (start -3.3 3) (end 3.3 3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9b6b8df6-319e-473f-90b4-2767032fea5a))
  (fp_line (start 3.3 3) (end 3.3 1.96)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9ed683b7-dabc-497d-8b0f-4d974ea5e08b))
  (fp_line (start 3.31 -3) (end -3.3 -3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 236dce24-91d3-406d-8d8d-c3debc1b18d9))
  (fp_line (start 3.31 -2.04) (end 3.31 -3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9083480a-825c-4208-91ab-c23c122661d1))
  (fp_line (start -4.46 -3.55) (end -4.46 3.55)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c902e1e2-bfd7-4d41-a86b-3966359c56cd))
  (fp_line (start -4.46 -3.55) (end 4.46 -3.55)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f0f4e979-bcff-4c5c-add7-8c380559318f))
  (fp_line (start 4.46 3.55) (end -4.46 3.55)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp cb9a0af9-5759-461c-bf0e-593d82392229))
  (fp_line (start 4.46 3.55) (end 4.46 -3.55)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a9d4f7e1-e77d-493e-9bb5-f161a3e80762))
  (fp_line (start -3.7 -3.3) (end -3.7 3.3)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e9d45662-d4fe-4936-967e-734e0b7b8971))
  (fp_line (start -3.7 3.3) (end 3.7 3.3)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d681014e-32e2-446b-9f6b-b01bbeb2372c))
  (fp_line (start 3.7 -3.3) (end -3.7 -3.3)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5d2ed84c-ef67-4fbf-9223-c7ad0e45cfe8))
  (fp_line (start 3.7 3.3) (end 3.7 -3.3)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6d2ea214-0c42-411a-8195-81e2ff77800e))
  (pad "1" smd rect (at -2.25 0) (size 1.7 5.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 2db8b6a1-ce1a-4372-b530-114fc71b89e8))
  (pad "2" smd rect (at 2.25 0) (size 1.7 5.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 36b0ba70-f9ae-43c7-867b-8a0ce7f14104))
  (model "E:/Wrk/pcb/kicad/tj-kicad-lib/3d/MWSA0603S.STEP"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
