(footprint "HANBO_SNO-1470_NanoSIM" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "卡托式 NanoSIM卡 卡座(https://atta.szlcsc.com/upload/public/pdf/source/20221209/04BB929FB70345A9F67DFFD9215825AB.pdf)")
  (tags "NanoSIM")
  (property "Sheetfile" "文件： EVB_Air780E_V1.5.kicad_sch")
  (property "Sheetname" "")
  (property "Value1" "SMC-202-7")
  (attr smd)
  (fp_text reference "REF**" (at 0.65 -16.7 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp fc745ada-e9c2-40b2-be91-6a64e69e4121)
  )
  (fp_text value "HANBO_SNO-1470" (at 0.15 -6.7 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4e0820f4-3f0b-49cc-8125-243c2a8b03c6)
  )
  (fp_line (start -6.35 -13.45) (end -6.35 -12.7)
    (stroke (width 0.2) (type default)) (layer "F.SilkS") (tstamp 07ebc0b8-48f5-4019-943a-a9635a24f24a))
  (fp_line (start -6.35 -10.7) (end -6.35 -1.75)
    (stroke (width 0.2) (type solid)) (layer "F.SilkS") (tstamp b9244581-1d27-4c88-8956-c35cb970d45b))
  (fp_line (start -5.95 -15.85) (end 0 -15.85)
    (stroke (width 0.2) (type solid)) (layer "F.SilkS") (tstamp de2887e0-028b-4cf3-8b7f-6320e84183e4))
  (fp_line (start 0 0) (end -6 0)
    (stroke (width 0.2) (type solid)) (layer "F.SilkS") (tstamp 9ad259e5-6403-4b30-800d-1d6b80f415bf))
  (fp_line (start 0 0) (end 6 0)
    (stroke (width 0.2) (type solid)) (layer "F.SilkS") (tstamp 5f5ebef9-69d3-4022-bd21-82646a87a9b4))
  (fp_line (start 5.95 -15.85) (end 0 -15.85)
    (stroke (width 0.2) (type solid)) (layer "F.SilkS") (tstamp 0428d5a8-b1f7-4ff7-ba19-213dfcebae18))
  (fp_line (start 6.35 -13.45) (end 6.35 -12.7)
    (stroke (width 0.2) (type default)) (layer "F.SilkS") (tstamp d94b47fe-ca28-4e9d-b158-b46392304c57))
  (fp_line (start 6.35 -10.7) (end 6.35 -1.75)
    (stroke (width 0.2) (type solid)) (layer "F.SilkS") (tstamp f44bdcfa-a8cf-47a9-a13a-df61c5071621))
  (fp_arc (start -6.35 -15.5) (mid -6.247488 -15.747488) (end -6 -15.85)
    (stroke (width 0.2) (type default)) (layer "F.SilkS") (tstamp 4dd45f6c-27f5-46c5-8da8-f6944863085a))
  (fp_arc (start 6 -15.85) (mid 6.247488 -15.747488) (end 6.35 -15.5)
    (stroke (width 0.2) (type default)) (layer "F.SilkS") (tstamp 95ff4f15-c887-4b85-897d-4b0c2473bef6))
  (fp_line (start -7.6 1.6) (end -7.2 1.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d3e3c2b7-90d9-423c-b051-4c578e9ea55b))
  (fp_line (start -7.6 3.2) (end -7.6 1.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 343bea67-139a-4b4d-a307-25cb08b5f2eb))
  (fp_line (start -7.2 -16.4) (end 7.2 -16.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f83b8008-7ab1-49cc-81d9-1a3187af074a))
  (fp_line (start -7.2 1.6) (end -7.2 -16.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 46ded05f-c300-4b66-9182-28bc0075f451))
  (fp_line (start 7.2 -16.4) (end 7.2 1.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp eb79d520-50a3-49c6-b3c0-5af5f31bed18))
  (fp_line (start 7.2 1.6) (end 7.6 1.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 76f7e912-4540-483b-acd9-ebe8c371db03))
  (fp_line (start 7.6 1.6) (end 7.6 3.2)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f3583ede-8482-4307-af49-c13a4210009f))
  (fp_line (start 7.6 3.2) (end -7.6 3.2)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp db05233c-4daf-4ff3-8572-43ed4187e69a))
  (fp_line (start -7.15 1.85) (end -6 1.85)
    (stroke (width 0.05) (type default)) (layer "F.Fab") (tstamp 4e490ec1-f1b1-4649-8172-55829fc4e40e))
  (fp_line (start -7.15 2.9) (end -7.15 1.85)
    (stroke (width 0.05) (type default)) (layer "F.Fab") (tstamp 579ccdfe-c709-43a6-be53-76af2ee5f47a))
  (fp_line (start -7.15 2.9) (end 7.15 2.9)
    (stroke (width 0.05) (type default)) (layer "F.Fab") (tstamp ada16d87-6261-447e-9fc8-613f976897f2))
  (fp_line (start -6 1.85) (end -6 0)
    (stroke (width 0.05) (type default)) (layer "F.Fab") (tstamp 309b095a-3e86-49bd-866d-95d57e5521c4))
  (fp_line (start 6 1.9) (end 6 0)
    (stroke (width 0.05) (type default)) (layer "F.Fab") (tstamp 4777b087-e591-4e8c-a59d-1e74b6aded15))
  (fp_line (start 7.15 1.9) (end 6 1.9)
    (stroke (width 0.05) (type default)) (layer "F.Fab") (tstamp 995b483f-85fb-4de5-b4ae-f0f8e9a78b57))
  (fp_line (start 7.15 2.9) (end 7.15 1.9)
    (stroke (width 0.05) (type default)) (layer "F.Fab") (tstamp 6cffdee2-e68a-4845-86a5-0d908c7f5bed))
  (pad "8" smd rect (at 6.5 -0.7 270) (size 1.7 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp bd5c0535-005e-472b-ac5a-1ec27f1e5bfd))
  (pad "9" smd rect (at 6.5 -11.7 270) (size 1.7 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 697977f0-8fe1-44ed-b40d-b59979faeda8))
  (pad "10" smd rect (at 6.5 -14.45 270) (size 1.7 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 6a520c9d-c0e6-4ad2-8459-b7af302035bb))
  (pad "11" smd rect (at -6.5 -14.45 270) (size 1.7 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 4cdc2e11-4c8a-4dab-9baa-5150d54145b8))
  (pad "12" smd rect (at -6.5 -11.7 270) (size 1.7 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 67356bab-b91e-4f06-a510-51a46c58e6b1))
  (pad "13" smd rect (at -6.5 -0.7 270) (size 1.7 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 64cda8a0-73be-40cf-b70f-38bf86fff7bc))
  (pad "C1" smd rect (at -2.54 -6.92) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 5cda6697-15f1-4402-9337-4d62612abf81))
  (pad "C2" smd rect (at 0 -6.92) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 8dab1880-d29f-4b63-ba8b-986c70392458))
  (pad "C3" smd rect (at 2.54 -6.92) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp cc60ec5f-d2b2-43aa-ba6c-6c8b2ec29c30))
  (pad "C5" smd rect (at -2.54 -5.1) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 170cd873-e2b5-40f8-8a47-a49daac41720))
  (pad "C6" smd rect (at 0 -5.1) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp c2c6b158-31be-46e8-81d1-d0ae8ed1f3dd))
  (pad "C7" smd rect (at 2.54 -5.1) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp c2ece3c5-630f-47f3-9015-e16f1d027db6))
  (pad "CD" smd rect (at 1.27 -12.71) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp f4bff81e-d05b-4065-85bc-92b996f95a9d))
  (zone (net 0) (net_name "") (layer "F.Cu") (tstamp 31d70b3d-2225-4f59-8c15-4ea7b6946e38) (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy -3.34 -10.12)
        (xy -1.74 -10.12)
        (xy -1.74 -11.62)
        (xy -3.34 -11.62)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (tstamp 6b30e6e1-f4ec-4c6b-88d7-240e3eade719) (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy -3.34 -2.5)
        (xy -1.74 -2.5)
        (xy -1.74 -4)
        (xy -3.34 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (tstamp d32c6c52-1b33-415b-a635-1d8dd20c94a7) (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy -0.8 -10.12)
        (xy 0.8 -10.12)
        (xy 0.8 -11.62)
        (xy -0.8 -11.62)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (tstamp 56290f11-d3d6-420f-b425-8049d6438d03) (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy -0.8 -2.5)
        (xy 0.8 -2.5)
        (xy 0.8 -4)
        (xy -0.8 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (tstamp 5ee0724f-0d7d-46a2-8b9e-5b98dfbcaac7) (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 0.17 -13.8)
        (xy 2.37 -13.8)
        (xy 2.37 -15.1)
        (xy 0.17 -15.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (tstamp 20d329a7-fd9c-48c8-9545-ae6bd4bee40d) (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 1.74 -10.12)
        (xy 3.34 -10.12)
        (xy 3.34 -11.62)
        (xy 1.74 -11.62)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (tstamp dc0831da-eb2f-4da1-8b38-1a4a162117bf) (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 1.74 -2.5)
        (xy 3.34 -2.5)
        (xy 3.34 -4)
        (xy 1.74 -4)
      )
    )
  )
)
