(module Potentiometer_Bourns_3296W_Vertical (layer F.Cu) (tedit 5CE34CFB)
  (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
  (tags "Potentiometer vertical Bourns 3296W")
  (fp_text reference REF** (at -2.54 -3.66) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Potentiometer_Bourns_3296W_Vertical (at -2.54 3.67) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center 0.955 1.15) (end 2.05 1.15) (layer F.Fab) (width 0.1))
  (fp_line (start -7.305 -2.41) (end -7.305 2.42) (layer F.Fab) (width 0.1))
  (fp_line (start -7.305 2.42) (end 2.225 2.42) (layer F.Fab) (width 0.1))
  (fp_line (start 2.225 2.42) (end 2.225 -2.41) (layer F.Fab) (width 0.1))
  (fp_line (start 2.225 -2.41) (end -7.305 -2.41) (layer F.Fab) (width 0.1))
  (fp_line (start 0.955 2.235) (end 0.956 0.066) (layer F.Fab) (width 0.1))
  (fp_line (start 0.955 2.235) (end 0.956 0.066) (layer F.Fab) (width 0.1))
  (fp_line (start -7.425 -2.53) (end 2.345 -2.53) (layer F.SilkS) (width 0.12))
  (fp_line (start -7.425 2.54) (end 2.345 2.54) (layer F.SilkS) (width 0.12))
  (fp_line (start -7.425 -2.53) (end -7.425 2.54) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.345 -2.53) (end 2.345 2.54) (layer F.SilkS) (width 0.12))
  (fp_line (start -7.6 -2.7) (end -7.6 2.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start -7.6 2.7) (end 2.5 2.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.5 2.7) (end 2.5 -2.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.5 -2.7) (end -7.6 -2.7) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at -3.175 0.005) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 1.3 2.3) (end 1.3 0.7) (layer F.SilkS) (width 0.12))
  (fp_circle (center 1.3 1.5) (end 2.1 1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -6 -2.5) (end -6 -2) (layer F.SilkS) (width 0.12))
  (fp_line (start -6 -2) (end 1 -2) (layer F.SilkS) (width 0.12))
  (fp_line (start 1 -2) (end 1 -2.5) (layer F.SilkS) (width 0.12))
  (pad 1 thru_hole rect (at 0 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -2.54 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -5.08 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
