(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "GD32E230C8T6" (pin_names (offset 1.27)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -2.54 49.53 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "GD32E230C8T6" (id 1) (at -2.54 46.99 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm" (id 2) (at 31.75 -5.08 0)
      (effects (font (size 1.27 1.27) italic))
    )
    (property "Datasheet" "http://www.gd32mcu.com/data/documents/shujushouce/GD32E230xx_Datasheet_Rev1.3.pdf" (id 3) (at 1.27 -48.26 0)
      (effects (font (size 1.27 1.27)))
    )
    (symbol "GD32E230C8T6_1_1"
      (rectangle (start -60.96 45.72) (end 60.96 -45.72)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin power_in line (at 68.58 -10.16 180) (length 7.62)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 40.64 0) (length 7.62)
        (name "PA0-WKUP/USART0_CTS,USART1_CTS,CMP_OUT,I2C1_SCL,ADC_IN0,CMP_IM6,RTC_TAMP1,WKUP0" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 38.1 0) (length 7.62)
        (name "PA1/USART0_RTS,USART1_RTS,I2C1_SDA,EVENTOUT,TIMER14_CH0_ON,ADC_IN1,CMP_IP" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 35.56 0) (length 7.62)
        (name "PA2/USART0_TX,USART1_TX,TIMER14_CH0,ADC_IN2,CMP_IM7" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 33.02 0) (length 7.62)
        (name "PA3/USART0_RX,USART1_RX,TIMER14_CH1,ADC_IN3" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 30.48 0) (length 7.62)
        (name "PA4/SPI0_NSS,I2S0_WS,USART0_CK,USART1_CK,TIMER13_CH0,SPI1_NSSADC_IN4,CMP_IM4" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 27.94 0) (length 7.62)
        (name "PA5/SPI0_SCK,I2S0_CK,ADC_IN5,CMP_IM5" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 25.4 0) (length 7.62)
        (name "PA6/SPI0_MISO,I2S0_MCK,TIMER2_CH0,TIMER0_BRKIN,TIMER15_CH0,EVENTOUT,CMP_OUT,ADC_IN6" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 22.86 0) (length 7.62)
        (name "PA7/SPI0_MOSI,I2S0_SD,TIMER2_CH1,TIMER13_CH0,TIMER0_CH0_ON,TIMER16_CH0,EVENTOUT,ADC_IN7" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 -2.54 0) (length 7.62)
        (name "PB0/TIMER2_CH2,TIMER0_CH1_ON,USART1_RX,EVENTOUT,ADC_IN8" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 -5.08 0) (length 7.62)
        (name "PB1/TIMER2_CH3,TIMER13_CH0,TIMER0_CH2_ON,SPI1_SCK,ADC_IN9" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 68.58 27.94 180) (length 7.62)
        (name "PC13-TAMPER-RTC/RTC_TAMP0,RTC_TS,RTC_OUT,WKUP1" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 -7.62 0) (length 7.62)
        (name "PB2/TIMER2_ETI" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 -27.94 0) (length 7.62)
        (name "PB10/I2C0_SCL,I2C1_SCL,SPI1_IO2,SPI1_SCK" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 -30.48 0) (length 7.62)
        (name "PB11/I2C0_SDA,I2C1_SDA,EVENTOUT,SPI1_IO3" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 68.58 -25.4 180) (length 7.62)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 68.58 -12.7 180) (length 7.62)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 -33.02 0) (length 7.62)
        (name "PB12/SPI0_NSS,SPI1_NSS,TIMER0_BRKIN,I2C1_SMBA,EVENTOUT" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 -35.56 0) (length 7.62)
        (name "PB13/SPI0_SCK,SPI1_SCK,TIMER0_CH0_ON,I2C1_TXFRAME,I2C1_SCL" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 -38.1 0) (length 7.62)
        (name "PB14/SPI0_MISO,SPI1_MISO,TIMER0_CH1_ON,TIMER14_CH0,I2C1_SDA" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 -40.64 0) (length 7.62)
        (name "PB15/SPI0_MOSI,SPI1_MOSI,TIMER0_CH2_ON,TIMER14_CH0_ON,TIMER14_CH1,RTC_REFIN,WKUP6" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 20.32 0) (length 7.62)
        (name "PA8/USART0_CK,TIMER0_CH0,CK_OUT,USART1_TX,EVENTOUT" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 68.58 25.4 180) (length 7.62)
        (name "PC14-OSC32IN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 17.78 0) (length 7.62)
        (name "PA9/USART0_TX,TIMER0_CH1,TIMER14_BRKIN,I2C0_SCL,CK_OUT" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 15.24 0) (length 7.62)
        (name "PA10/USART0_RX,TIMER0_CH2,TIMER16_BRKIN,I2C0_SDA" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 12.7 0) (length 7.62)
        (name "PA11/USART0_CTS,TIMER0_CH3,CMP_OUT,EVENTOUT,SPI1_IO2,I2C0_SMBA,I2C1_SCL" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 10.16 0) (length 7.62)
        (name "PA12/USART0_RTS,TIMER0_ETI,EVENTOUT,SPI1_IO3,I2C0_TXFRAME,I2C1_SDA" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 7.62 0) (length 7.62)
        (name "PA13/SWDIO/IFRP_OUT,SPI1_MISO" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 68.58 35.56 180) (length 7.62)
        (name "PF6/I2C0_SCL,I2C1_SCL" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 68.58 33.02 180) (length 7.62)
        (name "PF7/I2C0_SDA,I2C1_SDA" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 5.08 0) (length 7.62)
        (name "PA14/SWCLK/USART0_TX,USART1_TX,SWCLK,SPI1_MOSI" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 2.54 0) (length 7.62)
        (name "PA15/SPI0_NSS,I2S0_WS,USART0_RX,USART1_RX,SPI1_NSS,EVENTOUT" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 -10.16 0) (length 7.62)
        (name "PB3/SPI0_SCK,I2S0_CK,EVENTOUT" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 68.58 22.86 180) (length 7.62)
        (name "PC15-OSC32OUT" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 -12.7 0) (length 7.62)
        (name "PB4/SPI0_MISO,I2S0_MCK,TIMER2_CH0,EVENTOUT,I2C0_TXFRAME,TIMER16_BRKIN" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 -15.24 0) (length 7.62)
        (name "PB5/SPI0_MOSI,I2S0_SD,I2C0_SMBA,TIMER15_BRKIN,TIMER2_CH1/WKUP5" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 -17.78 0) (length 7.62)
        (name "PB6/I2C0_SCL,USART0_TX,TIMER15_CH0_ON" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 -20.32 0) (length 7.62)
        (name "PB7/I2C0_SDA,USART0_RX,TIMER16_CH0_ON" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 68.58 12.7 180) (length 7.62)
        (name "BOOT0" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 -22.86 0) (length 7.62)
        (name "PB8/I2C0_SCL,TIMER15_CH0" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -68.58 -25.4 0) (length 7.62)
        (name "PB9/I2C0_SDA,IFRP_OUT,TIMER16_CH0,EVENTOUT,I2S0_MCK,SPI1_NSS" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 68.58 -27.94 180) (length 7.62)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 68.58 -15.24 180) (length 7.62)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 68.58 40.64 180) (length 7.62)
        (name "F0-OSCIN/I2C0_SDA" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 68.58 38.1 180) (length 7.62)
        (name "PF1-OSC_OUT/I2C0_SCL" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 68.58 5.08 180) (length 7.62)
        (name "NRST" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 68.58 -40.64 180) (length 7.62)
        (name "VSSA" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 68.58 -33.02 180) (length 7.62)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "SWM181CBT6" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 25.4 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SWM181CBT6" (id 1) (at 0 21.59 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm" (id 2) (at -13.97 -67.31 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://download.s21i.faiusr.com/26573789/0/0/ABUIABA9GAAg-PjOhAYo-pKEngE.pdf?f=%E5%8D%8E%E8%8A%AF%E5%BE%AE%E7%89%B9SWM181%E6%95%B0%E6%8D%AE%E6%89%8B%E5%86%8CV2.03.pdf" (id 3) (at 3.81 -48.26 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SWM181CBT6_0_0"
      (pin bidirectional line (at -40.64 27.94 0) (length 2.54)
        (name "A3/SWDIO" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -40.64 30.48 0) (length 2.54)
        (name "A2/SWCLK" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -40.64 33.02 0) (length 2.54)
        (name "A1" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -40.64 35.56 0) (length 2.54)
        (name "A0/~{WAKEUP}" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 38.1 -10.16 180) (length 2.54)
        (name "XO" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -12.7 180) (length 2.54)
        (name "C1/XI" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -40.64 -35.56 0) (length 2.54)
        (name "VSS33" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -40.64 -30.48 0) (length 2.54)
        (name "VDD33" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -30.48 180) (length 2.54)
        (name "E4/ADC0_CH1/SPI0_CLK" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -40.64 -2.54 0) (length 2.54)
        (name "A15/ADC0_CH1/SPI0_CLK" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -40.64 7.62 0) (length 2.54)
        (name "A11/SEG21/SPI0_CLK" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -40.64 0 0) (length 2.54)
        (name "A14/ADC0_CH2/CP2P/SPI0_MOSI" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -40.64 2.54 0) (length 2.54)
        (name "A13/ADC0_CH3/CP2N/SPI0_MISO" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -40.64 5.08 0) (length 2.54)
        (name "A12/ADC0_CH4/SPI0_CS" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -40.64 -11.43 0) (length 2.54)
        (name "VDD33_ADC0" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -40.64 -16.51 0) (length 2.54)
        (name "ADC0_REFP" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -40.64 -22.86 0) (length 2.54)
        (name "VSS33_ADC0" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -5.08 180) (length 2.54)
        (name "C7/ADC1_CH0N/ADC0_CH5/SEG13/SPI1_CLK" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -2.54 180) (length 2.54)
        (name "C6/ADC1_CH0P/ADC0_CH6/SEG12/SPI1_MOSI" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -25.4 180) (length 2.54)
        (name "D3/SEG17" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -22.86 180) (length 2.54)
        (name "D2/SEG16" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -40.64 10.16 0) (length 2.54)
        (name "A10/SEG20/SPI0_MOSI" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -40.64 -25.4 0) (length 2.54)
        (name "VSS33_ADC1" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -40.64 -19.05 0) (length 2.54)
        (name "ADC1_REFP" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -40.64 -13.97 0) (length 2.54)
        (name "VDD33_ADC1" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -20.32 180) (length 2.54)
        (name "D1/ADC1_CH4N/SEG15" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -17.78 180) (length 2.54)
        (name "D0/ADC1_CH4P/SEG14_" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 0 180) (length 2.54)
        (name "C5/ADC1_CH1N/SEG11/SPI1_MISO" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 2.54 180) (length 2.54)
        (name "C4/ADC1_CH1P/SEG10/SPI1_CS" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 5.08 180) (length 2.54)
        (name "C3/ADC1_CH3N" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 7.62 180) (length 2.54)
        (name "C2/ADC1_CH3P" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 12.7 180) (length 2.54)
        (name "B9/SEG9" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -40.64 12.7 0) (length 2.54)
        (name "A9/SEG19/SPI0_MISO" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 15.24 180) (length 2.54)
        (name "B8/SEG8" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 17.78 180) (length 2.54)
        (name "B7/SEG7" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 20.32 180) (length 2.54)
        (name "B6/SEG6" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 22.86 180) (length 2.54)
        (name "B5/SEG5" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 25.4 180) (length 2.54)
        (name "B4/SEG4" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 27.94 180) (length 2.54)
        (name "B3/CP1P/SEG3" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 30.48 180) (length 2.54)
        (name "B2/CP1N/SEG2" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 33.02 180) (length 2.54)
        (name "B1/SEG1" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 35.56 180) (length 2.54)
        (name "B0/SEG0/BOOT" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -40.64 15.24 0) (length 2.54)
        (name "A8/SEG18/SPI0_CS" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -40.64 17.78 0) (length 2.54)
        (name "A7/COM3" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -40.64 20.32 0) (length 2.54)
        (name "A6/CP0P/COM2" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -40.64 22.86 0) (length 2.54)
        (name "A5/CP0N/COM1" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -40.64 25.4 0) (length 2.54)
        (name "A4/COM0" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "SWM181CBT6_0_1"
      (rectangle (start -38.1 39.37) (end 35.56 -39.37)
        (stroke (width 0.1524) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "SWM181CBT6_1_1"
      (pin input line (at -40.64 -7.62 0) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
