(footprint "UU9.8-Vertical" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 5CFB5536)
  (attr through_hole)
  (fp_text reference "REF**" (at 0 9.5) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6ac38bf0-e7a0-4e7f-aea4-4d669ca3ee50)
  )
  (fp_text value "UU9.8-Vertical" (at 0 -0.5) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 73740860-e445-4583-9312-3be64a0ba97f)
  )
  (fp_line (start -5.5 8) (end -5.5 -8) (layer "F.SilkS") (width 0.12) (tstamp 11ab3ac6-944a-471b-bf0a-b4fe446e5696))
  (fp_line (start -5.5 -8) (end 5.5 -8) (layer "F.SilkS") (width 0.12) (tstamp 1aecf0b1-784b-4145-9f02-43c3f9f13b37))
  (fp_line (start -1 -8) (end -1 8) (layer "F.SilkS") (width 0.12) (tstamp 220f5682-5c12-4c67-987a-54ea734d26c1))
  (fp_line (start 5.5 -8) (end 5.5 8) (layer "F.SilkS") (width 0.12) (tstamp 5e8bad9a-aa35-4151-981c-9465de4bd104))
  (fp_line (start 5.5 8) (end -5.5 8) (layer "F.SilkS") (width 0.12) (tstamp 667a068b-b3fd-422c-a0a7-dd62e92f866b))
  (fp_line (start -5.5 0) (end -1 0) (layer "F.SilkS") (width 0.12) (tstamp 84d04c8e-0548-419e-9152-0375aba60029))
  (fp_line (start 1 8) (end 1 -8) (layer "F.SilkS") (width 0.12) (tstamp 8b0e2a14-58dc-4d3c-95d9-9ee5fea68cfa))
  (fp_line (start 1 0) (end 5.5 0) (layer "F.SilkS") (width 0.12) (tstamp cae6afd4-40cc-4aeb-96e5-b5547b5c7d62))
  (pad "1" thru_hole circle (at -3.5 -4) (size 3 3) (drill 1.27) (layers *.Cu *.Mask) (tstamp 4c1383f2-7d2a-46a9-b270-78e423c8dccf))
  (pad "2" thru_hole circle (at 3.5 -4) (size 3 3) (drill 1.27) (layers *.Cu *.Mask) (tstamp 4b86fe3b-3b53-4cc1-8498-812242e2270e))
  (pad "3" thru_hole circle (at -3.5 4) (size 3 3) (drill 1.27) (layers *.Cu *.Mask) (tstamp b92bbf00-decb-4a8a-93ad-9a39e85d581c))
  (pad "4" thru_hole circle (at 3.5 4) (size 3 3) (drill 1.27) (layers *.Cu *.Mask) (tstamp d0b80d63-a42c-4792-baa6-e00c6f769734))
  (model "E:/Wrk/pcb/kicad/tj-kicad-lib/3d/UU9_8.STEP"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 90 180 90))
  )
)
