(footprint "LED_1206_3216Metric_Pad1.5x1.6mm_Reverse" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "LED SMD 1206 (3216 Metric), Reverse mount,(https://atta.szlcsc.com/upload/public/pdf/source/20180326/C125107_4FC6AAA9C4CB214F6084B48273B556C2.pdf)")
  (tags "LED handsolder")
  (attr smd)
  (fp_text reference "REF**" (at -0.1 -1.7) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ec4580be-7c4f-4abd-bc1e-435c20cf2e86)
  )
  (fp_text value "LED_1206_3216Metric_Pad1.5x1.6mm_Reverse" (at -0.1 1.8) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c019e27c-8c40-47db-b294-c1f6185fadb6)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.8 0.8) (thickness 0.12)))
    (tstamp bfe7e709-4f13-444f-97f0-1f29b7b73d3c)
  )
  (fp_line (start -2.7 -1.3) (end -2.7 1.3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3c27e0b0-6feb-4657-983a-61812ee19906))
  (fp_line (start -2.7 1.3) (end 1.65 1.3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 01276750-d0a2-4c23-927b-ce751f610fbe))
  (fp_line (start 1.65 -1.3) (end -2.7 -1.3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f8f7e630-bfcf-4a22-a68e-81ab6fa51546))
  (fp_line (start -0.9 -0.7) (end -0.9 0.7)
    (stroke (width 0.05) (type solid)) (layer "Edge.Cuts") (tstamp 3cadf6b9-98b4-4ed9-9a59-ce108d56261a))
  (fp_line (start -0.5 1.1) (end 0.5 1.1)
    (stroke (width 0.05) (type solid)) (layer "Edge.Cuts") (tstamp 0a9663a5-26ab-4aba-adae-0f1f58449bc1))
  (fp_line (start 0.5 -1.1) (end -0.5 -1.1)
    (stroke (width 0.05) (type solid)) (layer "Edge.Cuts") (tstamp ffe52cec-074a-495b-8b62-1896a83b7199))
  (fp_line (start 0.9 0.7) (end 0.9 -0.7)
    (stroke (width 0.05) (type solid)) (layer "Edge.Cuts") (tstamp 35d3dd09-d047-468d-b3c5-776a4266bc82))
  (fp_arc (start -0.9 -0.7) (mid -0.782842 -0.982841) (end -0.5 -1.1)
    (stroke (width 0.05) (type solid)) (layer "Edge.Cuts") (tstamp 73d3ea54-d239-411d-8f90-3ec70db293d9))
  (fp_arc (start -0.5 1.1) (mid -0.782842 0.982842) (end -0.9 0.7)
    (stroke (width 0.05) (type solid)) (layer "Edge.Cuts") (tstamp ff639c33-fbb1-42a1-a087-bd954fa45c1b))
  (fp_arc (start 0.5 -1.1) (mid 0.782842 -0.982842) (end 0.9 -0.7)
    (stroke (width 0.05) (type solid)) (layer "Edge.Cuts") (tstamp cf681ff2-75f6-4852-8412-0fa1ae8b997f))
  (fp_arc (start 0.9 0.7) (mid 0.782842 0.982842) (end 0.5 1.1)
    (stroke (width 0.05) (type solid)) (layer "Edge.Cuts") (tstamp 0c39261e-fd6d-4233-9b2a-12aab675ad89))
  (fp_line (start -2.7 -1.3) (end 2.7 -1.3)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 256084e6-6a86-4105-83d9-941b8fe89f7b))
  (fp_line (start -2.7 1.3) (end -2.7 -1.3)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a81e88c8-b908-4b9a-82ae-5878b7af85bc))
  (fp_line (start 2.7 -1.3) (end 2.7 1.3)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp da614eb1-3935-4eac-a6a8-d99a550af09a))
  (fp_line (start 2.7 1.3) (end -2.7 1.3)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5f7edf08-a5ce-48ee-851f-74d913f22762))
  (fp_line (start -1.6 -0.4) (end -1.6 0.8)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 72a825da-037b-4c5c-a990-154921b6b66d))
  (fp_line (start -1.6 0.8) (end 1.6 0.8)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f4db7c07-338f-4acf-b309-cec7eab4ddad))
  (fp_line (start -1.2 -0.8) (end -1.6 -0.4)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 65690f96-f025-47f9-8a87-4177e17926aa))
  (fp_line (start 1.6 -0.8) (end -1.2 -0.8)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5702b3c7-e70a-4be9-95fc-c882c5cec248))
  (fp_line (start 1.6 0.8) (end 1.6 -0.8)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5cbee81b-1037-4032-9a8a-a470bf86b65a))
  (pad "1" smd roundrect (at -1.7 0) (size 1.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1333333333) (tstamp 1a289d09-97f8-47c0-a150-135fda642326))
  (pad "2" smd roundrect (at 1.7 0) (size 1.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1333333333) (tstamp 61cd00f7-e3d5-4670-b611-41bfa2fed8f7))
  (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
    (offset (xyz 0 0 0.5))
    (scale (xyz 1 1 1))
    (rotate (xyz 180 0 0))
  )
)
