(module MountingHole_3.5x5.5mm_Pad_Via (layer F.Cu) (tedit 5F427F94)
  (descr "Mounting Hole 3.5x5.5mm")
  (tags "mounting hole 3.5x5.5mm")
  (attr virtual)
  (fp_text reference REF** (at 0 -4.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value MountingHole_3.5x5.5mm_Pad_Via (at 0 4.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0.4 0.2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_arc (start -1 0) (end -1 -3.5) (angle -180) (layer Cmts.User) (width 0.15))
  (fp_arc (start 1 0) (end 1 3.5) (angle -180) (layer Cmts.User) (width 0.15))
  (fp_line (start 1 -3.5) (end -1 -3.5) (layer Cmts.User) (width 0.15))
  (fp_line (start -1 3.5) (end 1 3.5) (layer Cmts.User) (width 0.15))
  (fp_arc (start -1 0) (end -1 -3.75) (angle -180) (layer F.CrtYd) (width 0.05))
  (fp_arc (start 1 0) (end 1 3.75) (angle -180) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1 3.75) (end 1 3.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1 -3.75) (end 1 -3.75) (layer F.CrtYd) (width 0.05))
  (pad 1 thru_hole oval (at 0 0) (size 9 7) (drill oval 5.5 3.5) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -1 2.625) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -2.856155 1.856155) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -3.625 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -2.856155 -1.856155) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -1 -2.625) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 3.625 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 1 2.625) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 2.856155 1.856155) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 1 -2.625) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 2.856155 -1.856155) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
)
