(footprint "SMA-IPX" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "SMA 内孔 弯头 插座")
  (tags "SMA 内孔 弯头 插座")
  (attr through_hole)
  (fp_text reference "REF**" (at -4.9 -0.2 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp dedaf6a8-95eb-45b6-95d1-4b7f7fc5edc0)
  )
  (fp_text value "SMA-IPX" (at 0 5) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1cdf1a9c-3d39-4c7c-b673-453103ca4a89)
  )
  (fp_line (start -4.1 -4.1) (end -4.1 4.1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f82a3ed9-334e-4f08-908d-abd886e85769))
  (fp_line (start -4.1 -4.1) (end 4.1 -4.1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 899ed846-def4-48fe-b6e4-2f28f81825d2))
  (fp_line (start -4.1 4.1) (end 4.1 4.1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 819c13f6-1a1a-47a9-94e8-3df87dac53c5))
  (fp_line (start -3 -4.1) (end -3 -5.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 73961ac9-7eff-4306-b69d-9a822b9a29c7))
  (fp_line (start -2.5 -5.5) (end -2.5 -5.9)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp b9007bc4-4268-4594-9bf3-d79a440f3855))
  (fp_line (start 0 3.6) (end -0.5 4.1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 85448d24-8159-4a33-93d6-ee1a011c102c))
  (fp_line (start 0.5 4.1) (end 0 3.6)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7acab08a-451c-45b5-8112-229a18290421))
  (fp_line (start 2.5 -5.5) (end 2.5 -5.9)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 7963b6da-c999-4f7d-8417-d717fcb60808))
  (fp_line (start 3 -5.5) (end -3 -5.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 756782ef-0981-4907-b14e-241bc8c00e28))
  (fp_line (start 3 -4.1) (end 3 -5.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 8ea0cf50-50a6-4ad9-98a8-198527733212))
  (fp_line (start 4.1 -4.1) (end 4.1 4.1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 651a735f-b1a6-421a-b15c-e73b03248481))
  (fp_line (start -4.3 -12) (end -4.3 4.3)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ffec2fae-fb0d-4281-9737-b71c36ce9e60))
  (fp_line (start -4.3 -12) (end 4.3 -12)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b21d6a8b-dd13-4d18-9510-c407880a1b26))
  (fp_line (start 4.3 4.3) (end -4.3 4.3)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 205fb57a-f119-4c2a-9419-6724483e058d))
  (fp_line (start 4.3 4.3) (end 4.3 -12)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8e55aaa6-b4fd-4442-8a46-c13fb1e5541c))
  (fp_line (start -3.5 -3.5) (end -3.5 3.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e3e8599f-55ea-4f6a-9989-c440896d2f7c))
  (fp_line (start -3.5 -3.5) (end 3.5 -3.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9151e6f4-687f-4aaf-a803-5e281e9082b3))
  (fp_line (start -3.5 3.5) (end 3.5 3.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f9fb1f1b-f6c6-4769-8fab-99eecf169860))
  (fp_line (start -3 -9.5) (end 3 -10)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0a9b5aaf-7c27-4c79-8cc4-f53066e944fe))
  (fp_line (start -3 -9) (end 3 -9.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e70c2c36-cdcc-4d1a-949c-7894cfcd581b))
  (fp_line (start -3 -8.5) (end 3 -9)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d6aa557e-b426-432c-b79d-8a30884b4a5a))
  (fp_line (start -3 -8) (end 3 -8.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fcd826be-9860-4d40-a152-d2bf43584112))
  (fp_line (start -3 -7.5) (end 3 -8)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c1404bfd-3f97-4b71-bd52-a37626ce4ef9))
  (fp_line (start -3 -7) (end 3 -7.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 793a9c54-4422-4b0a-b8b2-022dfaa281bf))
  (fp_line (start -3 -5.5) (end -3 -3.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3fbefa08-d2a2-4cd5-9e3d-6c788054e961))
  (fp_line (start -2.5 -11.5) (end -2.5 -5.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1d904d11-b2e4-4439-821f-c739de0a1c33))
  (fp_line (start -2.5 -11.5) (end 2.5 -11.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e1edd48b-6130-4cad-8d9e-a6e295700a36))
  (fp_line (start -1 3.5) (end 0 2.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3fb30408-9f0e-40e5-a5ba-9941a09b5cb5))
  (fp_line (start 0 2.5) (end 1 3.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4af43544-7153-4ac4-9144-aeca059d3e41))
  (fp_line (start 2.5 -11.5) (end 2.5 -5.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 93a11536-08c0-4281-99a1-05fdee101ccd))
  (fp_line (start 3 -5.5) (end -3 -5.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ee0deb54-d73e-4038-90fb-d527bccf9739))
  (fp_line (start 3 -5.5) (end 3 -3.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 14a5b21d-556a-4ec5-b6d6-b8f1a6845bfc))
  (fp_line (start 3.5 -3.5) (end 3.5 3.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 24038d72-9abe-4b1f-ac4a-2e93acb3de5b))
  (fp_line (start 4.3 -4.5) (end -4.3 -4.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f78bf029-e907-4428-b53a-981cd964b9ec))
  (pad "1" thru_hole circle (at -2.325 -2.325) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (tstamp 0eac634c-922d-4a77-9d58-375af155e13e))
  (pad "1" thru_hole circle (at -2.325 2.325) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (tstamp 0432e9f9-dc63-4f77-af17-f6fa16bf853f))
  (pad "1" thru_hole circle (at 2.325 -2.325) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (tstamp 337e6b68-a99f-4cd9-9d5e-87942f39cfb3))
  (pad "1" thru_hole circle (at 2.325 2.325) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (tstamp 5fbddc79-89f4-4da2-b086-94f26b96e588))
  (model "${TJ_LIB}/3d/SMA_RF_弯头PCB插座.stp"
    (offset (xyz 0 3.5 6))
    (scale (xyz 1 1 1))
    (rotate (xyz 90 180 0))
  )
)
