(footprint "Air600E_MODULE" (version 20221018) (generator pcbnew)
  locked (layer "F.Cu")
  (property "Sheetfile" "文件： Core_Air600C_A11.kicad_sch")
  (property "Sheetname" "")
  (attr smd)
  (fp_text reference "U4" (at 1.59 -3.84) (layer "F.SilkS")
      (effects (font (size 0.318 0.318) (thickness 0.032)) (justify left))
    (tstamp d0cde441-b188-4a07-bc22-1d1460a3f1e5)
  )
  (fp_text value "Air600E" (at -1.313 14.473) (layer "F.Fab") hide
      (effects (font (size 0.318 0.318) (thickness 0.032)) (justify left))
    (tstamp 4b7c3e4a-4afc-4748-aea5-3eb8d4b23d2c)
  )
  (fp_text user "gge2fd166bdb6936536" (at 0.55 1.525) (layer "Cmts.User") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1d76146c-83ad-4e9c-8b95-0868a919eb27)
  )
  (fp_line (start -11.6 -9.6) (end -11.6 -9.1)
    (stroke (width 0.2) (type solid)) (layer "F.SilkS") (tstamp 334b97c2-48c8-4900-bb55-503d99cfaf0f))
  (fp_line (start -11.6 9.1) (end -11.6 11.1)
    (stroke (width 0.2) (type solid)) (layer "F.SilkS") (tstamp c14e0a46-719d-4bf8-8edc-d7d71c0e5ea2))
  (fp_line (start -11.6 11.1) (end -9.6 11.1)
    (stroke (width 0.2) (type solid)) (layer "F.SilkS") (tstamp 80b2eacf-1cdc-47c7-b133-4747e1e33642))
  (fp_line (start -10.1 -11.1) (end -11.6 -9.6)
    (stroke (width 0.2) (type solid)) (layer "F.SilkS") (tstamp 1fa0ed19-856b-4b44-a88f-dc50541ee191))
  (fp_line (start -9.5 -11.1) (end -10.1 -11.1)
    (stroke (width 0.2) (type solid)) (layer "F.SilkS") (tstamp 1948845d-7762-4afe-bf2f-1089cc1036d6))
  (fp_line (start 10.6 11.1) (end 11.6 11.1)
    (stroke (width 0.2) (type solid)) (layer "F.SilkS") (tstamp 950c5b9a-30d7-4f40-98c1-a49e84cbd87e))
  (fp_line (start 11.6 -11.1) (end 10.7 -11.1)
    (stroke (width 0.2) (type solid)) (layer "F.SilkS") (tstamp baceb84f-174c-4fc6-8efa-3bae21ccd62a))
  (fp_line (start 11.6 -9.2) (end 11.6 -11.1)
    (stroke (width 0.2) (type solid)) (layer "F.SilkS") (tstamp d69e8257-ce37-473e-baea-e61a86a24536))
  (fp_line (start 11.6 11.1) (end 11.6 9.1)
    (stroke (width 0.2) (type solid)) (layer "F.SilkS") (tstamp 15ef7704-c0ec-4e36-a903-95b719d0600d))
  (fp_arc (start -11.407 -11.299) (mid -12.215016 -11.304882) (end -11.40698 -11.303372)
    (stroke (width 0.2) (type solid)) (layer "F.SilkS") (tstamp 385d017c-17c5-47e2-86dd-b2f83dcc0b71))
  (fp_line (start -12.8 -12.4) (end 12.8 -12.4)
    (stroke (width 0.013) (type solid)) (layer "Dwgs.User") (tstamp d95280f7-f869-4f90-9a1f-98d2da37b87d))
  (fp_line (start -12.8 12.4) (end -12.8 -12.4)
    (stroke (width 0.013) (type solid)) (layer "Dwgs.User") (tstamp 5a6b37d9-2240-42ff-9c85-9444f0147bd5))
  (fp_line (start 12.8 -12.4) (end 12.8 12.4)
    (stroke (width 0.013) (type solid)) (layer "Dwgs.User") (tstamp 431e4645-ad95-4cbb-9a1b-9e390a6f9dca))
  (fp_line (start 12.8 12.4) (end -12.8 12.4)
    (stroke (width 0.013) (type solid)) (layer "Dwgs.User") (tstamp f3acb434-b1e6-46ab-baf8-dccb77ba791c))
  (pad "1" smd oval locked (at -11.55 -8.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 1a316e47-5492-4bc5-a86e-c7994884c28a))
  (pad "2" smd oval locked (at -11.55 -7.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp f6fcdcf6-ac2a-4c30-b06e-d24bd79e44dc))
  (pad "3" smd oval locked (at -11.55 -6.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp bb4e55d4-9758-4c31-a60c-d6d6253d371f))
  (pad "4" smd oval locked (at -11.55 -5.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 41414ea0-4a2f-444d-93ed-421f5954034d))
  (pad "5" smd oval locked (at -11.55 -4.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 3dd50adf-416c-4538-ada0-0333d055547d))
  (pad "6" smd oval locked (at -11.55 -3.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 41f06cb8-4596-42d2-9275-3c5a381e3a8a))
  (pad "7" smd oval locked (at -11.55 -2.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp f3000572-2d1c-4384-a1d0-cfa6f13c4dd2))
  (pad "8" smd oval locked (at -11.55 -1.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp ddf92580-26ed-4c16-a335-ebded7101227))
  (pad "9" smd oval locked (at -11.55 -0.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp eadc416a-2610-4458-9c68-bd655dd4382d))
  (pad "10" smd oval locked (at -11.55 0.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 22a89b32-225f-4f8c-b0e7-2f87ccc0a4ab))
  (pad "11" smd oval locked (at -11.55 1.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp b5eb84b3-2843-49f4-9a3b-e500c54d90e8))
  (pad "12" smd oval locked (at -11.55 2.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp c242a715-2310-4f4e-bc56-e2e3e9358ec0))
  (pad "13" smd oval locked (at -11.55 3.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 7b22b5c3-50c0-418c-9b60-601299901187))
  (pad "14" smd oval locked (at -11.55 4.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 10be1947-828c-45af-b246-9db34bc9f5be))
  (pad "15" smd oval locked (at -11.55 5.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 33f2d89a-eee8-4a7a-9430-026abd797794))
  (pad "16" smd oval locked (at -11.55 6.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp db0ec91c-ccfa-4cad-a8f9-f42357c66279))
  (pad "17" smd oval locked (at -11.55 7.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 8587cd29-0a08-4a24-82de-e64068c56e7d))
  (pad "18" smd oval locked (at -11.55 8.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 4bb72bc9-754d-4bc9-83a0-fde2880d14da))
  (pad "19" smd oval locked (at -9 11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp ad601cc4-27d4-48df-ba5c-00847c71cbe9))
  (pad "20" smd oval locked (at -8 11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp c9809706-c2ba-4eff-8710-cf25244a96c3))
  (pad "21" smd oval locked (at -7 11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp b26a2321-2150-4275-b135-7568ac873914))
  (pad "22" smd oval locked (at -6 11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 84030546-683a-49a2-8bcf-b1fd859a280b))
  (pad "23" smd oval locked (at -5 11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp d7417798-256b-4d8b-9cf1-791a84427e30))
  (pad "24" smd oval locked (at -4 11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 78404f1d-5760-48b6-9ad9-b0ee8cf9023c))
  (pad "25" smd oval locked (at -3 11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 7fd7eda2-d8e8-49c7-888e-dfee273b68a4))
  (pad "26" smd oval locked (at -2 11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp aaf1b7be-899f-42a5-b1f8-ecaf1c2ed0c5))
  (pad "27" smd oval locked (at -1 11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp f592edf4-57d5-4637-97ac-2e554a6bbbcd))
  (pad "28" smd oval locked (at 0 11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp fdd85d7b-a781-42fa-a77c-6b0adc369466))
  (pad "29" smd oval locked (at 1 11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 508a7975-4e36-46c2-9f53-246f9157345d))
  (pad "30" smd oval locked (at 2 11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 513ca82e-4bf8-4355-8c21-ed2b47782ca0))
  (pad "31" smd oval locked (at 3 11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp e651dfde-417e-47b9-85c9-465c89334350))
  (pad "32" smd oval locked (at 4 11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 2d18ea37-05a4-4e64-980e-fe2aa205f7d6))
  (pad "33" smd oval locked (at 5 11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 091b3898-30b4-4f1a-8760-137edcdf857b))
  (pad "34" smd oval locked (at 6 11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 0afc38d6-376a-4726-9c1e-e1620249a596))
  (pad "35" smd oval locked (at 7 11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 252644fd-494e-461a-9aa3-d8b990a76e00))
  (pad "36" smd oval locked (at 8 11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 9e9ce94a-b37e-4f4b-9cdf-7dc7871e6b91))
  (pad "37" smd oval locked (at 9 11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp b2d9eb7b-8627-4f7f-aee5-1dbf99516304))
  (pad "38" smd oval locked (at 10 11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 52d8c2ed-32d7-4c97-b27e-8b2c7ee04cd8))
  (pad "39" smd oval locked (at 11.55 8.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 5c139856-8c34-46a7-8986-60f09278a926))
  (pad "40" smd oval locked (at 11.55 7.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 45e5ea95-d7d5-4aee-b882-ff57e1134acc))
  (pad "41" smd oval locked (at 11.55 6.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp a57d784c-41b0-4d4f-8377-f5290ed855f3))
  (pad "42" smd oval locked (at 11.55 5.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp a0e1e7bc-5001-437c-a53f-a0d7c7a22a5f))
  (pad "43" smd oval locked (at 11.55 4.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 4a9f8d3a-218e-4fc6-9027-698cf4c19473))
  (pad "44" smd oval locked (at 11.55 3.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 36fd6a33-1afa-4882-b9b8-0019659c25b0))
  (pad "45" smd oval locked (at 11.55 2.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 3ef0b599-b994-4564-bd66-0fb816b69385))
  (pad "46" smd oval locked (at 11.55 1.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp c51780b2-8d61-4dca-b09d-8c08ca18e656))
  (pad "47" smd oval locked (at 11.55 0.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp c36c9e0a-0eb4-4a81-87a9-a1f68806f695))
  (pad "48" smd oval locked (at 11.55 -0.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 5681f436-447b-4a3e-825e-843c6a694824))
  (pad "49" smd oval locked (at 11.55 -1.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp c53f9ec0-9701-4ff2-8625-bd1f4b8d7c97))
  (pad "50" smd oval locked (at 11.55 -2.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 51bf9605-b0d3-4596-a697-42f8dc0fee3c))
  (pad "51" smd oval locked (at 11.55 -3.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 8659ee6d-c68e-4bac-921e-0cc0a2af2dfc))
  (pad "52" smd oval locked (at 11.55 -4.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp d5de0449-f6e2-4776-bf20-95a798c98912))
  (pad "53" smd oval locked (at 11.55 -5.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 6bb1aa81-c7fe-43f1-9336-0ab080533aa3))
  (pad "54" smd oval locked (at 11.55 -6.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 66321ef6-7a73-4bb1-a1ea-a69f2b1f2f16))
  (pad "55" smd oval locked (at 11.55 -7.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 5e79e4c6-c989-4a9a-ae9f-835eb81b35c4))
  (pad "56" smd oval locked (at 11.55 -8.5) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 181bdfd7-f365-4bdc-9b2a-3cf6628c1509))
  (pad "57" smd oval locked (at 10 -11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp fba35900-8732-4356-836b-ed2d1c9c0899))
  (pad "58" smd oval locked (at 9 -11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 1f8a46d8-4752-4f83-b199-c1cbfa0b9135))
  (pad "59" smd oval locked (at 8 -11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 7d088a3e-1a5a-4ea3-9ca8-20b02f0246ef))
  (pad "60" smd oval locked (at 7 -11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 418d1625-bc6c-459c-81c2-d83e11773b42))
  (pad "61" smd oval locked (at 6 -11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp ced43369-a858-46ec-baa9-75194f30f971))
  (pad "62" smd oval locked (at 5 -11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 0ae572a9-d87f-42af-b1fd-2471eacf9102))
  (pad "63" smd oval locked (at 4 -11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 55617386-7b9d-4379-a3eb-713228848e1a))
  (pad "64" smd oval locked (at 3 -11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp b14d5c67-35b2-483c-a66e-1a55711a1263))
  (pad "65" smd oval locked (at 2 -11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 6efdf8da-f573-417f-9de4-a2c6fffa9361))
  (pad "66" smd oval locked (at 1 -11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp ad99d1ba-e283-413a-a0d1-b79eb0aeb175))
  (pad "67" smd oval locked (at 0 -11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 0cdf064b-f372-4428-b66b-840a8f08ea88))
  (pad "68" smd oval locked (at -1 -11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp afba5634-8288-4050-ba5d-2945f0c45e69))
  (pad "69" smd oval locked (at -2 -11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp b6590a00-1795-4707-8912-e72339c52b24))
  (pad "70" smd oval locked (at -3 -11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 9dca5f6f-1d9f-42b1-aa26-74fcd22dc85a))
  (pad "71" smd oval locked (at -4 -11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 70639f8d-75bb-4bf6-965d-26de8c4b55a5))
  (pad "72" smd oval locked (at -5 -11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 286b0090-0934-42c0-88cd-89c585f19aa6))
  (pad "73" smd oval locked (at -6 -11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 565da9da-1a32-4b79-bfb1-4a6a13062ff4))
  (pad "74" smd oval locked (at -7 -11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 567d4fa9-c1a9-492c-b2c3-36a5e300e5f0))
  (pad "75" smd oval locked (at -8 -11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 92e05425-a991-47c3-9edb-bd997e28feb2))
  (pad "76" smd oval locked (at -9 -11.1 90) (size 1.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 495edc11-fb6d-4b83-9452-bdb18e1c5c18))
  (pad "77" smd rect locked (at -3 -3) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 29f835c4-586d-4fa3-a02e-5ee193b21aa7))
  (pad "78" smd rect locked (at -3 -1) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 4aa242f5-1934-47ae-91bc-a89ec10b9c38))
  (pad "79" smd rect locked (at -3 1) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 193cce7d-6eca-4e0b-96c2-c3b087eb45f5))
  (pad "80" smd rect locked (at -3 3) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp ecb5d767-7f18-4853-a27a-14d376f96bec))
  (pad "81" smd rect locked (at -1 3) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp b8d54dd6-e3ad-4c27-920f-11425be16506))
  (pad "82" smd rect locked (at 1 3) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 3b6b6a13-6568-4b35-ac1d-98f8c65c8444))
  (pad "83" smd rect locked (at 3 3) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 76d5cc99-2e0a-44e4-8730-bfec70bc9648))
  (pad "84" smd rect locked (at 3 1) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 058bd059-db56-411b-9985-59655af65a6f))
  (pad "85" smd rect locked (at 3 -1) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp eb70688c-ff4d-4177-95f2-9a749be1202b))
  (pad "86" smd rect locked (at 3 -3) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 8cb24e09-6ca7-4f43-9d53-0484209534d0))
  (pad "87" smd rect locked (at 1 -3) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 537b6d28-e539-4225-bf1d-d2c06d4e562f))
  (pad "88" smd rect locked (at -1 -3) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 75d00180-10fb-4a4f-97c7-5b22fd445c7b))
  (pad "89" smd rect locked (at -1 -1) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 5dcc1dea-6558-4bb2-9abd-555922b9014e))
  (pad "90" smd rect locked (at -1 1) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 2f59291d-efa1-4119-99e4-80c14a6375c1))
  (pad "91" smd rect locked (at 1 1) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp a186d52e-62a8-4af6-bf6d-0648860de62c))
  (pad "92" smd rect locked (at 1 -1) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp c496d44f-57cc-48d6-b426-994f01b3d5a0))
  (pad "145" smd rect locked (at 7 3) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 15bb957d-fc8a-44d5-b53b-256be04786c2))
  (pad "146" smd rect locked (at 7 1) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 988fbebc-c295-41dd-b910-d067b37fa5a7))
  (pad "147" smd rect locked (at 7 -1) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp b0daeb79-4c8d-4d17-9873-930447091a6c))
  (pad "148" smd rect locked (at 7 -3) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp dfb253cf-7380-4c7a-8cda-027692191108))
  (model "C:/Users/TMALL/Downloads/Air600E_Module.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
