(footprint "Fuse_1812_4532Metric" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 5F68FEF1)
  (descr "Fuse SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
  (tags "fuse")
  (attr smd)
  (fp_text reference "REF**" (at 0 -2.65) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 5245ab1e-f807-46fa-bfbc-2e26056cc998)
  )
  (fp_text value "Fuse_1812_4532Metric" (at 0 2.65) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp cc625dd9-a38e-4ba4-ac1b-fa35e101dccb)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 16ab2d3d-c426-4d07-8935-a8a8bf364aee)
  )
  (fp_line (start -1.386252 1.71) (end 1.386252 1.71) (layer "F.SilkS") (width 0.12) (tstamp b11a6d24-faed-4e48-bdad-30d7e07e9aeb))
  (fp_line (start -1.386252 -1.71) (end 1.386252 -1.71) (layer "F.SilkS") (width 0.12) (tstamp daebee6f-3069-40ab-af86-3f85a99ee0f5))
  (fp_line (start 2.95 1.95) (end -2.95 1.95) (layer "F.CrtYd") (width 0.05) (tstamp 75415e5b-bc5e-4089-9f74-be80b64dfebf))
  (fp_line (start -2.95 -1.95) (end 2.95 -1.95) (layer "F.CrtYd") (width 0.05) (tstamp 9a728c20-882a-42de-a66e-6a4523a5faf4))
  (fp_line (start 2.95 -1.95) (end 2.95 1.95) (layer "F.CrtYd") (width 0.05) (tstamp b9772c96-771a-41db-b29a-6c2e27da7e5d))
  (fp_line (start -2.95 1.95) (end -2.95 -1.95) (layer "F.CrtYd") (width 0.05) (tstamp f3e0f25d-60a8-4e8e-aa48-b1cf2bd27da9))
  (fp_line (start 2.25 1.6) (end -2.25 1.6) (layer "F.Fab") (width 0.1) (tstamp 11a5ba8c-8e32-4d26-b648-8fdea84ea69d))
  (fp_line (start -2.25 -1.6) (end 2.25 -1.6) (layer "F.Fab") (width 0.1) (tstamp 1a1b149c-7792-4db1-90e6-3070799718db))
  (fp_line (start 2.25 -1.6) (end 2.25 1.6) (layer "F.Fab") (width 0.1) (tstamp 29986c84-a25e-4209-bfe4-987b9eb80000))
  (fp_line (start -2.25 1.6) (end -2.25 -1.6) (layer "F.Fab") (width 0.1) (tstamp 509336d2-f34c-43ea-8dbf-3f07d50d2911))
  (pad "1" smd roundrect (at -2.1375 0) (size 1.125 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222) (tstamp 0fa0ef3b-a818-4956-92a3-9d3468164575))
  (pad "2" smd roundrect (at 2.1375 0) (size 1.125 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222) (tstamp 77fdca82-18c5-42c7-b525-1ad163c85f18))
  (model "E:/Wrk/pcb/kicad/tj-kicad-lib/3d/Fuse-1812.STEP"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
