(module LED_RGB_1210 (layer F.Cu) (tedit 5D78A2A5)
  (descr "RGB LED 3.2x2.7mm http://www.avagotech.com/docs/AV02-0610EN")
  (tags "LED 3227")
  (attr smd)
  (fp_text reference REF** (at 0 -2.3) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value LED_RGB_1210 (at 0 2.45) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 -2.3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.6 -0.675) (end -0.925 -1.35) (layer F.Fab) (width 0.1))
  (fp_line (start -1.6 1.35) (end -1.6 -0.675) (layer F.Fab) (width 0.1))
  (fp_line (start 1.6 1.35) (end -1.6 1.35) (layer F.Fab) (width 0.1))
  (fp_line (start 1.6 -1.35) (end 1.6 1.35) (layer F.Fab) (width 0.1))
  (fp_line (start -0.925 -1.35) (end 1.6 -1.35) (layer F.Fab) (width 0.1))
  (fp_line (start -2.8 1.5) (end -2.8 -1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.7 -1.5) (end -2.8 -1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.7 1.5) (end -2.8 1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.85 1.65) (end 2.85 -1.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.85 -1.65) (end -2.95 -1.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.95 -1.65) (end -2.95 1.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.95 1.65) (end 2.85 1.65) (layer F.CrtYd) (width 0.05))
  (pad 3 smd rect (at 1.75 0.7 180) (size 1.5 1) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 1.75 -0.7 180) (size 1.5 1) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.75 0.7 180) (size 1.5 1) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -1.75 -0.7 180) (size 1.5 1) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_RGB_1210.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
