(module JTJ-USB_A_F_90_10.0_C_H6.5 (layer F.Cu) (tedit 5E75E8D2)
  (descr "USB连接器/A/F90度 C款10前两脚无卷边铁壳PBT白胶=6.5,C42494, (https://atta.szlcsc.com/upload/public/pdf/source/20150916/1457707375091.pdf)")
  (tags "USB A Vertical Female C42494")
  (fp_text reference REF** (at 5.9 8.8) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value JTJ-USB_A_F_90_10.0_C_H6.5 (at 2.9 -0.1 180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 5.8 6.7) (end -0.3 6.7) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.9 -6.7) (end -0.3 -6.7) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.3 6.7) (end -0.3 4.3) (layer F.SilkS) (width 0.12))
  (fp_line (start 9.9 6.7) (end 9.9 -6.7) (layer F.SilkS) (width 0.12))
  (fp_line (start 9.9 6.7) (end 8.7 6.7) (layer F.SilkS) (width 0.12))
  (fp_line (start 9.9 -6.7) (end 8.7 -6.7) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.96 6.55) (end -0.96 4.15) (layer F.Fab) (width 0.1))
  (fp_line (start -0.96 2.85) (end -0.96 -6.55) (layer F.Fab) (width 0.1))
  (fp_line (start -0.2 3.5) (end -0.96 4.15) (layer F.Fab) (width 0.1))
  (fp_line (start -0.96 2.85) (end -0.2 3.5) (layer F.Fab) (width 0.1))
  (fp_line (start 10.1 -7.8) (end 10.1 7.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.4 -7.8) (end 10.1 -7.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.4 7.8) (end -1.4 -7.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 10.1 7.8) (end -1.4 7.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.96 -6.55) (end 9.76 -6.55) (layer F.Fab) (width 0.1))
  (fp_line (start 9.76 6.55) (end -0.96 6.55) (layer F.Fab) (width 0.1))
  (fp_line (start 9.76 -6.55) (end 9.76 6.55) (layer F.Fab) (width 0.1))
  (fp_text user %R (at 3.3 -0.1) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -0.3 2.7) (end -0.3 1.8) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.3 0.2) (end -0.3 -0.2) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.3 -1.8) (end -0.3 -2.7) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.3 -4.3) (end -0.3 -6.7) (layer F.SilkS) (width 0.12))
  (pad 5 thru_hole oval (at 7.25 6.4 270) (size 1.5 2.5) (drill oval 0.8 1.5) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at 7.25 -6.4 90) (size 1.5 2.5) (drill oval 0.8 1.5) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 3.5 270) (size 1.3 2) (drill 0.95) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 0 1 270) (size 1.3 2) (drill 0.95) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 0 -1 270) (size 1.3 2) (drill 0.95) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 0 -3.5 270) (size 1.3 2) (drill 0.95) (layers *.Cu *.Mask))
  (model {KISYS3DMOD}/Connector_USB.3dshapes/USB_A_Molex_105057_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
