(footprint "EE10_N2,4" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 0.4 -5.8 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 590807e7-b83b-4d6d-8cbe-3dab214a8311)
  )
  (fp_text value "EE10_N2,4" (at -1.428 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c28ffc6b-0b01-45db-90e0-3a9ca6563d07)
  )
  (fp_line (start -5.5 3.2) (end -5.5 5.3)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp b73e94c7-1013-4444-bf39-b3f27a236f38))
  (fp_line (start -5.5 5.3) (end -3.2 5.3)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp d71a24b2-095d-49f5-88e1-6f7e0c5ddabe))
  (fp_rect (start -5.6 -1.25) (end 5.6 1.25)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp 78e6282c-11c8-43fc-932a-e0e6a867c344))
  (fp_rect (start -5.3 -5.1) (end 5.3 5.1)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp c8ae8919-38cc-4b76-9a23-c0f8a6f42cd0))
  (pad "1" thru_hole rect (at -3.75 4) (size 2 1.4) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp 4432af19-9d75-4d6c-bd0e-b10f6ceb585c))
  (pad "3" thru_hole oval (at 1.25 4) (size 2 1.4) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp 23fc923e-a331-431e-a4b2-0288213b96fe))
  (pad "5" thru_hole oval (at 3.75 -4) (size 2 1.4) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp f4632103-2d30-4827-916c-ec9374db131d))
  (pad "6" thru_hole oval (at 1.25 -4) (size 2 1.4) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp 2dda12f9-d0bf-4ca4-9b3b-c6f2c24a26b2))
  (pad "7" thru_hole oval (at -1.25 -4) (size 2 1.4) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp 9d4faeeb-e0e6-462e-be61-a8ec2e5999a6))
  (pad "8" thru_hole oval (at -3.75 -4) (size 2 1.4) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp 5d57235a-c721-4767-b3b0-62646c179a74))
  (model "${TJ_LIB}/3d/User Library-E10-8T-V.STEP"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 -90))
  )
)
