(footprint "KF65C-11.0-4P"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "fc77cbdc-7980-47e7-9c6d-331c498c3ea3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "KF65C-11.0-4P"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "ccf276f9-ed5f-4853-bbfc-9be236ab6f65")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "167e8501-e120-43ba-9319-6897c52fb1a4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1439f5a3-739e-4c74-bfec-4365f34b6b8f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0af29543-efb6-4e90-9eb2-72f8f9f2d380")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -6.8 -8.7)
		(end -6.8 8.7)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "84646983-0261-4998-b3b9-4176f8c38ca3")
	)
	(fp_line
		(start -6.8 8.7)
		(end 0 8.7)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "80680a1d-2340-4158-879b-4619578bb4ea")
	)
	(fp_line
		(start 0 -8.7)
		(end -6.8 -8.7)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "3080c8bf-a7c1-4495-91dd-8947c4244720")
	)
	(fp_line
		(start 0 8.7)
		(end 33 8.7)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "4e4c772c-498a-4e23-8a0a-9f2acfed4b8b")
	)
	(fp_line
		(start 33 -8.7)
		(end 0 -8.7)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "171297a0-472d-4458-a3c0-278e46c8cb29")
	)
	(fp_line
		(start 33 -8.7)
		(end 39.8 -8.7)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "12a40e01-d1aa-4d0b-a69f-3fc16b77fe4e")
	)
	(fp_line
		(start 39.8 -8.7)
		(end 39.8 8.7)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "d2cd74ea-f516-4b75-98e4-221e8bfde370")
	)
	(fp_line
		(start 39.8 8.7)
		(end 33 8.7)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "2db86a2d-b3be-4a15-8554-1664af0e2b48")
	)
	(fp_line
		(start -6.9 -8.8)
		(end 0 -8.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "984ef7c3-005e-4b66-b693-4b1dc512e851")
	)
	(fp_line
		(start -6.9 8.8)
		(end -6.9 -8.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ab8dc0da-0ab2-40d1-8196-4862877813fd")
	)
	(fp_line
		(start 0 -8.8)
		(end 33 -8.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "f986228a-813c-4a37-8647-f7cd442f026a")
	)
	(fp_line
		(start 0 8.8)
		(end -6.9 8.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "cf7e38e7-1b40-47df-8336-2991a8e99ac3")
	)
	(fp_line
		(start 33 8.8)
		(end 0 8.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "631596a7-5e48-441f-a520-0d22a1d62b54")
	)
	(fp_line
		(start 33 8.8)
		(end 39.9 8.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "6a4dfb5c-3463-4495-9a88-fb19d20082a0")
	)
	(fp_line
		(start 39.9 -8.8)
		(end 33 -8.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "88576eda-5cf7-4f2d-8a08-fc419ca373e4")
	)
	(fp_line
		(start 39.9 8.8)
		(end 39.9 -8.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e0439dc5-cdf8-428e-951e-e04bc15629cd")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 3.6 5)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.1640419948)
		(uuid "b4217021-9dbc-430a-a5e5-82f7aeaa07ef")
	)
	(pad "2" thru_hole oval
		(at 11 0)
		(size 3.6 5)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "92ce47e8-6adc-4791-b05d-8e21dd444018")
	)
	(pad "3" thru_hole oval
		(at 22 0)
		(size 3.6 5)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c38734fe-a570-4741-8525-1f1ab127497c")
	)
	(pad "4" thru_hole oval
		(at 33 0)
		(size 3.6 5)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1c854260-d6b3-4601-97d0-97a7da1e6639")
	)
)
