(footprint "LED_0602_1706Metric_Size"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "LED SMD 0602 Size Look (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://atta.szlcsc.com/upload/public/pdf/source/20240218/1776525B289579D8995F3961D0B0ED19.pdf),")
	(tags "LED,PCB 透光,侧贴")
	(property "Reference" "REF**"
		(at 0.3 1.4 0)
		(layer "F.SilkS")
		(uuid "292741c4-f38a-46be-96b4-e8e4adda1eb8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "LED_0602_1706Metric_Size"
		(at 0 1.43 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "53d18d0d-7a8b-4ada-90ab-6382184ad4c2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f879c7a5-b57d-4609-b166-0f5e4e3638ed")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "350331dd-6b44-440d-a5af-faf2735eab5c")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.45 -0.6)
		(end -1.45 0.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a61009e0-7d1c-4008-bc11-4b210fbb5f45")
	)
	(fp_line
		(start -1.45 0.6)
		(end 1.1 0.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "14a2ba1c-1389-4245-b264-01e350a58427")
	)
	(fp_line
		(start -0.86 -1.1)
		(end 0.86 -1.1)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "40baf8f1-755a-47a7-a355-ab5da88dfce1")
	)
	(fp_line
		(start -0.86 -0.6)
		(end -1.45 -0.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ca086f38-23cb-437f-98b5-9eb3543ea14c")
	)
	(fp_line
		(start -0.86 -0.6)
		(end -0.86 -1.1)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "a1c3e36a-b2d6-4431-bfa4-11639ef5df6d")
	)
	(fp_line
		(start 0.86 -0.6)
		(end 0.86 -1.1)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "38d558d6-3332-4163-834d-7fb49ee313e6")
	)
	(fp_line
		(start 0.86 -0.6)
		(end 1.1 -0.6)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "1c7f4860-6f28-4a3f-942b-3c9ece5ea548")
	)
	(fp_line
		(start -1.45 0.6)
		(end -1.45 -0.6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2dde7546-5f04-46b7-ad48-8cf9f8394899")
	)
	(fp_line
		(start -0.72 -1.1)
		(end 0.72 -1.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "18e6565f-7293-488c-b3cf-710a71824868")
	)
	(fp_line
		(start -0.72 -0.6)
		(end -1.45 -0.6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "dffc6aac-5e2a-48cb-97be-dd2d88f1ca77")
	)
	(fp_line
		(start -0.72 -0.6)
		(end -0.72 -1.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "7e8ca1d3-fa79-41ae-8e3a-21df1a942dc7")
	)
	(fp_line
		(start 0.72 -1.1)
		(end 0.72 -0.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9be56754-da18-48a9-852a-bf69e5802c67")
	)
	(fp_line
		(start 1.45 -0.6)
		(end 0.72 -0.6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "e9018e53-bc19-4638-9619-00b564bb0d69")
	)
	(fp_line
		(start 1.45 -0.6)
		(end 1.45 0.6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "7bfde076-eefc-4f5b-8e45-4f5e4bf15a48")
	)
	(fp_line
		(start 1.45 0.6)
		(end -1.45 0.6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "86486440-4856-4c98-ad7d-3958c0cdb18d")
	)
	(fp_line
		(start -0.8 -0.1)
		(end -0.8 0.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "98c2e268-ea04-482a-83b8-8f38c3203b78")
	)
	(fp_line
		(start -0.8 0.4)
		(end 0.8 0.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "af641bc8-d996-4a2a-895a-06d3b5ad3322")
	)
	(fp_line
		(start -0.5 -0.4)
		(end -0.8 -0.1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "087d096f-0c5a-4d2c-ad5f-1bef65ca374d")
	)
	(fp_line
		(start 0.8 -0.4)
		(end -0.5 -0.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e85c8247-c2d8-4e42-8fe5-79ef729f3ed5")
	)
	(fp_line
		(start 0.8 0.4)
		(end 0.8 -0.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "496d1695-30f2-45b1-a793-58b2f6fdd52b")
	)
	(fp_line
		(start 1 -0.9)
		(end 1.4 -0.9)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "9fa376a9-4e54-48e9-9e49-cf762b8f80fd")
	)
	(fp_line
		(start 1.2 -0.7)
		(end 1.2 -1.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "a35737f0-f55b-45dd-96c4-b02da7f29116")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "1d693d84-fdc3-48eb-afa5-40e190cdca80")
		(effects
			(font
				(size 0.4 0.4)
				(thickness 0.06)
			)
		)
	)
	(pad "1" smd roundrect
		(at -0.82 0)
		(size 0.78 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "902f25b0-cb45-4114-bb5f-def34f8704c7")
	)
	(pad "2" smd roundrect
		(at 0.82 0)
		(size 0.78 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "dd9eecb5-87cb-42a6-baae-af0c098b27ff")
	)
	(embedded_fonts no)
	(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
		(offset
			(xyz 0 -0.22 0.3)
		)
		(scale
			(xyz 1 0.7 1)
		)
		(rotate
			(xyz 90 0 0)
		)
	)
)
