(module USB_A_F_180 (layer F.Cu) (tedit 5E8B0018)
  (descr "USB连接器/ A/F180度插板直脚平边铜3.7(https://item.taobao.com/item.htm?spm=a230r.1.14.41.7ca990f6rOA62u&id=42717783937)")
  (tags "USB A Vertical Female ")
  (fp_text reference REF** (at 0.1 4.2 180) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value USB_A_F_180 (at 0.3 1.04) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0.05 0.29 180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 6.55 2.9) (end -6.55 2.9) (layer F.Fab) (width 0.1))
  (fp_line (start -6.55 2.9) (end -6.55 -2.82) (layer F.Fab) (width 0.1))
  (fp_line (start 6.55 -2.82) (end 6.55 2.9) (layer F.Fab) (width 0.1))
  (fp_line (start -7.5 3.2) (end -7.5 -3.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -7.5 -3.2) (end 7.5 -3.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 7.5 -3.2) (end 7.5 3.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 7.5 3.2) (end -7.5 3.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.85 -2.82) (end -3.5 -2.06) (layer F.Fab) (width 0.1))
  (fp_line (start -3.5 -2.06) (end -4.15 -2.82) (layer F.Fab) (width 0.1))
  (fp_line (start -2.85 -2.82) (end 6.55 -2.82) (layer F.Fab) (width 0.1))
  (fp_line (start -6.55 -2.82) (end -4.15 -2.82) (layer F.Fab) (width 0.1))
  (fp_line (start -5.9 3) (end 5.9 3) (layer F.SilkS) (width 0.15))
  (fp_line (start -6.7 -3) (end 6.7 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start 6.7 -0.96) (end 6.7 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start -6.7 -0.96) (end -6.7 -3) (layer F.SilkS) (width 0.15))
  (pad 4 thru_hole oval (at 3.5 -1.26 180) (size 1.3 2) (drill 0.9) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 1 -1.26 180) (size 1.3 2) (drill 0.9) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at -1 -1.26 180) (size 1.3 2) (drill 0.9) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at -3.5 -1.26 180) (size 1.3 2) (drill 0.9) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at 6.45 1.24) (size 2 3.5) (drill oval 1 2.3) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at -6.45 1.24 180) (size 2 3.5) (drill oval 1 2.3) (layers *.Cu *.Mask))
  (model {KISYS3DMOD}/Connector_USB.3dshapes/USB_A_Molex_105057_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
