(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "47L04"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "47L04"
			(at -3.81 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SOIC127P600-8M"
			(at -5.08 -22.86 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "4Kbit (512 x 8), 2-wire Bus Automotive Serial EEPROM with Write Protect, 2.5V, 8-Pin SOIC, Bulk"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -5.08 -27.94 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Package" "SOIC-8"
			(at -5.08 -33.02 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Part_Number" "47L04"
			(at -5.08 -35.56 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -5.08 -38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Comment" "47L04"
			(at -1.27 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Created" "5/05/2006"
			(at -5.08 -40.64 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(symbol "47L04_1_1"
			(rectangle
				(start 0 -17.78)
				(end 15.24 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "VCAP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 -7.62 0)
				(length 5.08)
				(name "A1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 -10.16 0)
				(length 5.08)
				(name "A2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -5.08 -15.24 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "VCC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "HS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input clock
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "SCL"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "SDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "74HC125D"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U15"
			(at -5.08 1.397 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "74HC125D"
			(at -3.81 3.937 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SOIC127P600-14M"
			(at -5.08 -17.907 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Quad Bus Buffer Gates with 3-State Outputs"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Part_Number" "74HC125D"
			(at -5.08 -20.447 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -5.08 -22.987 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Note" "*"
			(at -5.08 -25.527 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Package" "SOIC-14"
			(at -5.08 -28.067 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Manufacturer" "NXP"
			(at -5.08 -30.607 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -5.08 -33.147 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(symbol "74HC125D_0_1"
			(pin power_in line
				(at -5.08 -10.16 0)
				(length 5.08)
				(hide yes)
				(name "VCC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 12.7 -12.7 180)
				(length 5.08)
				(hide yes)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "74HC125D_1_1"
			(polyline
				(pts
					(xy 0 -1.27) (xy 7.62 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -8.89) (xy 0 -1.27)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -8.89) (xy 7.62 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 0) (xy 0 0)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 -3.048) (xy 3.81 0)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(pin input inverted
				(at -5.08 0 0)
				(length 5.08)
				(name "1~{C}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 -5.08 0)
				(length 5.08)
				(name "1A"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin tri_state line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "1Y"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "74HC125D_2_1"
			(polyline
				(pts
					(xy 0 -1.27) (xy 7.62 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -8.89) (xy 0 -1.27)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -8.89) (xy 7.62 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 0) (xy 0 0)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 -3.048) (xy 3.81 0)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(pin input inverted
				(at -5.08 0 0)
				(length 5.08)
				(name "2~{C}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 -5.08 0)
				(length 5.08)
				(name "2A"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin tri_state line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "2Y"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "74HC125D_3_1"
			(polyline
				(pts
					(xy 0 -1.27) (xy 7.62 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -8.89) (xy 0 -1.27)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -8.89) (xy 7.62 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 0) (xy 0 0)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 -3.048) (xy 3.81 0)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(pin input inverted
				(at -5.08 0 0)
				(length 5.08)
				(name "3~{C}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 -5.08 0)
				(length 5.08)
				(name "3A"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin tri_state line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "3Y"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "74HC125D_4_1"
			(polyline
				(pts
					(xy 0 -1.27) (xy 7.62 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -8.89) (xy 0 -1.27)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -8.89) (xy 7.62 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 0) (xy 0 0)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 -3.048) (xy 3.81 0)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(pin input inverted
				(at -5.08 0 0)
				(length 5.08)
				(name "4~{C}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 -5.08 0)
				(length 5.08)
				(name "4A"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin tri_state line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "4Y"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G08"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "74LVC1G08"
			(at 6.35 -3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Single AND Gate, Low-Voltage CMOS"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Single Gate AND LVC CMOS"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "74LVC1G08_0_1"
			(arc
				(start 0 2.54)
				(mid 2.529 0)
				(end 0 -2.54)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -3.81 -2.54) (xy -3.81 2.54) (xy 0 2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
		)
		(symbol "74LVC1G08_1_1"
			(pin input line
				(at -7.62 1.27 0)
				(length 3.81)
				(name "~"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin input line
				(at -7.62 -1.27 0)
				(length 3.81)
				(name "~"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 0 5.08 270)
				(length 2.54)
				(name "+"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -5.08 90)
				(length 2.54)
				(name "G"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin output line
				(at 6.35 0 180)
				(length 3.81)
				(name "~"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVC1G384GV"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "74LVC1G384GV"
			(at -3.81 11.43 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SOT23-5AM"
			(at -5.08 -10.16 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Part_Number" "74LVC1G384GV"
			(at -5.08 -12.7 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -5.08 -15.24 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -5.08 -17.78 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Note" "*"
			(at -5.08 -20.32 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Package" "SOT-23-5"
			(at -5.08 -22.86 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(symbol "74LVC1G384GV_1_1"
			(rectangle
				(start 0 -5.08)
				(end 15.24 7.62)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 3.81 5.08) (xy 7.62 5.08) (xy 7.62 3.556)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 3.81 2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 5.5626 2.5146)
				(mid 5.5692 2.4893)
				(end 5.5626 2.4638)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.588 2.794) (xy 9.906 4.064)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 10.1346 2.5146)
				(mid 10.1409 2.4893)
				(end 10.1346 2.4638)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 10.16 2.54) (xy 11.43 2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(pin passive input_low
				(at -5.08 5.08 0)
				(length 5.08)
				(name "E"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 5.08)
				(name "Z"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "Y"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "VCC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD8603"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U9"
			(at -5.08 6.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "AD8603"
			(at -3.81 8.89 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SOT23-5AN"
			(at -5.08 -20.32 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Low-Noise J-FET Dual Operational Amplifier"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Package" "SO-8"
			(at -5.08 -25.4 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -5.08 -30.48 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -5.08 -33.02 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Part_Number" "AD8603AUJZ-R2"
			(at -5.08 -35.56 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Comment" "AD8603"
			(at -1.27 6.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(symbol "AD8603_0_1"
			(pin power_in line
				(at 5.08 5.08 270)
				(length 5.08)
				(name "V+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 5.08)
				(name "V-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "AD8603_1_1"
			(polyline
				(pts
					(xy 0 0) (xy 0 -10.16)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 10.16 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -10.16) (xy 10.16 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.016 -2.54) (xy 2.54 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.016 -7.62) (xy 2.54 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.778 -6.858) (xy 1.778 -8.382)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 0) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -7.62) (xy 5.08 -10.16)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(pin input line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "IN-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 -7.62 0)
				(length 5.08)
				(name "IN+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS1118IDGS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "ADS1118IDGS"
			(at -3.81 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "TSSOP50P490-10AM"
			(at -5.08 -27.94 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "TI"
			(at -5.08 -30.48 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Package" "VSSOP-10"
			(at -5.08 -35.56 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -5.08 -38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -5.08 -40.64 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Part_Number" "ADS1118IDGS"
			(at -5.08 -43.18 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right bottom)
			)
		)
		(symbol "ADS1118IDGS_1_1"
			(rectangle
				(start 0 -22.86)
				(end 20.32 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin input line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "AIN0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 -7.62 0)
				(length 5.08)
				(name "AIN1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 -15.24 0)
				(length 5.08)
				(name "AIN2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 -20.32 0)
				(length 5.08)
				(name "AIN3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "VCC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "SCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "DIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "DOUT~{/DRD}Y"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "CS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS1230IPW"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 11.43 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "ADS1230IPW"
			(at 6.35 11.43 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 6.35 13.97 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.ti.com.cn/cn/lit/gpn/ADS1230"
			(at -12.7 10.16 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "20-Bit Analog-to-Digital Converter For Bridge Sensors, Two-Wire Serial Digital Interface, TSSOP-16 package"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "adc"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "*TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "ADS1230IPW_0_1"
			(rectangle
				(start -15.24 10.16)
				(end 15.24 -10.16)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(symbol "ADS1230IPW_1_1"
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "REFP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "REFN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "CAP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -17.78 0 0)
				(length 2.54)
				(name "CAP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "AINP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "AINN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -5.08 12.7 270)
				(length 2.54)
				(name "AVDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -5.08 -12.7 90)
				(length 2.54)
				(name "AGND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "DVDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "DGND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "SCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "DOUT/~{DRDY}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "~{PDWN}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "SPEED"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "GAIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input clock
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "CLKIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS1255"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 22.86 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "ADS1255"
			(at -16.51 25.4 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" ""
			(at 21.59 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
					(italic yes)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.ti.com.cn/cn/lit/ds/symlink/ads1256.pdf"
			(at -1.27 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "24-bit ADC, 2 Channels, SPI compatible, PGA 1 to 128, SSOP-20"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "24bit ADC 2 Channels PGA SPI"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "ADS1255_0_1"
			(rectangle
				(start -12.7 21.59)
				(end 12.7 -21.59)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(symbol "ADS1255_1_1"
			(pin input line
				(at -16.51 17.78 0)
				(length 3.81)
				(name "AIN0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 15.24 0)
				(length 3.81)
				(name "AIN1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 12.7 0)
				(length 3.81)
				(name "AINCOM"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 -7.62 0)
				(length 3.81)
				(name "VREFP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 -12.7 0)
				(length 3.81)
				(name "VREFN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 3.81)
				(name "AVDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -5.08 -25.4 90)
				(length 3.81)
				(name "AGND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 3.81)
				(name "DVDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 5.08 -25.4 90)
				(length 3.81)
				(name "DGND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 16.51 1.27 180)
				(length 3.81)
				(name "D0/CLKOUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 16.51 -1.27 180)
				(length 3.81)
				(name "D1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input clock
				(at 17.78 17.78 180)
				(length 5.08)
				(name "SCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "DOUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "DIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input input_low
				(at 17.78 10.16 180)
				(length 5.08)
				(name "~{CS}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output output_low
				(at 17.78 5.08 180)
				(length 5.08)
				(name "~{DRDY}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input input_low
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "~{RESET}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input input_low
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "~{SYNC}/~{PDWN}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "XTAL1/CLKIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "XTAL2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS8321"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "ADS8321"
			(at -3.81 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "Dummy"
			(at -5.08 -22.86 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "16-Bit, High Speed, MicroPower Sampling Analog-to-Digital Converter"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "TI"
			(at -5.08 -25.4 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Package" "MSOP-8"
			(at -5.08 -30.48 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -5.08 -33.02 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -5.08 -35.56 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Part_Number" "ADS8321E"
			(at -5.08 -38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right bottom)
			)
		)
		(symbol "ADS8321_1_1"
			(rectangle
				(start 0 -17.78)
				(end 20.32 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin input line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "VREF"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 -7.62 0)
				(length 5.08)
				(name "+IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 -10.16 0)
				(length 5.08)
				(name "-IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -5.08 -15.24 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "VCC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "SCK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "SDO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "~{CS}/SHDN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM1201"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "ADuM1201"
			(at -3.81 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SOIC127P600-8M"
			(at -5.08 -22.86 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "High Speed 2-Channel Digital Isolators(Transmit/Receive Channels:1/1)"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Note" "*"
			(at -5.08 -25.4 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Manufacturer" "ADI"
			(at -5.08 -27.94 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -5.08 -30.48 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -5.08 -33.02 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Price" "5.8"
			(at -5.08 -35.56 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "供应商" "力创"
			(at -5.08 -38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Part_Number" "ADuM1201AR"
			(at -5.08 -40.64 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Package" "SOIC-8"
			(at -5.08 -43.18 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Comment" "1201"
			(at -1.27 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(symbol "ADuM1201_1_1"
			(polyline
				(pts
					(xy 0 -7.62) (xy 2.54 -7.62)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -10.16) (xy 2.54 -10.16)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start 0 -17.78)
				(end 17.78 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 5.08 -7.62) (xy 7.62 -7.62)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -10.16) (xy 7.62 -10.16)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start 7.62 -17.78)
				(end 10.16 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 10.16 -7.62) (xy 12.7 -7.62)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 10.16 -10.16) (xy 12.7 -10.16)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 15.24 -7.62) (xy 17.78 -7.62)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 15.24 -10.16) (xy 17.78 -10.16)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "VDD1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 5.08)
				(name "VO1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 5.08)
				(name "VI2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 5.08)
				(name "GND1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "VDD2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "VI1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "VO2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "GND2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "AX58100"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 22.86 2.54 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "AX58100"
			(at 10.16 2.54 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "tj_IC:LQFP-80_1EP_10x10mm_P0.4mm"
			(at 0 -60.96 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.asix.com.tw/cn/support/download/file/1153"
			(at 25.4 -2.54 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "EtherCAT Slave Controller"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "lcsc_no" "C968587"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "EtherCAT Slave Controller"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "AX58100_0_0"
			(pin bidirectional line
				(at -5.08 -5.08 0)
				(length 5.08)
				(name "IO[0]/LDA[0]/MSCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -7.62 0)
				(length 5.08)
				(name "IO[1]/LDA[1]/MMOSI"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -10.16 0)
				(length 5.08)
				(name "IO[2]/LDA[2]/MMISO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -12.7 0)
				(length 5.08)
				(name "IO[3]/LDA[3]/MINT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "51"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -15.24 0)
				(length 5.08)
				(name "IO[4]/LDA[4]/MSS[0]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "60"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -17.78 0)
				(length 5.08)
				(name "IO[5]/LDA[5]/MSS[1]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "53"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -20.32 0)
				(length 5.08)
				(name "IO[6]/LDA[6]/MSS[2]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "67"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -22.86 0)
				(length 5.08)
				(name "IO[7]/LDA[7]/MSS[3]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "69"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -27.94 0)
				(length 5.08)
				(name "IO[8]/LA[0]/MDRLD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "71"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -30.48 0)
				(length 5.08)
				(name "IO[9]/LA[1]/MTRG"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "74"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -33.02 0)
				(length 5.08)
				(name "IO[10]/LA[2]/SFINT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "49"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -35.56 0)
				(length 5.08)
				(name "IO[11]/LA[3]/FMISO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -38.1 0)
				(length 5.08)
				(name "IO[12]/LA[4]/FSCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -40.64 0)
				(length 5.08)
				(name "IO[13]/LA[5]/SMOSI"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -43.18 0)
				(length 5.08)
				(name "IO[14]/LA[6]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -45.72 0)
				(length 5.08)
				(name "IO[15]/LA[7]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -50.8 0)
				(length 5.08)
				(name "IO[16]/LA[8]/LINK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -53.34 0)
				(length 5.08)
				(name "IO[17]/LA[9]/PULAB/MDIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -55.88 0)
				(length 5.08)
				(name "IO[18]/LA[10]/PULC/MDC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "50"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -58.42 0)
				(length 5.08)
				(name "IO[19]/LA[11]/PULZ/TXD[0]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "52"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -60.96 0)
				(length 5.08)
				(name "IO[20]/LA[12]/PULB/TXD[1]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -63.5 0)
				(length 5.08)
				(name "IO[21]/LA[13]/PULA/TXD[2]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "66"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -66.04 0)
				(length 5.08)
				(name "IO[22]/LBHE/PWM3H/TXD[3]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "68"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -68.58 0)
				(length 5.08)
				(name "IO[23]/PWM3L/TX_EN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "70"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -73.66 0)
				(length 5.08)
				(name "IO[24]/LDA[8]/PWM2H/RXD[0]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "73"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -76.2 0)
				(length 5.08)
				(name "IO[25]/LDA[9]/PWM2L/RXD[1]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "75"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -78.74 0)
				(length 5.08)
				(name "IO[26]/LDA[10]/PWM1H/RXD[2]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "76"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -81.28 0)
				(length 5.08)
				(name "IO[27]/LDA[11]/PWM1L/RXD[3]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -83.82 0)
				(length 5.08)
				(name "IO[28]/LDA[12]/EMn/RX_ER"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -86.36 0)
				(length 5.08)
				(name "IO[29]/LDA[13]/ENCA/RX_DV"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -88.9 0)
				(length 5.08)
				(name "IO[30]/LDA[14]/ENCB/RX_CLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -91.44 0)
				(length 5.08)
				(name "IO[31]/LDA[15]/ENCZ/MCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 -96.52 0)
				(length 5.08)
				(name "OE_EXT/LRDn/SCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "64"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at -5.08 -99.06 0)
				(length 5.08)
				(name "OUTVLD/LWRn/MOSI"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "78"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at -5.08 -101.6 0)
				(length 5.08)
				(name "SOF/LECSn/SCS_ESC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "79"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at -5.08 -104.14 0)
				(length 5.08)
				(name "EOF/LFCSn/SCS_FUNC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "80"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -106.68 0)
				(length 5.08)
				(name "LAT_IN/LRDY/MISO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at -5.08 -109.22 0)
				(length 5.08)
				(name "WD_TRIG/LINT/SINT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin open_collector line
				(at -5.08 -114.3 0)
				(length 5.08)
				(name "SCL"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "62"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -116.84 0)
				(length 5.08)
				(name "SDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "63"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -121.92 0)
				(length 5.08)
				(name "SYNC_LATCH[0]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -124.46 0)
				(length 5.08)
				(name "SYNC_LATCH[1]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 58.42 -5.08 180)
				(length 5.08)
				(name "P0_TXOP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 58.42 -7.62 180)
				(length 5.08)
				(name "P0_TXON"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 58.42 -10.16 180)
				(length 5.08)
				(name "P0_RXIP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 58.42 -12.7 180)
				(length 5.08)
				(name "P0_RXIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 58.42 -15.24 180)
				(length 5.08)
				(name "P0_SD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 58.42 -17.78 180)
				(length 5.08)
				(name "P0_ACT_LED/P0_FIBER"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 58.42 -22.86 180)
				(length 5.08)
				(name "P1_TXOP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 58.42 -25.4 180)
				(length 5.08)
				(name "P1_TXON"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 58.42 -27.94 180)
				(length 5.08)
				(name "P1_RXIP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 58.42 -30.48 180)
				(length 5.08)
				(name "P1_RXIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 58.42 -33.02 180)
				(length 5.08)
				(name "P1_SD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 58.42 -35.56 180)
				(length 5.08)
				(name "P1_ACT_LED/P1_FIBER"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 58.42 -40.64 180)
				(length 5.08)
				(name "RSET_BG"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 58.42 -45.72 180)
				(length 5.08)
				(name "XSCI"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 58.42 -48.26 180)
				(length 5.08)
				(name "XSCO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 58.42 -53.34 180)
				(length 5.08)
				(name "RSTn"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "57"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 58.42 -55.88 180)
				(length 5.08)
				(name "RSTO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "58"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 58.42 -60.96 180)
				(length 5.08)
				(name "LED_RUN/3PORT_MODE"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 58.42 -63.5 180)
				(length 5.08)
				(name "LED_ERR/EEP_SIZE"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 58.42 -66.04 180)
				(length 5.08)
				(name "EEP_DONE"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 58.42 -68.58 180)
				(length 5.08)
				(name "PDI_EMU"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "61"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 58.42 -73.66 180)
				(length 5.08)
				(name "TEST"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "59"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 58.42 -76.2 180)
				(length 5.08)
				(name "NC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "56"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 58.42 -81.28 180)
				(length 5.08)
				(name "VCCK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 58.42 -83.82 180)
				(length 5.08)
				(name "VCCK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 58.42 -86.36 180)
				(length 5.08)
				(name "VCCK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 58.42 -88.9 180)
				(length 5.08)
				(name "VCCK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 58.42 -91.44 180)
				(length 5.08)
				(name "VCCK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "55"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 58.42 -93.98 180)
				(length 5.08)
				(name "VCCK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "72"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 58.42 -99.06 180)
				(length 5.08)
				(name "VCC12A_PLL"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "54"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 58.42 -104.14 180)
				(length 5.08)
				(name "VCC3IO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "77"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 58.42 -106.68 180)
				(length 5.08)
				(name "VCC3IO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "65"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 58.42 -109.22 180)
				(length 5.08)
				(name "VCC3IO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 58.42 -111.76 180)
				(length 5.08)
				(name "VCC3IO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 58.42 -116.84 180)
				(length 5.08)
				(name "VCC33A"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 58.42 -119.38 180)
				(length 5.08)
				(name "VCC33A"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 58.42 -121.92 180)
				(length 5.08)
				(name "VCC33A"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 58.42 -124.46 180)
				(length 5.08)
				(name "VCC33A"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 58.42 -129.54 180)
				(length 5.08)
				(name "GND_EPAD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "81"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "AX58100_0_1"
			(rectangle
				(start 0 0)
				(end 53.34 -134.62)
				(stroke
					(width 0.1524)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "A_S-2WR2"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 21.59 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "A_S-2WR2"
			(at -3.81 24.13 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "Mornsun-A-S-2W"
			(at -5.08 -5.1054 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Package" "SIP"
			(at -5.08 -10.1854 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "插件"
			(at -5.08 -15.2654 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -5.08 -17.8054 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Price" "13"
			(at -5.08 -20.3454 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "供应商" "昌久"
			(at -5.08 -22.8854 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Part_Number" "A2405S-2WR2"
			(at -5.08 -25.4254 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(symbol "A_S-2WR2_1_1"
			(rectangle
				(start 0 0)
				(end 7.62 20.32)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(rectangle
				(start 8.382 0)
				(end 9.398 20.32)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(rectangle
				(start 10.16 0)
				(end 17.78 20.32)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 5.08)
				(name "Vin"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "+Vo"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "0V"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "-Vo"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "BL0939-SSOP20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 -17.78 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "BL0939-SSOP20"
			(at 10.414 -19.558 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_SO:SSOP-20_3.9x8.7mm_P0.635mm"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.belling.com.cn/media/file_object/bel_product/BL0939/datasheet/BL0939_V1.4_cn.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "内置时钟免校准计量芯片,ssop-20"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "power sensor"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "SOP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "BL0939-SSOP20_0_1"
			(rectangle
				(start -10.16 16.51)
				(end 10.16 -16.51)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(symbol "BL0939-SSOP20_1_0"
			(pin input line
				(at -12.7 13.97 0)
				(length 2.54)
				(name "VT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -12.7 -3.81 0)
				(length 2.54)
				(name "IP2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -12.7 -6.35 0)
				(length 2.54)
				(name "IN2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin free line
				(at 1.27 19.05 270)
				(length 2.54)
				(name "VPP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin open_collector line
				(at 12.7 13.97 180)
				(length 2.54)
				(name "TX/SDO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 12.7 11.43 180)
				(length 2.54)
				(name "RX/SDI"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 12.7 8.89 180)
				(length 2.54)
				(name "SCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "ZX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 12.7 -6.35 180)
				(length 2.54)
				(name "A1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 12.7 -8.89 180)
				(length 2.54)
				(name "A2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 12.7 -11.43 180)
				(length 2.54)
				(name "A3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 12.7 -13.97 180)
				(length 2.54)
				(name "A4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "BL0939-SSOP20_1_1"
			(pin input line
				(at -12.7 8.89 0)
				(length 2.54)
				(name "IP1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -12.7 6.35 0)
				(length 2.54)
				(name "IN1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -12.7 -13.97 0)
				(length 2.54)
				(name "VP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -2.54 19.05 270)
				(length 2.54)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -19.05 90)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SEL"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CF"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "I_leak"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "BL9342"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "BL9342"
			(at 0 6.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -8.89 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.belling.com.cn/media/file_object/bel_product/BL9342/datasheet/BL9342_V1.3_cn.pdf"
			(at -7.62 8.89 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "40V, 600mA 降压型稳压电路, SOT-23-6"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "BL9342_0_1"
			(rectangle
				(start -7.62 5.08)
				(end 7.62 -5.08)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(symbol "BL9342_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "BST"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "SW"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "BTS443P"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 1.27 0)
			(effects
				(font
					(size 1.397 1.397)
				)
				(justify left bottom)
			)
		)
		(property "Value" "BTS443P"
			(at -3.81 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "TO-252-5"
			(at -5.08 -15.24 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Part_Number" "BTS443P"
			(at -5.08 -17.78 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Package" "TO-252-5"
			(at -5.08 -20.32 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Note" "*"
			(at -5.08 -22.86 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Manufacturer" "*"
			(at -5.08 -25.4 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -5.08 -27.94 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -5.08 -30.48 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(symbol "BTS443P_1_1"
			(rectangle
				(start 0 -10.16)
				(end 15.24 0)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin input line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin tri_state line
				(at -5.08 -7.62 0)
				(length 5.08)
				(name "IS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "VBB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "B_D-1WR2"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "B_D-1WR2"
			(at -6.35 13.97 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "MORNSUN-D-1W"
			(at -7.62 -5.1054 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Package" "MORNSUN-D-1W"
			(at -7.62 -10.1854 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "插件"
			(at -7.62 -15.2654 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -7.62 -17.8054 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Price" "13"
			(at -7.62 -20.3454 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "供应商" "昌久"
			(at -7.62 -22.8854 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Part_Number" "B2405D-1WR2"
			(at -7.62 -25.4254 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(symbol "B_D-1WR2_1_1"
			(rectangle
				(start 0 0)
				(end 7.62 10.16)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(rectangle
				(start 8.382 0.254)
				(end 9.398 9.906)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(rectangle
				(start 10.16 0)
				(end 17.78 10.16)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 7.62)
				(name "Vin"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 7.62)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 7.62)
				(name "+Vo"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 25.4 2.54 180)
				(length 7.62)
				(name "0V"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "B_LS-1W"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "B_LS-1W"
			(at -4.445 5.715 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "tj_IC:MORNSUN-B_LS-1W"
			(at -6.35 -1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.mornsun.cn/public/uploads/pdf/B_LS-1WR3.pdf"
			(at -6.35 -5.08 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "B_LS-1W_0_1"
			(polyline
				(pts
					(xy 0 4.445) (xy 0 3.175)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 1.27)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0.635) (xy 0 -0.635)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -1.27) (xy 0 -2.54)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -3.175) (xy 0 -4.445)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
		)
		(symbol "B_LS-1W_1_1"
			(rectangle
				(start -7.62 -5.08)
				(end 7.62 5.08)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "Vin"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vo"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "0V"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "B_S-2WR2"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "B_S-2WR2"
			(at -6.35 13.97 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "Mornsun-B-S-2W"
			(at -7.62 -5.1054 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Package" "SIP"
			(at -7.62 -10.1854 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "插件"
			(at -7.62 -15.2654 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -7.62 -17.8054 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Price" "13"
			(at -7.62 -20.3454 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "供应商" "昌久"
			(at -7.62 -22.8854 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Part_Number" "B2405S-2WR2"
			(at -7.62 -25.4254 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(symbol "B_S-2WR2_1_1"
			(rectangle
				(start 0 0)
				(end 7.62 10.16)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(rectangle
				(start 8.382 0.254)
				(end 9.398 9.906)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(rectangle
				(start 10.16 0)
				(end 17.78 10.16)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 7.62)
				(name "Vin"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 7.62)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 7.62)
				(name "+Vo"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 25.4 2.54 180)
				(length 7.62)
				(name "0V"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "CA-IS3741xN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 19.05 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "CA-IS3741xN"
			(at 0 16.51 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -14.605 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://item.szlcsc.com/datasheet/CA-IS3741LN/548120.htm"
			(at -20.32 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Quad Channel Digital Isolator, 150Mbps, SOIC-16"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Digital Isolator"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "CA-IS3741xN_0_0"
			(polyline
				(pts
					(xy -6.985 7.62) (xy -7.62 7.62)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -6.985 5.08) (xy -7.62 5.08)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -6.985 2.54) (xy -7.62 2.54)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -6.985 0) (xy -7.62 0)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -4.445 -1.27) (xy -4.445 -0.635)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -4.445 -1.27) (xy -4.445 -5.08) (xy -5.715 -5.08)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 7.62) (xy -1.27 7.62)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 5.08) (xy -1.27 5.08)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 2.54) (xy -1.27 2.54)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start -1.905 0.635)
				(end -6.985 -0.635)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 0) (xy -1.27 0)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start -1.27 8.636)
				(end 1.27 6.604)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 8.382) (xy -0.508 8.382)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 6.858) (xy -0.508 6.858)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start -1.27 6.096)
				(end 1.27 4.064)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 5.842) (xy -0.508 5.842)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 4.318) (xy -0.508 4.318)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start -1.27 3.556)
				(end 1.27 1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 3.302) (xy -0.508 3.302)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 1.778) (xy -0.508 1.778)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start -1.27 1.016)
				(end 1.27 -1.016)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 0.762) (xy -0.508 0.762)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 -0.762) (xy -0.508 -0.762)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -0.508 8.382)
				(mid -0.2551 8.128)
				(end -0.508 7.874)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -0.508 7.874)
				(mid -0.2551 7.62)
				(end -0.508 7.366)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -0.508 7.366)
				(mid -0.2551 7.112)
				(end -0.508 6.858)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -0.508 5.842)
				(mid -0.2551 5.588)
				(end -0.508 5.334)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -0.508 5.334)
				(mid -0.2551 5.08)
				(end -0.508 4.826)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -0.508 4.826)
				(mid -0.2551 4.572)
				(end -0.508 4.318)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -0.508 3.302)
				(mid -0.2551 3.048)
				(end -0.508 2.794)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -0.508 2.794)
				(mid -0.2551 2.54)
				(end -0.508 2.286)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -0.508 2.286)
				(mid -0.2551 2.032)
				(end -0.508 1.778)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -0.508 0.762)
				(mid -0.2551 0.508)
				(end -0.508 0.254)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -0.508 0.254)
				(mid -0.2551 0)
				(end -0.508 -0.254)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -0.508 -0.254)
				(mid -0.2551 -0.508)
				(end -0.508 -0.762)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 15.24) (xy 0 14.605)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 12.7) (xy 0 13.97)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 10.795) (xy 0 12.065)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 8.89) (xy 0 10.16)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -1.27) (xy 0 -2.54)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -3.175) (xy 0 -4.445)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -5.08) (xy 0 -6.35)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -6.985) (xy 0 -8.255)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -8.89) (xy 0 -10.16)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -10.795) (xy 0 -12.065)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -12.7) (xy 0 -13.97)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -14.605) (xy 0 -15.24)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 0.508 7.874)
				(mid 0.255 8.128)
				(end 0.508 8.382)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 0.508 7.366)
				(mid 0.255 7.62)
				(end 0.508 7.874)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 0.508 6.858)
				(mid 0.255 7.112)
				(end 0.508 7.366)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 0.508 5.334)
				(mid 0.255 5.588)
				(end 0.508 5.842)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 0.508 4.826)
				(mid 0.255 5.08)
				(end 0.508 5.334)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 0.508 4.318)
				(mid 0.255 4.572)
				(end 0.508 4.826)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 0.508 2.794)
				(mid 0.255 3.048)
				(end 0.508 3.302)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 0.508 2.286)
				(mid 0.255 2.54)
				(end 0.508 2.794)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 0.508 1.778)
				(mid 0.255 2.032)
				(end 0.508 2.286)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 0.508 0.254)
				(mid 0.255 0.508)
				(end 0.508 0.762)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 0.508 -0.254)
				(mid 0.255 0)
				(end 0.508 0.254)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 0.508 -0.762)
				(mid 0.255 -0.508)
				(end 0.508 -0.254)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 8.382) (xy 0.508 8.382)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 6.858) (xy 0.508 6.858)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 5.842) (xy 0.508 5.842)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 4.318) (xy 0.508 4.318)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 3.302) (xy 0.508 3.302)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 1.778) (xy 0.508 1.778)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0.762) (xy 0.508 0.762)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -0.762) (xy 0.508 -0.762)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start 1.905 8.255)
				(end 6.985 6.985)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 7.62) (xy 1.27 7.62)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start 1.905 5.715)
				(end 6.985 4.445)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 5.08) (xy 1.27 5.08)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start 1.905 3.175)
				(end 6.985 1.905)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 2.54) (xy 1.27 2.54)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start 1.905 0.635)
				(end 6.985 -0.635)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 0) (xy 1.27 0)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 4.445 5.715) (xy 4.445 6.985)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 4.445 3.175) (xy 4.445 4.445)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 4.445 0.635) (xy 4.445 1.905)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.715 -5.08) (xy 4.445 -5.08) (xy 4.445 -0.635)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 6.985 7.62) (xy 7.62 7.62)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 6.985 5.08) (xy 7.62 5.08)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 6.985 2.54) (xy 7.62 2.54)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 6.985 0) (xy 7.62 0)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(text "ENCODE"
				(at -4.445 7.62 0)
				(effects
					(font
						(size 0.635 0.635)
					)
				)
			)
			(text "ENCODE"
				(at -4.445 5.08 0)
				(effects
					(font
						(size 0.635 0.635)
					)
				)
			)
			(text "ENCODE"
				(at -4.445 2.54 0)
				(effects
					(font
						(size 0.635 0.635)
					)
				)
			)
			(text "DECODE"
				(at -4.445 0 0)
				(effects
					(font
						(size 0.635 0.635)
					)
				)
			)
			(text "DECODE"
				(at 4.445 7.62 0)
				(effects
					(font
						(size 0.635 0.635)
					)
				)
			)
			(text "DECODE"
				(at 4.445 5.08 0)
				(effects
					(font
						(size 0.635 0.635)
					)
				)
			)
			(text "DECODE"
				(at 4.445 2.54 0)
				(effects
					(font
						(size 0.635 0.635)
					)
				)
			)
			(text "ENCODE"
				(at 4.445 0 0)
				(effects
					(font
						(size 0.635 0.635)
					)
				)
			)
		)
		(symbol "CA-IS3741xN_0_1"
			(rectangle
				(start -12.7 15.24)
				(end 12.7 -15.24)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(rectangle
				(start -1.905 8.255)
				(end -6.985 6.985)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start -1.905 5.715)
				(end -6.985 4.445)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start -1.905 3.175)
				(end -6.985 1.905)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
		)
		(symbol "CA-IS3741xN_1_1"
			(pin power_in line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "VDDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VI1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "VI2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "VI3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at -15.24 0 0)
				(length 2.54)
				(name "VO4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "ENA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "GNDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "GNDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "VDDB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VO1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "VO2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "VO3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "VI4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "ENB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "GNDB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "GNDB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "CJ431"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 2.54 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "CJ431"
			(at 0 -2.54 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -3.81 0)
			(effects
				(font
					(size 1.27 1.27)
					(italic yes)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://atta.szlcsc.com/upload/public/pdf/source/20180115/C3113_15160149461261269385.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
					(italic yes)
				)
				(hide yes)
			)
		)
		(property "Description" "Shunt Regulator, SOT-23"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "diode device shunt regulator"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "SOT?23* SOT?89* TO?92*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "CJ431_0_1"
			(polyline
				(pts
					(xy -1.27 0) (xy 0 0) (xy 1.27 0)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -0.762 0.762) (xy 0.762 0) (xy -0.762 -0.762) (xy -0.762 0.762)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0.508 -1.016) (xy 0.762 -0.762) (xy 0.762 0.762) (xy 0.762 0.762)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
		)
		(symbol "CJ431_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 1.524)
				(name "A"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 0.635 0.635)
						)
					)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.159)
				(name "REF"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0.635 0.635)
						)
					)
				)
			)
			(pin passive line
				(at 2.54 0 180)
				(length 1.524)
				(name "K"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0.635 0.635)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "CSC7133D"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.27 10.16 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "CSC7133D"
			(at -5.08 7.62 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "tj_IC:SOP-7_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
					(italic yes)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.xhcicled.com/?c=download&id=1058"
			(at 0 -1.27 90)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "低待机功耗原边反馈 AC/DC 驱动芯片"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "CSC7133D_0_0"
			(pin passive line
				(at 7.62 -3.81 180)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "CSC7133D_0_1"
			(rectangle
				(start -5.08 -6.35)
				(end 5.08 6.35)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(symbol "CSC7133D_1_1"
			(pin input line
				(at -7.62 3.81 0)
				(length 2.54)
				(name "FB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -7.62 1.27 0)
				(length 2.54)
				(name "VCC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -7.62 -1.27 0)
				(length 2.54)
				(name "CS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 -3.81 0)
				(length 2.54)
				(name "E"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin open_collector line
				(at 7.62 3.81 180)
				(length 2.54)
				(name "HV"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin open_collector line
				(at 7.62 1.27 180)
				(length 2.54)
				(name "HV"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "CSC7720"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.27 -7.62 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "CSC7720"
			(at -5.08 -10.16 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_SO:SOP-8_3.9x4.9mm_P1.27mm"
			(at 0 -1.27 0)
			(effects
				(font
					(size 1.27 1.27)
					(italic yes)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.xhcicled.com/?c=download&id=1058"
			(at 0 -1.27 90)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "同步整流控制器芯片"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "PowerIntegrations?eSIP?7C*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "CSC7720_0_0"
			(pin open_collector line
				(at 10.16 3.81 180)
				(length 2.54)
				(name "SW"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin open_collector line
				(at 10.16 1.27 180)
				(length 2.54)
				(name "SW"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "CSC7720_0_1"
			(rectangle
				(start -7.62 -6.35)
				(end 7.62 6.35)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(symbol "CSC7720_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 0 8.89 270)
				(length 2.54)
				(name "VCC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin open_collector line
				(at 10.16 -1.27 180)
				(length 2.54)
				(name "SW"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin open_collector line
				(at 10.16 -3.81 180)
				(length 2.54)
				(name "SW"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "CX7527C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "CX7527C"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_SO:SOP-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "http://tj20.top:81/datasheet/CX7527X-60V_Datasheet_ReV1.0.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "高性能多模式 PWM反激式控制器,AC/DC"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "PWM,AC/DC,PWM"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "CX7527C_0_0"
			(pin free line
				(at -10.16 1.27 0)
				(length 2.54)
				(name "Cs"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -10.16 -3.81 0)
				(length 2.54)
				(name "Fb"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 8.89 270)
				(length 2.54)
				(name "Vdd"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -8.89 90)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin open_collector line
				(at 10.16 3.81 180)
				(length 2.54)
				(name "Drain"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin open_collector line
				(at 10.16 1.27 180)
				(length 2.54)
				(name "Drain"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin open_collector line
				(at 10.16 -1.27 180)
				(length 2.54)
				(name "Drain"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin open_collector line
				(at 10.16 -3.81 180)
				(length 2.54)
				(name "Drain"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "CX7527C_1_1"
			(rectangle
				(start -7.62 6.35)
				(end 7.62 -6.35)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type color)
					(color 255 255 194 1)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "DG4052A"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "DG4052A"
			(at -3.81 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SOP65P640-16N"
			(at -5.08 -40.64 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Analog Multiplexer/Demultiplexer"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Vishay"
			(at -5.08 -43.18 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Package" "TSSOP-16"
			(at -5.08 -48.26 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -5.08 -50.8 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -5.08 -53.34 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Part_Number" "DG4052AEQ-T1-E3"
			(at -5.08 -55.88 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right bottom)
			)
		)
		(symbol "DG4052A_1_1"
			(rectangle
				(start 0 -35.56)
				(end 17.78 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin input line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "~{EN}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 -7.62 0)
				(length 5.08)
				(name "A"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 -10.16 0)
				(length 5.08)
				(name "B"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -15.24 0)
				(length 5.08)
				(name "X"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -27.94 0)
				(length 5.08)
				(name "Y"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -5.08 -33.02 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "VCC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "X0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "X1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "X2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "X3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 5.08)
				(name "Y0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "Y1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "Y2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "Y3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "VEE"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "DG409DQ"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 20.955 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "DG409DQ"
			(at -7.62 19.05 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 6.35 -21.59 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.vishay.com/docs/70062/dg408.pdf"
			(at 0.254 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Dual 4-Ch High-Performance CMOS Analog Multiplexers"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "analog switch selector multiplexer Dual  4-to-1"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "DG409DQ_0_1"
			(rectangle
				(start -7.62 17.78)
				(end 7.62 -20.32)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(rectangle
				(start -7.62 6.35)
				(end -2.54 16.51)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.032 11.43) (xy -2.54 11.43)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.524 2.54) (xy -3.302 2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.524 0) (xy -3.302 0)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.524 -2.54) (xy -3.302 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.524 -5.08) (xy -3.302 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.524 -10.16) (xy -3.302 -10.16)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.524 -12.7) (xy -3.302 -12.7)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.524 -15.24) (xy -3.302 -15.24)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.524 -17.78) (xy -3.302 -17.78)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 11.43) (xy -0.635 11.43)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 3.556) (xy 1.778 3.556)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 1.016) (xy 1.778 1.016)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 -1.524) (xy 1.778 -1.524)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 -4.064) (xy 1.778 -4.064)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 -9.144) (xy 1.778 -9.144)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 -11.684) (xy 1.778 -11.684)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 -14.224) (xy 1.778 -14.224)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 -16.764) (xy 1.778 -16.764)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center -1.016 2.54)
				(radius 0.508)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center -1.016 0)
				(radius 0.508)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center -1.016 -2.54)
				(radius 0.508)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center -1.016 -5.08)
				(radius 0.508)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center -1.016 -10.16)
				(radius 0.508)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center -1.016 -12.7)
				(radius 0.508)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center -1.016 -15.24)
				(radius 0.508)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center -1.016 -17.78)
				(radius 0.508)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.254 11.43) (xy 0 11.43)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.254 10.16) (xy 0.254 10.922)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.254 8.89) (xy 0.254 9.525)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.254 7.62) (xy 0.254 8.255)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.254 6.35) (xy 0.254 6.985)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.254 5.08) (xy 0.254 5.715)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.254 3.81) (xy 0.254 4.445)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.254 2.54) (xy 0.254 3.175)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.254 1.27) (xy 0.254 1.905)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.254 0) (xy 0.254 0.635)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.254 -1.27) (xy 0.254 -0.635)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.254 -2.54) (xy 0.254 -1.905)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.254 -3.81) (xy 0.254 -3.175)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.254 -5.334) (xy 0.254 -4.699)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.254 -6.604) (xy 0.254 -5.969)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.254 -7.874) (xy 0.254 -7.239)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.254 -9.144) (xy 0.254 -8.509)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.254 -10.414) (xy 0.254 -9.779)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.254 -11.684) (xy 0.254 -11.049)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.254 -12.954) (xy 0.254 -12.319)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.254 -14.224) (xy 0.254 -13.589)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.254 -15.494) (xy 0.254 -14.859)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.254 -16.764) (xy 0.254 -16.129)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 1.524 2.54)
				(radius 0.508)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 1.524 0)
				(radius 0.508)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 1.524 -2.54)
				(radius 0.508)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 1.524 -5.08)
				(radius 0.508)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 1.524 -10.16)
				(radius 0.508)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 1.524 -12.7)
				(radius 0.508)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 1.524 -15.24)
				(radius 0.508)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 1.524 -17.78)
				(radius 0.508)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 -5.08) (xy 2.54 -5.08) (xy 2.54 2.54) (xy 1.905 2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 -10.16) (xy 2.54 -10.16) (xy 2.54 -17.78) (xy 1.905 -17.78)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.032 0) (xy 2.54 0)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.032 -2.54) (xy 2.54 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.032 -12.7) (xy 2.54 -12.7)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.032 -15.24) (xy 2.54 -15.24)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0) (xy 4.572 0)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 4.572 -12.7) (xy 2.54 -12.7)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
		)
		(symbol "DG409DQ_1_1"
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "A0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "A1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "EN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "S1A"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "S2A"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "S3A"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "S4A"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "S1B"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "S2B"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "S3B"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "S4B"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 5.08 -22.86 90)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "V+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "V-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "DA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "DB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "DSPIC30F6014A-30I_PF"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 1.27 0)
			(effects
				(font
					(size 1.397 1.397)
				)
				(justify left bottom)
			)
		)
		(property "Value" "DSPIC30F6014A-30I_PF"
			(at -6.35 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "Package_QFP:TQFP-80_14x14mm_P0.65mm"
			(at -7.62 -134.62 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "High-Performance 16-bit Digital Signal Controller, 144 KB Flash, 8 KB SRAM, 4 KB EEPROM, 80-Pin TQFP, Industrial Temperature"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "DSPIC30F6014A-30I_PF_1_1"
			(rectangle
				(start 0 -129.54)
				(end 58.42 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 7.62)
				(name "~{MCLR}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input clock
				(at -7.62 -7.62 0)
				(length 7.62)
				(name "OSC1/CLKI"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "49"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 -12.7 0)
				(length 7.62)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 -15.24 0)
				(length 7.62)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 -17.78 0)
				(length 7.62)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 -20.32 0)
				(length 7.62)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "71"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 -22.86 0)
				(length 7.62)
				(name "AVDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 -27.94 0)
				(length 7.62)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 -30.48 0)
				(length 7.62)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 -33.02 0)
				(length 7.62)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "51"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 -35.56 0)
				(length 7.62)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "70"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 -38.1 0)
				(length 7.62)
				(name "AVSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -73.66 0)
				(length 7.62)
				(name "C1RX/RF0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "72"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -76.2 0)
				(length 7.62)
				(name "C1TX/RF1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "73"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -78.74 0)
				(length 7.62)
				(name "U1RX/RF2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -81.28 0)
				(length 7.62)
				(name "U1TX/RF3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -83.82 0)
				(length 7.62)
				(name "U2RX/CN17/RF4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -86.36 0)
				(length 7.62)
				(name "U2TX/CN18/RF5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional clock
				(at -7.62 -88.9 0)
				(length 7.62)
				(name "EMUC3/SCK1/INT0/RF6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -91.44 0)
				(length 7.62)
				(name "SDI1/RF7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -93.98 0)
				(length 7.62)
				(name "EMUD3/SDO1/RF8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -99.06 0)
				(length 7.62)
				(name "C2RX/RG0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "75"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -101.6 0)
				(length 7.62)
				(name "C2TX/RG1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "74"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional clock
				(at -7.62 -104.14 0)
				(length 7.62)
				(name "SCL/RG2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -106.68 0)
				(length 7.62)
				(name "SDA/RG3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional clock
				(at -7.62 -109.22 0)
				(length 7.62)
				(name "SCK2/CN8/RG6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -111.76 0)
				(length 7.62)
				(name "SDI2/CN9/RG7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -114.3 0)
				(length 7.62)
				(name "SDO2/CN10/RG8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -116.84 0)
				(length 7.62)
				(name "~{SS2}/CN11/RG9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -119.38 0)
				(length 7.62)
				(name "CSDI/RG12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "79"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -121.92 0)
				(length 7.62)
				(name "CSDO/RG13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "80"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional clock
				(at -7.62 -124.46 0)
				(length 7.62)
				(name "CSCK/RG14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "78"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -127 0)
				(length 7.62)
				(name "COFS/RG15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -2.54 180)
				(length 7.62)
				(name "CN22/RA6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "76"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -5.08 180)
				(length 7.62)
				(name "CN23/RA7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "77"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -7.62 180)
				(length 7.62)
				(name "VREF-/RA9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -10.16 180)
				(length 7.62)
				(name "VREF+/RA10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -12.7 180)
				(length 7.62)
				(name "INT1/RA12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -15.24 180)
				(length 7.62)
				(name "INT2/RA13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -17.78 180)
				(length 7.62)
				(name "INT3/RA14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "52"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -20.32 180)
				(length 7.62)
				(name "INT4/RA15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "53"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -25.4 180)
				(length 7.62)
				(name "PGD/EMUD/AN0/CN2/RB0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional clock
				(at 66.04 -27.94 180)
				(length 7.62)
				(name "PGC/EMUC/AN1/CN3/RB1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -30.48 180)
				(length 7.62)
				(name "AN2/~{SS1}/LVDIN/CN4/RB2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -33.02 180)
				(length 7.62)
				(name "AN3/CN5/RB3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -35.56 180)
				(length 7.62)
				(name "AN4/CN6/RB4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -38.1 180)
				(length 7.62)
				(name "AN5/CN7/RB5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -40.64 180)
				(length 7.62)
				(name "AN6/OCFA/RB6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -43.18 180)
				(length 7.62)
				(name "AN7/RB7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -45.72 180)
				(length 7.62)
				(name "AN8/RB8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -48.26 180)
				(length 7.62)
				(name "AN9/RB9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -50.8 180)
				(length 7.62)
				(name "AN10/RB10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -53.34 180)
				(length 7.62)
				(name "AN11/RB11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -55.88 180)
				(length 7.62)
				(name "AN12/RB12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -58.42 180)
				(length 7.62)
				(name "AN13/RB13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -60.96 180)
				(length 7.62)
				(name "AN14/RB14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -63.5 180)
				(length 7.62)
				(name "AN15/OCFB/CN12/RB15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional clock
				(at 66.04 -68.58 180)
				(length 7.62)
				(name "T2CK/RC1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional clock
				(at 66.04 -71.12 180)
				(length 7.62)
				(name "T3CK/RC2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional clock
				(at 66.04 -73.66 180)
				(length 7.62)
				(name "T4CK/RC3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional clock
				(at 66.04 -76.2 180)
				(length 7.62)
				(name "T5CK/RC4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional clock
				(at 66.04 -78.74 180)
				(length 7.62)
				(name "EMUD1/SOSCI/CN1/RC13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "59"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional clock
				(at 66.04 -81.28 180)
				(length 7.62)
				(name "EMUC1/SOSCO/T1CK/CN0/RC14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "60"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -83.82 180)
				(length 7.62)
				(name "OSC2/CLKO/RC15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "50"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -88.9 180)
				(length 7.62)
				(name "EMUC2/OC1/RD0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "58"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -91.44 180)
				(length 7.62)
				(name "EMUD2/OC2/RD1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "61"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -93.98 180)
				(length 7.62)
				(name "OC3/RD2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "62"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -96.52 180)
				(length 7.62)
				(name "OC4/RD3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "63"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -99.06 180)
				(length 7.62)
				(name "OC5/CN13/RD4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "66"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -101.6 180)
				(length 7.62)
				(name "OC6/CN14/RD5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "67"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -104.14 180)
				(length 7.62)
				(name "OC7/CN15/RD6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "68"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -106.68 180)
				(length 7.62)
				(name "OC8/CN16/RD7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "69"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -109.22 180)
				(length 7.62)
				(name "IC1/RD8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "54"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -111.76 180)
				(length 7.62)
				(name "IC2/RD9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "55"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -114.3 180)
				(length 7.62)
				(name "IC3/RD10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "56"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -116.84 180)
				(length 7.62)
				(name "IC4/RD11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "57"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -119.38 180)
				(length 7.62)
				(name "IC5/RD12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "64"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -121.92 180)
				(length 7.62)
				(name "IC6/CN19/RD13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "65"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -124.46 180)
				(length 7.62)
				(name "IC7/CN20/RD14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 66.04 -127 180)
				(length 7.62)
				(name "IC8/CN21/RD15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "EL354N"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "EL354N"
			(at -3.81 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SOP2.54-4"
			(at -5.08 -15.24 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "4-Pin Phototransistor Optocoupler"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Package" "SOP-4"
			(at -5.08 -20.32 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -5.08 -22.86 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -5.08 -25.4 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Manufacturer" "EL"
			(at -5.08 -27.94 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Part_Number" "EL354N(A)(TA)-G"
			(at -5.08 -30.48 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Comment" "354"
			(at -1.27 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(symbol "EL354N_1_1"
			(polyline
				(pts
					(xy 0 -2.54) (xy 7.874 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -7.62) (xy 7.874 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start 0 -10.16)
				(end 20.32 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 1.27 -3.81) (xy 5.334 -3.81) (xy 3.302 -5.842) (xy 1.27 -3.81)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 3.302 -2.54) (xy 3.302 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.334 -6.096) (xy 5.334 -6.35) (xy 1.27 -6.35) (xy 1.27 -6.096) (xy 5.334 -6.096)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 5.842 -4.064) (xy 5.842 -3.81) (xy 9.906 -3.81) (xy 9.906 -4.064) (xy 5.842 -4.064)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 7.874 -7.62) (xy 7.874 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 9.906 -6.35) (xy 5.842 -6.35) (xy 7.874 -4.318) (xy 9.906 -6.35)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 11.684 -3.302) (xy 10.16 -4.826)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 11.684 -3.81) (xy 11.684 -3.302) (xy 11.176 -3.302) (xy 11.684 -3.81)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 11.684 -4.572) (xy 10.16 -6.096)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 11.684 -5.08) (xy 11.684 -4.572) (xy 11.176 -4.572) (xy 11.684 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 14.478 -3.302) (xy 14.224 -3.302) (xy 14.224 -6.858) (xy 14.478 -6.858) (xy 14.478 -3.302)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 14.478 -5.842) (xy 16.256 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 16.002 -2.54) (xy 14.478 -4.064)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 16.002 -2.54) (xy 20.32 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 16.002 -6.604) (xy 16.002 -7.366) (xy 15.24 -7.366) (xy 16.002 -6.604)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 16.256 -7.62) (xy 20.32 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "A"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 5.08)
				(name "K"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "C"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "E"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "EL357N"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "EL357N"
			(at -1.27 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SOP2.54-4"
			(at -2.54 -14.224 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "4-Pin Phototransistor Optocoupler"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Package" "SOP-4"
			(at -2.54 -19.304 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Part_Number1" "PC357N3"
			(at -2.54 -21.844 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Manufacturer" "EL"
			(at -2.54 -24.384 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -2.54 -26.924 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -2.54 -29.464 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Part_Number" "EL357N(C)(TA)-G"
			(at -2.54 -32.004 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Comment" "357"
			(at 1.27 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(symbol "EL357N_1_1"
			(polyline
				(pts
					(xy 2.54 -1.016) (xy 2.54 -9.144)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -1.016) (xy 17.78 -1.016)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -2.54) (xy 5.842 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -7.62) (xy 5.842 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -9.144) (xy 17.78 -9.144)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 -3.81) (xy 7.874 -3.81) (xy 5.842 -5.842) (xy 3.81 -3.81)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 5.842 -2.54) (xy 5.842 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.874 -6.096) (xy 7.874 -6.35) (xy 3.81 -6.35) (xy 3.81 -6.096) (xy 7.874 -6.096)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 11.176 -3.302) (xy 9.652 -4.826)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 11.176 -3.81) (xy 11.176 -3.302) (xy 10.668 -3.302) (xy 11.176 -3.81)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 11.176 -4.572) (xy 9.652 -6.096)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 11.176 -5.08) (xy 11.176 -4.572) (xy 10.668 -4.572) (xy 11.176 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 13.462 -3.302) (xy 13.208 -3.302) (xy 13.208 -6.858) (xy 13.462 -6.858) (xy 13.462 -3.302)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 13.462 -5.842) (xy 15.24 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 14.986 -2.54) (xy 13.462 -4.064)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 14.986 -2.54) (xy 17.78 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 14.986 -6.604) (xy 14.986 -7.366) (xy 14.224 -7.366) (xy 14.986 -6.604)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 15.24 -7.62) (xy 17.78 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 17.78 -1.016) (xy 17.78 -9.144)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -2.54 -2.54 0)
				(length 5.08)
				(name "A"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.54 -7.62 0)
				(length 5.08)
				(name "K"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "C"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "E"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "HS1838"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -0.0254 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "HS1838"
			(at 1.2446 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "HS1838"
			(at -0.0254 -20.32 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "红外线接收头"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Part_Number" "HS1838"
			(at -0.0254 -22.86 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Note" "*"
			(at -0.0254 -25.4 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Package" "HS1838"
			(at -0.0254 -27.94 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "插件"
			(at -0.0254 -30.48 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -0.0254 -33.02 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(symbol "HS1838_1_1"
			(rectangle
				(start 0 -15.24)
				(end 20.32 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 3.556 -6.35) (xy 3.556 -6.858) (xy 3.048 -6.858) (xy 3.556 -6.35)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 3.556 -6.858) (xy 2.032 -5.334)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.556 -7.62) (xy 3.556 -8.128) (xy 3.048 -8.128) (xy 3.556 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 3.556 -8.128) (xy 2.032 -6.604)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -8.89) (xy 9.144 -8.89) (xy 7.112 -6.858) (xy 5.08 -8.89)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 7.112 -10.16) (xy 7.112 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 9.144 -6.604) (xy 9.144 -6.35) (xy 5.08 -6.35) (xy 5.08 -6.604) (xy 9.144 -6.604)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "VCC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO1050DUB"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "ISO1050DUB"
			(at -3.81 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SOP2.54-8"
			(at -5.08 -25.4 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Package" "SOP2.54-8"
			(at -5.08 -33.02 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -5.08 -38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -5.08 -40.64 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Price" "6"
			(at -5.08 -43.18 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Part_Number" "ISO1050DUB"
			(at -5.08 -45.72 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(symbol "ISO1050DUB_1_1"
			(rectangle
				(start 0 -20.32)
				(end 8.382 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(rectangle
				(start 8.382 -20.32)
				(end 9.398 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(rectangle
				(start 9.398 -20.32)
				(end 17.78 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "VCC1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 5.08)
				(name "RxD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 5.08)
				(name "TxD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 5.08)
				(name "GND1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "VCC2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "CANH"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "CANL"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "GND2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO3082DW"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "ISO3082DW"
			(at -3.81 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SOIC127P1030-16M"
			(at -5.08 -35.56 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Isolated 5-V Half-Duplex RS-485 Transceivers"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Note" "*"
			(at -5.08 -38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Manufacturer" "TI"
			(at -5.08 -40.64 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -5.08 -43.18 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -5.08 -45.72 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Price" "8.5"
			(at -5.08 -48.26 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "供应商" "力创"
			(at -5.08 -50.8 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Package" "SOIC-16"
			(at -5.08 -53.34 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Part_Number" "ISO3082DW"
			(at -5.08 -55.88 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(symbol "ISO3082DW_1_1"
			(rectangle
				(start 0 -30.48)
				(end 20.32 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(rectangle
				(start 8.89 -30.48)
				(end 11.43 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin power_in line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "VCC1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 5.08)
				(name "GND1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at -5.08 -10.16 0)
				(length 5.08)
				(name "R"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 -15.24 0)
				(length 5.08)
				(name "RE"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 -17.78 0)
				(length 5.08)
				(name "DE"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 -22.86 0)
				(length 5.08)
				(name "D"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -5.08 -25.4 0)
				(length 5.08)
				(name "GND1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -5.08 -27.94 0)
				(length 5.08)
				(name "GND1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "VCC2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "GND2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "NC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "B"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "A"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "NC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "GND2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "GND2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "JW3510"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 8.89 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "JW3510"
			(at -6.35 8.89 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 16.51 -8.89 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.joulwatt.com/Upload/file/201905/20190521175642_0919.pdf"
			(at 2.54 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "42VIN Micropower No-Opto Isolated Flyback Converter with 65V/1.4A Switch"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Flyback switcher"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "JW3510_0_1"
			(rectangle
				(start -7.62 7.62)
				(end 7.62 -7.62)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(symbol "JW3510_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN/UVLO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "RFB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "LDS-1106AX"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "DS"
			(at -5.08 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "LDS-1106AX"
			(at -3.81 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "LEDDIP-10/C30.48RHD"
			(at -5.08 -27.94 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "7段数码管，共阴，字高1英寸,3,8脚公共线"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Package" "LEDDIP-10/C30.48RHD"
			(at -5.08 -30.48 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Part_Number" "LDS-1106AX"
			(at -5.08 -33.02 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Colour" "Red"
			(at -5.08 -38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "插件"
			(at -5.08 -40.64 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Price" "1.0"
			(at -5.08 -43.18 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -5.08 -48.26 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Created" "23/09/2003"
			(at -5.08 -50.8 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(symbol "LDS-1106AX_1_1"
			(rectangle
				(start 0 -22.86)
				(end 15.24 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 4.826 -16.51) (xy 5.334 -16.256) (xy 9.144 -16.256) (xy 9.652 -16.51) (xy 9.144 -16.764) (xy 5.334 -16.764)
					(xy 4.826 -16.51) (xy 4.826 -16.51)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 5.334 -11.43) (xy 5.842 -11.176) (xy 9.652 -11.176) (xy 10.16 -11.43) (xy 9.652 -11.684) (xy 5.842 -11.684)
					(xy 5.334 -11.43) (xy 5.334 -11.43)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 5.334 -11.684) (xy 5.08 -11.938) (xy 4.572 -16.002) (xy 4.826 -16.256) (xy 5.08 -16.002) (xy 5.588 -11.938)
					(xy 5.334 -11.684) (xy 5.334 -11.684)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 5.842 -6.35) (xy 6.35 -6.096) (xy 10.16 -6.096) (xy 10.668 -6.35) (xy 10.16 -6.604) (xy 6.35 -6.604)
					(xy 5.842 -6.35) (xy 5.842 -6.35)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 5.842 -6.604) (xy 5.588 -6.858) (xy 5.08 -10.922) (xy 5.334 -11.176) (xy 5.588 -10.922) (xy 6.096 -6.858)
					(xy 5.842 -6.604) (xy 5.842 -6.604)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 10.414 -11.684) (xy 10.16 -11.938) (xy 9.652 -16.002) (xy 9.906 -16.256) (xy 10.16 -16.002)
					(xy 10.668 -11.938) (xy 10.414 -11.684) (xy 10.414 -11.684)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 10.922 -6.604) (xy 10.668 -6.858) (xy 10.16 -10.922) (xy 10.414 -11.176) (xy 10.668 -10.922)
					(xy 11.176 -6.858) (xy 10.922 -6.604) (xy 10.922 -6.604)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(circle
				(center 12.446 -16.51)
				(radius 0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "a"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 5.08)
				(name "b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 5.08)
				(name "c"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 5.08)
				(name "d"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 5.08)
				(name "e"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 5.08)
				(name "f"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 5.08)
				(name "g"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 5.08)
				(name "dp"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "C"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "C"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "LDS-8106AX"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "DS"
			(at -5.08 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "LDS-8106AX"
			(at -3.81 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "LEDDIP-10/C21.60RHD"
			(at -5.08 -27.94 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "7段数码管，共阴，字高0.8英寸,3,8脚公共线"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Package" "LEDDIP-10/C30.48RHD"
			(at -5.08 -30.48 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Part_Number" "LDS-8106AX"
			(at -5.08 -33.02 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Colour" "Red"
			(at -5.08 -38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "插件"
			(at -5.08 -40.64 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Price" "0.6"
			(at -5.08 -43.18 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -5.08 -48.26 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Created" "23/09/2003"
			(at -5.08 -50.8 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(symbol "LDS-8106AX_1_1"
			(rectangle
				(start 0 -22.86)
				(end 15.24 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 4.826 -16.51) (xy 5.334 -16.256) (xy 9.144 -16.256) (xy 9.652 -16.51) (xy 9.144 -16.764) (xy 5.334 -16.764)
					(xy 4.826 -16.51) (xy 4.826 -16.51)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 5.334 -11.43) (xy 5.842 -11.176) (xy 9.652 -11.176) (xy 10.16 -11.43) (xy 9.652 -11.684) (xy 5.842 -11.684)
					(xy 5.334 -11.43) (xy 5.334 -11.43)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 5.334 -11.684) (xy 5.08 -11.938) (xy 4.572 -16.002) (xy 4.826 -16.256) (xy 5.08 -16.002) (xy 5.588 -11.938)
					(xy 5.334 -11.684) (xy 5.334 -11.684)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 5.842 -6.35) (xy 6.35 -6.096) (xy 10.16 -6.096) (xy 10.668 -6.35) (xy 10.16 -6.604) (xy 6.35 -6.604)
					(xy 5.842 -6.35) (xy 5.842 -6.35)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 5.842 -6.604) (xy 5.588 -6.858) (xy 5.08 -10.922) (xy 5.334 -11.176) (xy 5.588 -10.922) (xy 6.096 -6.858)
					(xy 5.842 -6.604) (xy 5.842 -6.604)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 10.414 -11.684) (xy 10.16 -11.938) (xy 9.652 -16.002) (xy 9.906 -16.256) (xy 10.16 -16.002)
					(xy 10.668 -11.938) (xy 10.414 -11.684) (xy 10.414 -11.684)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 10.922 -6.604) (xy 10.668 -6.858) (xy 10.16 -10.922) (xy 10.414 -11.176) (xy 10.668 -10.922)
					(xy 11.176 -6.858) (xy 10.922 -6.604) (xy 10.922 -6.604)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(circle
				(center 12.446 -16.51)
				(radius 0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "a"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 5.08)
				(name "b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 5.08)
				(name "c"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 5.08)
				(name "d"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 5.08)
				(name "e"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 5.08)
				(name "f"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 5.08)
				(name "g"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 5.08)
				(name "dp"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "C"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "C"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM335DT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 13.97 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "LM335DT"
			(at 3.81 -2.54 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/lm335.pdf"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Precision temperature sensors"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "LM335DT_0_1"
			(rectangle
				(start -1.27 6.35)
				(end -1.27 6.35)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start 2.54 1.27)
				(end 2.54 1.27)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start 2.54 0)
				(end 2.54 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
		)
		(symbol "LM335DT_1_1"
			(rectangle
				(start 0 12.7)
				(end 8.89 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin no_connect line
				(at -2.54 10.16 0)
				(length 2.54)
				(name "NC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin no_connect line
				(at -2.54 7.62 0)
				(length 2.54)
				(name "NC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin no_connect line
				(at -2.54 5.08 0)
				(length 2.54)
				(name "NC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin free line
				(at -2.54 2.54 0)
				(length 2.54)
				(name "V-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin free line
				(at 11.43 10.16 180)
				(length 2.54)
				(name "V+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin no_connect line
				(at 11.43 7.62 180)
				(length 2.54)
				(name "NC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin no_connect line
				(at 11.43 5.08 180)
				(length 2.54)
				(name "NC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 11.43 2.54 180)
				(length 2.54)
				(name "ADJ"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM335Z"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 2.54 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "LM335Z"
			(at 0 -2.54 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Wide"
			(at 0 -3.81 0)
			(effects
				(font
					(size 1.27 1.27)
					(italic yes)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/lm335.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
					(italic yes)
				)
				(hide yes)
			)
		)
		(property "Description" "Precision temperature sensors, TO-92"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "TO*92*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "LM335Z_0_1"
			(polyline
				(pts
					(xy -1.27 0) (xy 0 0) (xy 1.27 0)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -0.762 0.762) (xy 0.762 0) (xy -0.762 -0.762)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0.508 -1.016) (xy 0.762 -0.762) (xy 0.762 0.762) (xy 0.762 0.762)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
		)
		(symbol "LM335Z_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "V-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "ADJ"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "V+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM337-N"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "LM337IMP/NOPB"
			(at 0 3.175 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.ti.com/cn/lit/ds/symlink/lm337-n.pdf"
			(at 2.54 -6.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LM337IMP/NOPB  LM337IMPX/NOPB"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "LM337-N_0_1"
			(rectangle
				(start -5.08 -5.08)
				(end 5.08 1.905)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(symbol "LM337-N_1_1"
			(pin power_out line
				(at -7.62 0 0)
				(length 2.54)
				(name "VON"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 7.62 0 180)
				(length 2.54)
				(name "VIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1871"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "LTC1871"
			(at -3.81 8.89 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at -15.24 -12.7 0)
			(effects
				(font
					(size 1.27 1.27)
					(italic yes)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1871fe.pdf"
			(at -6.35 11.43 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Wide Input Range, No RSENSE™ Current Mode Boost,Flyback and SEPIC Controller"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "a wide input range, current mode, boost, flyback or SEPIC controller"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "LTC1871_0_1"
			(rectangle
				(start -10.16 7.62)
				(end 10.16 -10.16)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(symbol "LTC1871_1_0"
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SENSE"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "LTC1871_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "RUN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "ITH"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "FB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "FREQ"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "MODE/SYNC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "INTVcc"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GATE"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX132CNG"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 22.86 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "MAX132CNG"
			(at 25.4 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-24_W7.62mm"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.mouser.cn/datasheet/2/256/MAX132-1514523.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "Package_DIP:DIP-24_W7.62mm Package_SO:SOIC-24W_7.5x15.4mm_P1.27mm"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "MAX132CNG_0_1"
			(rectangle
				(start 0 0)
				(end 29.21 -40.64)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(symbol "MAX132CNG_1_1"
			(pin input line
				(at -5.08 -7.62 0)
				(length 5.08)
				(name "~{CS}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 -10.16 0)
				(length 5.08)
				(name "DIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 5.08)
				(name "DOUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 -15.24 0)
				(length 5.08)
				(name "SCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 5.08)
				(name "EOC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 5.08)
				(name "P0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 5.08)
				(name "P1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 5.08)
				(name "P2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 5.08)
				(name "P3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 5.08 270)
				(length 5.08)
				(name "CREF-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 7.62 -45.72 90)
				(length 5.08)
				(name "OSC1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 17.78 5.08 270)
				(length 5.08)
				(name "CRFEF+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 17.78 -45.72 90)
				(length 5.08)
				(name "OSC2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 34.29 -5.08 180)
				(length 5.08)
				(name "V+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 34.29 -7.62 180)
				(length 5.08)
				(name "BUF_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 34.29 -10.16 180)
				(length 5.08)
				(name "INT_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 34.29 -12.7 180)
				(length 5.08)
				(name "INT_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 34.29 -17.78 180)
				(length 5.08)
				(name "REF+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 34.29 -20.32 180)
				(length 5.08)
				(name "REF-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 34.29 -22.86 180)
				(length 5.08)
				(name "AGND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 34.29 -27.94 180)
				(length 5.08)
				(name "IN_LO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 34.29 -30.48 180)
				(length 5.08)
				(name "IN_HI"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 34.29 -35.56 180)
				(length 5.08)
				(name "V-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 34.29 -38.1 180)
				(length 5.08)
				(name "DGND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX13487EESA+"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.096 11.43 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "MAX13487EESA+"
			(at 0.762 11.43 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" ""
			(at 0 -17.78 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX13487E-MAX13488E.pdf"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Half-Duplex RS-485-/RS-422-Compatible Transceiver with AutoDirection Control, SOIC-8"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Half-Duplex RS-485-/RS-422-Compatible Transceiver with AutoDirection Control, SOIC-8"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "MAX13487EESA+_0_1"
			(rectangle
				(start -7.62 10.16)
				(end 7.62 -12.7)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy -4.826 -7.62) (xy -0.508 -7.62)
				)
				(stroke
					(width 0.127)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -4.064 5.08) (xy -1.27 5.08)
				)
				(stroke
					(width 0.127)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -4.064 0) (xy -1.27 0)
				)
				(stroke
					(width 0.127)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -7.493) (xy -2.54 -3.81) (xy -1.27 -3.81)
				)
				(stroke
					(width 0.127)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 5.08) (xy 1.27 6.35) (xy 1.27 3.81) (xy -1.27 5.08)
				)
				(stroke
					(width 0.127)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start -1.27 1.778)
				(end 1.27 -4.445)
				(stroke
					(width 0.127)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -0.508 -5.715) (xy -0.508 -8.255) (xy 2.032 -6.985) (xy -0.508 -5.715)
				)
				(stroke
					(width 0.127)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -0.508 -5.715) (xy -0.508 -8.255) (xy 2.032 -6.985) (xy -0.508 -5.715)
				)
				(stroke
					(width 0.127)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center -0.0254 4.0386)
				(radius 0.3556)
				(stroke
					(width 0.0508)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 3.81) (xy 0 2.54) (xy 0 1.778)
				)
				(stroke
					(width 0.127)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.127 -4.445) (xy 0.127 -5.9944)
				)
				(stroke
					(width 0.127)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.762 -7.62) (xy 5.207 -7.62)
				)
				(stroke
					(width 0.127)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 1.0922 -6.223)
				(radius 0.3556)
				(stroke
					(width 0.0508)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 1.27 5.715) (xy 3.81 5.715) (xy 3.81 -7.62)
				)
				(stroke
					(width 0.127)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start 1.27 5.715)
				(end 1.27 5.715)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 2.54 0)
				)
				(stroke
					(width 0.127)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -1.905) (xy 3.81 -1.905)
				)
				(stroke
					(width 0.127)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 1.651 4.445)
				(radius 0.3556)
				(stroke
					(width 0.0508)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 1.905 4.445) (xy 4.445 4.445) (xy 4.445 5.08) (xy 5.334 5.08)
				)
				(stroke
					(width 0.127)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.048 4.445) (xy 3.048 -6.35) (xy 1.397 -6.35)
				)
				(stroke
					(width 0.127)
					(type default)
				)
				(fill
					(type none)
				)
			)
		)
		(symbol "MAX13487EESA+_1_1"
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "RO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{RE}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SHDN}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "DI"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "B"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX2323TSSOP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 16.51 0)
			(effects
				(font
					(size 1.143 1.143)
				)
				(justify left bottom)
			)
		)
		(property "Value" "MAX2323TSSOP"
			(at 3.81 -20.32 0)
			(effects
				(font
					(size 1.143 1.143)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "TSSOP16"
			(at 2.54 22.86 0)
			(effects
				(font
					(size 0.508 0.508)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.524 1.524)
				)
				(hide yes)
			)
		)
		(property "Description" "RS232 Transceiver This part covers 232 drivers that are compatible with the MAX3232. <a href=\"http://cdn.sparkfun.com/datasheets/Components/General%20IC/SP3232EBCA-L.pdf\">Sipex SP3232EB Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href=\"https://www.sparkfun.com/products/589\">SOIC component</a> (COM-00589 /  IC-08171)</li><li><b>Retired</b> DIP component (COM-00316 / IC-08446)</li><li><a href=\"https://www.sparkfun.com/products/11189\">SparkFun Transceiver Breakout - MAX3232</a> (BOB-11189)</li><li><a href=\"https://www.sparkfun.com/products/13225\">SparkFun XBee Explorer Serial</a> (WRL-13225)</li></ul>"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "PROD_ID:NA-XXXXX"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "*TSSOP16* *TSSOP-16*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "MAX2323TSSOP_1_1"
			(rectangle
				(start -10.16 15.24)
				(end 15.24 -17.78)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 5.08)
				(name "C1+"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 5.08)
				(name "C1-"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "C2+"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "C2-"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 5.08)
				(name "T1IN"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 5.08)
				(name "T2IN"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin output line
				(at -15.24 -12.7 0)
				(length 5.08)
				(name "R1OUT"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin output line
				(at -15.24 -15.24 0)
				(length 5.08)
				(name "R2OUT"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 5.08)
				(name "VCC"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "V+"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "V-"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin output line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "T1OUT"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin output line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "T2OUT"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin input line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "R1IN"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin input line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "R2IN"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX809STRG"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "MAX809STRG"
			(at -3.81 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SOT23-3N"
			(at -5.08 -20.32 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "ON Semiconductor"
			(at -5.08 -22.86 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Part_Number" "MAX809STRG"
			(at -5.08 -25.4 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Allied_Number" "70100462"
			(at -5.08 -27.94 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Arrow Part Number" "MAX809STRG"
			(at -5.08 -33.02 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/max809strg/on-semiconductor"
			(at -5.08 -35.56 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet Link" "http://www.onsemi.com/pub/Collateral/MAX809S-D.PDF"
			(at -5.08 -38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Geometry.Height" "1.11mm"
			(at -5.08 -40.64 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Comment" "MAX809STRG"
			(at -1.27 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(symbol "MAX809STRG_1_1"
			(rectangle
				(start 0 -10.16)
				(end 20.32 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin power_in line
				(at -5.08 -5.08 0)
				(length 5.08)
				(name "VCC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 10.16 -15.24 90)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "RESET"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "ME3110AM6G"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -0.127 -1.143 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "ME3110AM6G"
			(at 6.35 12.573 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://atta.szlcsc.com/upload/public/pdf/source/20200430/C526187_9477A8F3003D2FD22256EDDC2AADDD85.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "DCDC STEP DOWN; 3.6~40V; 1A; 550KHz;"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "POWER,dcdc"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "ME3110AM6G_0_1"
			(rectangle
				(start -5.08 5.08)
				(end 5.08 -10.16)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
		)
		(symbol "ME3110AM6G_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "EN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "BST"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "LX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "FB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "MK22FX512AVLL12"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "MK22FX512AVLL12"
			(at -3.81 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SQFP50P1600X1600-100M"
			(at -5.08 -223.52 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Part_Number" "MK22FX512AVLL12"
			(at -5.08 -226.06 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Note" "*"
			(at -5.08 -228.6 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -5.08 -231.14 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Package" "LQFP100"
			(at -5.08 -233.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -5.08 -238.76 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Comment" "MK22FX512AVLL12"
			(at -1.27 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(symbol "MK22FX512AVLL12_1_1"
			(rectangle
				(start 0 -218.44)
				(end 124.46 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 5.08)
				(name "PTA0/JTAG_TCLK/SWD_CLK/EZP_CLK/UART0_CTS_b/FTM0_CH5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 5.08)
				(name "PTA1/JTAG_TDI/EZP_DI/UART0_RX/FTM0_CH6/JTAG_TDI/EZP_DI"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 5.08)
				(name "PTA2/JTAG_TDO/TRACE_SWO/EZP_DO/UART0_TX/FTM0_CH7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 5.08)
				(name "PTA3/JTAG_TMS/SWD_DIO/UART0_RTS_b/FTM0_CH0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 5.08)
				(name "PTA4/LLWU_P3/NMI_b/EZP_CS_b/FTM0_CH1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 5.08)
				(name "PTA5/USB_CLKIN/FTM0_CH2/I2S0_TX_BCLK/JTAG_TRST_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 5.08)
				(name "PTA12/FTM1_CH0/I2S0_TXD0/FTM1_QD_PHA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 5.08)
				(name "PTA13/LLWU_P4/FTM1_CH1/I2S0_TX_FS/FTM1_QD_PHB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 5.08)
				(name "PTA14/SPI0_PCS0/UART0_TX/I2S0_RX_BCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 5.08)
				(name "PTA15/SPI0_SCK/UART0_RX/I2S0_RXD0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 5.08)
				(name "PTA16/SPI0_SOUT/UART0_CTS_b/I2S0_RX_FS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 5.08)
				(name "PTA17/ADC1_SE17/SPI0_SIN/UART0_RTS_b/I2S0_MCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 5.08)
				(name "PTA18/EXTAL0/FTM0_FLT2/FTM_CLKIN0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "50"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 5.08)
				(name "PTA19/XTAL0/FTM1_FLT0/FTM_CLKIN1/LPTMR0_ALT1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "51"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 5.08)
				(name "PTB0/LLWU_P5/ADC0_SE8/ADC1_SE8/I2C0_SCL/FTM1_CH0/FTM1_QD_PHA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "53"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 5.08)
				(name "PTB1/ADC0_SE9/ADC1_SE9/I2C0_SDA/FTM1_CH1/FTM1_QD_PHB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "54"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 5.08)
				(name "PTB2/ADC0_SE12/I2C0_SCL/UART0_RTS_b/FTM0_FLT3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "55"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 5.08)
				(name "PTB3/ADC0_SE13/I2C0_SDA/UART0_CTS_b/FTM0_FLT0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "56"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 5.08)
				(name "PTB9/SPI1_PCS1/LPUART0_CTS_b/FB_AD20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "57"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 5.08)
				(name "PTB10/ADC1_SE14/SPI1_PCS0/LPUART0_RX/FB_AD19/FTM0_FLT1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "58"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 5.08)
				(name "PTB11/ADC1_SE15/SPI1_SCK/LPUART0_TX/FB_AD18/FTM0_FLT2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "59"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 5.08)
				(name "PTB16/SPI1_SOUT/UART0_RX/FTM_CLKIN0/FB_AD17/EWM_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "62"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 5.08)
				(name "PTB17/SPI1_SIN/UART0_TX/FTM_CLKIN1/FB_AD16/EWM_OUT_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "63"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 5.08)
				(name "PTB18/CAN0_TX/FTM2_CH0/I2S0_TX_BCLK/FB_AD15/FTM2_QD_PHA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "64"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -71.12 0)
				(length 5.08)
				(name "PTB19/CAN0_RX/FTM2_CH1/I2S0_TX_FS/FB_OE_b/FTM2_QD_PHB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "65"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -73.66 0)
				(length 5.08)
				(name "PTB20/FB_AD31/CMP0_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "66"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -76.2 0)
				(length 5.08)
				(name "PTB21/FB_AD30/CMP1_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "67"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -78.74 0)
				(length 5.08)
				(name "PTB22/FB_AD29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "68"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -81.28 0)
				(length 5.08)
				(name "PTB23/SPI0_PCS5/FB_AD28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "69"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -88.9 0)
				(length 5.08)
				(name "PTC0/ADC0_SE14/SPI0_PCS4/PDB0_EXTRG/USB_SOF_OUT/FB_AD14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "70"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -91.44 0)
				(length 5.08)
				(name "PTC1/LLWU_P6/ADC0_SE15/SPI0_PCS3/UART1_RTS_b/FTM0_CH0/FB_AD13/I2S0_TXD0/LPUART0_RTS_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "71"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -93.98 0)
				(length 5.08)
				(name "PTC2/ADC0_SE4b/CMP1_IN0/SPI0_PCS2/UART1_CTS_b/FTM0_CH1/FB_AD12/I2S0_TX_FS/LPUART0_CTS_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "72"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -96.52 0)
				(length 5.08)
				(name "PTC3/LLWU_P7/CMP1_IN1/SPI0_PCS1/UART1_RX/FTM0_CH2/CLKOUT/I2S0_TX_BCLK/LPUART0_RX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "73"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -99.06 0)
				(length 5.08)
				(name "PTC4/LLWU_P8/SPI0_PCS0/UART1_TX/FTM0_CH3/FB_AD11/CMP1_OUT/LPUART0_TX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "76"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -101.6 0)
				(length 5.08)
				(name "PTC5/LLWU_P9/SPI0_SCK/LPTMR0_ALT2/I2S0_RXD0/FB_AD10/CMP0_OUT/FTM0_CH2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "77"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -104.14 0)
				(length 5.08)
				(name "PTC6/LLWU_P10/CMP0_IN0/SPI0_SOUT/PDB0_EXTRG/I2S0_RX_BCLK/FB_AD9/I2S0_MCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "78"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -106.68 0)
				(length 5.08)
				(name "PTC7/CMP0_IN1/SPI0_SIN/USB_SOF_OUT/I2S0_RX_FS/FB_AD8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "79"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -109.22 0)
				(length 5.08)
				(name "PTC8/ADC1_SE4b/CMP0_IN2/FTM3_CH4/I2S0_MCLK/FB_AD7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "80"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -111.76 0)
				(length 5.08)
				(name "PTC9/ADC1_SE5b/CMP0_IN3/FTM3_CH5/I2S0_RX_BCLK/FB_AD6/FTM2_FLT0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "81"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -114.3 0)
				(length 5.08)
				(name "PTC10/ADC1_SE6b/I2C1_SCL/FTM3_CH6/I2S0_RX_FS/FB_AD5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "82"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -116.84 0)
				(length 5.08)
				(name "PTC11/LLWU_P11/ADC1_SE7b/I2C1_SDA/FTM3_CH7/FB_RW_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "83"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -119.38 0)
				(length 5.08)
				(name "PTC12/FB_AD27/FTM3_FLT0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "84"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -121.92 0)
				(length 5.08)
				(name "PTC13/FB_AD26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "85"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -124.46 0)
				(length 5.08)
				(name "PTC14/FB_AD25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "86"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -127 0)
				(length 5.08)
				(name "PTC15/FB_AD24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "87"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -129.54 0)
				(length 5.08)
				(name "PTC16/LPUART0_RX/FB_CS5_b/FB_TSIZ1/FB_BE23_16_BLS15_8_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "90"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -132.08 0)
				(length 5.08)
				(name "PTC17/LPUART0_TX/FB_CS4_b/FB_TSIZ0/FB_BE31_24_BLS7_0_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "91"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -134.62 0)
				(length 5.08)
				(name "PTC18/LPUART0_RTS_b/FB_TBST_b/FB_CS2_b/FB_BE15_8_BLS23_16_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "92"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -142.24 0)
				(length 5.08)
				(name "PTD0/LLWU_P12/SPI0_PCS0/UART2_RTS_b/FTM3_CH0/FB_ALE/FB_CS1_b/FB_TS_b/LPUART0_RTS_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "93"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -144.78 0)
				(length 5.08)
				(name "PTD1/ADC0_SE5b/SPI0_SCK/UART2_CTS_b/FTM3_CH1/FB_CS0_bLPUART0_CTS_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "94"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -147.32 0)
				(length 5.08)
				(name "PTD2/LLWU_P13/SPI0_SOUT/UART2_RX/FTM3_CH2/FB_AD4/LPUART0_RX/I2C0_SCL"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "95"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -149.86 0)
				(length 5.08)
				(name "PTD3/SPI0_SIN/UART2_TX/FTM3_CH3/FB_AD3/LPUART0_TX/I2C0_SDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "96"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -152.4 0)
				(length 5.08)
				(name "PTD4/LLWU_P14/SPI0_PCS1/UART0_RTS_b/FTM0_CH4/FB_AD2/EWM_IN/SPI1_PCS0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "97"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -154.94 0)
				(length 5.08)
				(name "PTD5/ADC0_SE6b/SPI0_PCS2/UART0_CTS_b/FTM0_CH5/FB_AD1/EWM_OUT_b/SPI1_SCK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "98"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -157.48 0)
				(length 5.08)
				(name "PTD6/LLWU_P15/ADC0_SE7b/SPI0_PCS3/UART0_RX/FTM0_CH6/FB_AD0/FTM0_FLT0/SPI1_SOUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "99"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -160.02 0)
				(length 5.08)
				(name "PTD7/UART0_TX/FTM0_CH7/FTM0_FLT1/SPI1_SIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "100"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -167.64 0)
				(length 5.08)
				(name "PTE0/CLKOUT32K/ADC1_SE4a/SPI1_PCS1/UART1_TX/I2C1_SDA/RTC_CLKOUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -170.18 0)
				(length 5.08)
				(name "PTE1/LLWU_P0/ADC1_SE5a/SPI1_SOUT/UART1_RX/I2C1_SCL/SPI1_SIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -172.72 0)
				(length 5.08)
				(name "PTE2/LLWU_P1/ADC1_SE6a/SPI1_SCK/UART1_CTS_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -175.26 0)
				(length 5.08)
				(name "PTE3/ADC1_SE7a/SPI1_SIN/UART1_RTS_b/SPI1_SOUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -177.8 0)
				(length 5.08)
				(name "PTE4/LLWU_P2/SPI1_PCS0/LPUART0_TX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -180.34 0)
				(length 5.08)
				(name "PTE5/SPI1_PCS2/LPUART0_RX/FTM3_CH0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -182.88 0)
				(length 5.08)
				(name "PTE6/SPI1_PCS3/LPUART0_CTS_b/I2S0_MCLK/FTM3_CH1/USB_SOF_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -185.42 0)
				(length 5.08)
				(name "USB0_DP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -187.96 0)
				(length 5.08)
				(name "USB0_DM"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -190.5 0)
				(length 5.08)
				(name "VOUT33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -193.04 0)
				(length 5.08)
				(name "VREGIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -195.58 0)
				(length 5.08)
				(name "PTE24/ADC0_SE17/I2C0_SCL/EWM_OUT_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -198.12 0)
				(length 5.08)
				(name "PTE25/ADC0_SE18/I2C0_SDA/EWM_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -200.66 0)
				(length 5.08)
				(name "PTE26/CLKOUT32K/RTC_CLKOUT/USB_CLKIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -205.74 0)
				(length 5.08)
				(name "ADC0_DP1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -208.28 0)
				(length 5.08)
				(name "ADC0_DM1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -210.82 0)
				(length 5.08)
				(name "ADC1_DP1/ADC0_DP2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -213.36 0)
				(length 5.08)
				(name "ADC1_DM1/ADC0_DM2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -5.08 180)
				(length 5.08)
				(name "ADC0_DP0/ADC1_DP3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -10.16 180)
				(length 5.08)
				(name "ADC0_DM0/ADC1_DM3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -15.24 180)
				(length 5.08)
				(name "ADC1_DP0/ADC0_DP3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -20.32 180)
				(length 5.08)
				(name "ADC1_DM0/ADC0_DM3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -25.4 180)
				(length 5.08)
				(name "VREF_OUT/CMP1_IN5/CMP0_IN5/ADC1_SE18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -43.18 180)
				(length 5.08)
				(name "DAC0_OUT/CMP1_IN3/ADC0_SE23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -76.2 180)
				(length 5.08)
				(name "RESET_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "52"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -91.44 180)
				(length 5.08)
				(name "XTAL32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -106.68 180)
				(length 5.08)
				(name "EXTAL32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -124.46 180)
				(length 5.08)
				(name "VBAT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -142.24 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -144.78 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -147.32 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -149.86 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "61"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -152.4 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "75"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -154.94 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "89"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -167.64 180)
				(length 5.08)
				(name "VDDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -170.18 180)
				(length 5.08)
				(name "VREFH"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -177.8 180)
				(length 5.08)
				(name "VREFL"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -180.34 180)
				(length 5.08)
				(name "VSSA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -193.04 180)
				(length 5.08)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "88"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -195.58 180)
				(length 5.08)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "74"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -198.12 180)
				(length 5.08)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "60"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -200.66 180)
				(length 5.08)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "49"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -203.2 180)
				(length 5.08)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -205.74 180)
				(length 5.08)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "MK22LL_LQFP100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "MK22LL_LQFP100"
			(at -3.81 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SQFP50P1600X1600-100M"
			(at -5.08 -223.52 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -5.08 -228.6 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Package" "LQFP100"
			(at -5.08 -233.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Part_Number" "MK22FN512VLL12"
			(at -5.08 -236.22 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -5.08 -238.76 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Comment" "MK22FN512VLL12"
			(at -1.27 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(symbol "MK22LL_LQFP100_1_1"
			(rectangle
				(start 0 -218.44)
				(end 124.46 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 5.08)
				(name "PTA0/JTAG_TCLK/SWD_CLK/EZP_CLK/UART0_CTS_b/FTM0_CH5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 5.08)
				(name "PTA1/JTAG_TDI/EZP_DI/UART0_RX/FTM0_CH6/JTAG_TDI/EZP_DI"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 5.08)
				(name "PTA2/JTAG_TDO/TRACE_SWO/EZP_DO/UART0_TX/FTM0_CH7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 5.08)
				(name "PTA3/JTAG_TMS/SWD_DIO/UART0_RTS_b/FTM0_CH0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 5.08)
				(name "PTA4/LLWU_P3/NMI_b/EZP_CS_b/FTM0_CH1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 5.08)
				(name "PTA5/USB_CLKIN/FTM0_CH2/I2S0_TX_BCLK/JTAG_TRST_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 5.08)
				(name "PTA12/FTM1_CH0/I2S0_TXD0/FTM1_QD_PHA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 5.08)
				(name "PTA13/LLWU_P4/FTM1_CH1/I2S0_TX_FS/FTM1_QD_PHB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 5.08)
				(name "PTA14/SPI0_PCS0/UART0_TX/I2S0_RX_BCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 5.08)
				(name "PTA15/SPI0_SCK/UART0_RX/I2S0_RXD0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 5.08)
				(name "PTA16/SPI0_SOUT/UART0_CTS_b/I2S0_RX_FS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 5.08)
				(name "PTA17/ADC1_SE17/SPI0_SIN/UART0_RTS_b/I2S0_MCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 5.08)
				(name "PTA18/EXTAL0/FTM0_FLT2/FTM_CLKIN0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "50"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 5.08)
				(name "PTA19/XTAL0/FTM1_FLT0/FTM_CLKIN1/LPTMR0_ALT1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "51"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 5.08)
				(name "PTB0/LLWU_P5/ADC0_SE8/ADC1_SE8/I2C0_SCL/FTM1_CH0/FTM1_QD_PHA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "53"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 5.08)
				(name "PTB1/ADC0_SE9/ADC1_SE9/I2C0_SDA/FTM1_CH1/FTM1_QD_PHB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "54"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 5.08)
				(name "PTB2/ADC0_SE12/I2C0_SCL/UART0_RTS_b/FTM0_FLT3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "55"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 5.08)
				(name "PTB3/ADC0_SE13/I2C0_SDA/UART0_CTS_b/FTM0_FLT0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "56"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 5.08)
				(name "PTB9/SPI1_PCS1/LPUART0_CTS_b/FB_AD20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "57"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 5.08)
				(name "PTB10/ADC1_SE14/SPI1_PCS0/LPUART0_RX/FB_AD19/FTM0_FLT1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "58"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 5.08)
				(name "PTB11/ADC1_SE15/SPI1_SCK/LPUART0_TX/FB_AD18/FTM0_FLT2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "59"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 5.08)
				(name "PTB16/SPI1_SOUT/UART0_RX/FTM_CLKIN0/FB_AD17/EWM_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "62"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 5.08)
				(name "PTB17/SPI1_SIN/UART0_TX/FTM_CLKIN1/FB_AD16/EWM_OUT_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "63"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 5.08)
				(name "PTB18/FTM2_CH0/I2S0_TX_BCLK/FB_AD15/FTM2_QD_PHA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "64"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -71.12 0)
				(length 5.08)
				(name "PTB19/FTM2_CH1/I2S0_TX_FS/FB_OE_b/FTM2_QD_PHB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "65"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -73.66 0)
				(length 5.08)
				(name "PTB20/FB_AD31/CMP0_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "66"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -76.2 0)
				(length 5.08)
				(name "PTB21/FB_AD30/CMP1_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "67"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -78.74 0)
				(length 5.08)
				(name "PTB22/FB_AD29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "68"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -81.28 0)
				(length 5.08)
				(name "PTB23/SPI0_PCS5/FB_AD28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "69"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -88.9 0)
				(length 5.08)
				(name "PTC0/ADC0_SE14/SPI0_PCS4/PDB0_EXTRG/USB_SOF_OUT/FB_AD14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "70"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -91.44 0)
				(length 5.08)
				(name "PTC1/LLWU_P6/ADC0_SE15/SPI0_PCS3/UART1_RTS_b/FTM0_CH0/FB_AD13/I2S0_TXD0/LPUART0_RTS_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "71"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -93.98 0)
				(length 5.08)
				(name "PTC2/ADC0_SE4b/CMP1_IN0/SPI0_PCS2/UART1_CTS_b/FTM0_CH1/FB_AD12/I2S0_TX_FS/LPUART0_CTS_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "72"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -96.52 0)
				(length 5.08)
				(name "PTC3/LLWU_P7/CMP1_IN1/SPI0_PCS1/UART1_RX/FTM0_CH2/CLKOUT/I2S0_TX_BCLK/LPUART0_RX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "73"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -99.06 0)
				(length 5.08)
				(name "PTC4/LLWU_P8/SPI0_PCS0/UART1_TX/FTM0_CH3/FB_AD11/CMP1_OUT/LPUART0_TX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "76"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -101.6 0)
				(length 5.08)
				(name "PTC5/LLWU_P9/SPI0_SCK/LPTMR0_ALT2/I2S0_RXD0/FB_AD10/CMP0_OUT/FTM0_CH2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "77"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -104.14 0)
				(length 5.08)
				(name "PTC6/LLWU_P10/CMP0_IN0/SPI0_SOUT/PDB0_EXTRG/I2S0_RX_BCLK/FB_AD9/I2S0_MCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "78"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -106.68 0)
				(length 5.08)
				(name "PTC7/CMP0_IN1/SPI0_SIN/USB_SOF_OUT/I2S0_RX_FS/FB_AD8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "79"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -109.22 0)
				(length 5.08)
				(name "PTC8/ADC1_SE4b/CMP0_IN2/FTM3_CH4/I2S0_MCLK/FB_AD7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "80"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -111.76 0)
				(length 5.08)
				(name "PTC9/ADC1_SE5b/CMP0_IN3/FTM3_CH5/I2S0_RX_BCLK/FB_AD6/FTM2_FLT0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "81"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -114.3 0)
				(length 5.08)
				(name "PTC10/ADC1_SE6b/I2C1_SCL/FTM3_CH6/I2S0_RX_FS/FB_AD5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "82"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -116.84 0)
				(length 5.08)
				(name "PTC11/LLWU_P11/ADC1_SE7b/I2C1_SDA/FTM3_CH7/FB_RW_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "83"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -119.38 0)
				(length 5.08)
				(name "PTC12/FB_AD27/FTM3_FLT0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "84"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -121.92 0)
				(length 5.08)
				(name "PTC13/FB_AD26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "85"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -124.46 0)
				(length 5.08)
				(name "PTC14/FB_AD25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "86"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -127 0)
				(length 5.08)
				(name "PTC15/FB_AD24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "87"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -129.54 0)
				(length 5.08)
				(name "PTC16/LPUART0_RX/FB_CS5_b/FB_TSIZ1/FB_BE23_16_BLS15_8_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "90"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -132.08 0)
				(length 5.08)
				(name "PTC17/LPUART0_TX/FB_CS4_b/FB_TSIZ0/FB_BE31_24_BLS7_0_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "91"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -134.62 0)
				(length 5.08)
				(name "PTC18/LPUART0_RTS_b/FB_TBST_b/FB_CS2_b/FB_BE15_8_BLS23_16_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "92"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -142.24 0)
				(length 5.08)
				(name "PTD0/LLWU_P12/SPI0_PCS0/UART2_RTS_b/FTM3_CH0/FB_ALE/FB_CS1_b/FB_TS_b/LPUART0_RTS_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "93"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -144.78 0)
				(length 5.08)
				(name "PTD1/ADC0_SE5b/SPI0_SCK/UART2_CTS_b/FTM3_CH1/FB_CS0_bLPUART0_CTS_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "94"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -147.32 0)
				(length 5.08)
				(name "PTD2/LLWU_P13/SPI0_SOUT/UART2_RX/FTM3_CH2/FB_AD4/LPUART0_RX/I2C0_SCL"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "95"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -149.86 0)
				(length 5.08)
				(name "PTD3/SPI0_SIN/UART2_TX/FTM3_CH3/FB_AD3/LPUART0_TX/I2C0_SDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "96"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -152.4 0)
				(length 5.08)
				(name "PTD4/LLWU_P14/SPI0_PCS1/UART0_RTS_b/FTM0_CH4/FB_AD2/EWM_IN/SPI1_PCS0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "97"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -154.94 0)
				(length 5.08)
				(name "PTD5/ADC0_SE6b/SPI0_PCS2/UART0_CTS_b/FTM0_CH5/FB_AD1/EWM_OUT_b/SPI1_SCK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "98"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -157.48 0)
				(length 5.08)
				(name "PTD6/LLWU_P15/ADC0_SE7b/SPI0_PCS3/UART0_RX/FTM0_CH6/FB_AD0/FTM0_FLT0/SPI1_SOUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "99"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -160.02 0)
				(length 5.08)
				(name "PTD7/UART0_TX/FTM0_CH7/FTM0_FLT1/SPI1_SIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "100"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -167.64 0)
				(length 5.08)
				(name "PTE0/CLKOUT32K/ADC1_SE4a/SPI1_PCS1/UART1_TX/I2C1_SDA/RTC_CLKOUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -170.18 0)
				(length 5.08)
				(name "PTE1/LLWU_P0/ADC1_SE5a/SPI1_SOUT/UART1_RX/I2C1_SCL/SPI1_SIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -172.72 0)
				(length 5.08)
				(name "PTE2/LLWU_P1/ADC1_SE6a/SPI1_SCK/UART1_CTS_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -175.26 0)
				(length 5.08)
				(name "PTE3/ADC1_SE7a/SPI1_SIN/UART1_RTS_b/SPI1_SOUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -177.8 0)
				(length 5.08)
				(name "PTE4/LLWU_P2/SPI1_PCS0/LPUART0_TX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -180.34 0)
				(length 5.08)
				(name "PTE5/SPI1_PCS2/LPUART0_RX/FTM3_CH0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -182.88 0)
				(length 5.08)
				(name "PTE6/SPI1_PCS3/LPUART0_CTS_b/I2S0_MCLK/FTM3_CH1/USB_SOF_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -185.42 0)
				(length 5.08)
				(name "USB0_DP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -187.96 0)
				(length 5.08)
				(name "USB0_DM"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -190.5 0)
				(length 5.08)
				(name "VOUT33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -193.04 0)
				(length 5.08)
				(name "VREGIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -195.58 0)
				(length 5.08)
				(name "PTE24/ADC0_SE17/I2C0_SCL/EWM_OUT_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -198.12 0)
				(length 5.08)
				(name "PTE25/ADC0_SE18/I2C0_SDA/EWM_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -200.66 0)
				(length 5.08)
				(name "PTE26/CLKOUT32K/RTC_CLKOUT/USB_CLKIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -205.74 0)
				(length 5.08)
				(name "ADC0_DP1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -208.28 0)
				(length 5.08)
				(name "ADC0_DM1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -210.82 0)
				(length 5.08)
				(name "ADC1_DP1/ADC0_DP2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -213.36 0)
				(length 5.08)
				(name "ADC1_DM1/ADC0_DM2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -5.08 180)
				(length 5.08)
				(name "ADC0_DP0/ADC1_DP3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -10.16 180)
				(length 5.08)
				(name "ADC0_DM0/ADC1_DM3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -15.24 180)
				(length 5.08)
				(name "ADC1_DP0/ADC0_DP3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -20.32 180)
				(length 5.08)
				(name "ADC1_DM0/ADC0_DM3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -25.4 180)
				(length 5.08)
				(name "VREF_OUT/CMP1_IN5/CMP0_IN5/ADC1_SE18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -43.18 180)
				(length 5.08)
				(name "DAC0_OUT/CMP1_IN3/ADC0_SE23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -76.2 180)
				(length 5.08)
				(name "RESET_b"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "52"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -91.44 180)
				(length 5.08)
				(name "XTAL32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -106.68 180)
				(length 5.08)
				(name "EXTAL32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -124.46 180)
				(length 5.08)
				(name "VBAT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -142.24 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -144.78 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -147.32 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -149.86 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "61"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -152.4 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "75"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -154.94 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "89"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -167.64 180)
				(length 5.08)
				(name "VDDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -170.18 180)
				(length 5.08)
				(name "VREFH"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -177.8 180)
				(length 5.08)
				(name "VREFL"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -180.34 180)
				(length 5.08)
				(name "VSSA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -193.04 180)
				(length 5.08)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "88"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -195.58 180)
				(length 5.08)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "74"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -198.12 180)
				(length 5.08)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "60"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -200.66 180)
				(length 5.08)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "49"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -203.2 180)
				(length 5.08)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 129.54 -205.74 180)
				(length 5.08)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "MP2161AGJ"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "MP2161AGJ"
			(at -1.27 11.43 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-8"
			(at 3.81 -8.89 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.monolithicpower.cn/cn/documentview/productdocument/index/version/2/document_type/Datasheet/lang/EN/sku/MP2161A/document_id/935/"
			(at 0 13.97 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "2A, 6V, 1.5MHz, 17μA IQ, COT Synchronous Step-Down Converter in 8-pin TSOT23"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "step-down dc-dc buck regulator"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "*TSOT*23*8*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "MP2161AGJ_0_1"
			(rectangle
				(start -7.62 10.16)
				(end 7.62 -7.62)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(symbol "MP2161AGJ_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "EN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PG"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "PGND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "AGND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SW"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "MT3608"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 -7.62 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "MT3608"
			(at 0 7.62 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 2.54 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://atta.szlcsc.com/upload/public/pdf/source/20161110/1478743351706.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "High Efficiency 1.2MHz,2A Step Up Converter"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "POWER,dcdc"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "MT3608_0_1"
			(rectangle
				(start -5.08 5.08)
				(end 5.08 -5.08)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(symbol "MT3608_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SW"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(name "NC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "FB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "NV080C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "NV080C-SOP8"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_SO:SOP-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.n-ec.cn/static/upload/file/20221103/1667456113693687.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "语音芯片"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "NV080C_0_0"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0/BUSY"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "PA0/CLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PA1/SDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 15.24 3.81 180)
				(length 2.54)
				(name "VPP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "PWM1/DAC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PWM2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "NV080C_1_1"
			(rectangle
				(start -12.7 5.08)
				(end 12.7 -5.08)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "PC357"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "PC357"
			(at -1.27 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SOP2.54-4"
			(at -2.54 -14.224 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "4-Pin Phototransistor Optocoupler"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Part_Number" "PC357N"
			(at -2.54 -19.304 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Package" "SOP-4-OP"
			(at -2.54 -21.844 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -2.54 -26.924 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -2.54 -29.464 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Comment" "PC357"
			(at 1.27 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(symbol "PC357_1_1"
			(polyline
				(pts
					(xy 2.54 -1.016) (xy 2.54 -9.144)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -1.016) (xy 17.78 -1.016)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -2.54) (xy 5.842 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -7.62) (xy 5.842 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -9.144) (xy 17.78 -9.144)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 -3.81) (xy 7.874 -3.81) (xy 5.842 -5.842) (xy 3.81 -3.81)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 5.842 -2.54) (xy 5.842 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.874 -6.096) (xy 7.874 -6.35) (xy 3.81 -6.35) (xy 3.81 -6.096) (xy 7.874 -6.096)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 11.176 -3.302) (xy 9.652 -4.826)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 11.176 -3.81) (xy 11.176 -3.302) (xy 10.668 -3.302) (xy 11.176 -3.81)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 11.176 -4.572) (xy 9.652 -6.096)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 11.176 -5.08) (xy 11.176 -4.572) (xy 10.668 -4.572) (xy 11.176 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 13.462 -3.302) (xy 13.208 -3.302) (xy 13.208 -6.858) (xy 13.462 -6.858) (xy 13.462 -3.302)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 13.462 -5.842) (xy 15.24 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 14.986 -2.54) (xy 13.462 -4.064)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 14.986 -2.54) (xy 17.78 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 14.986 -6.604) (xy 14.986 -7.366) (xy 14.224 -7.366) (xy 14.986 -6.604)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 15.24 -7.62) (xy 17.78 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 17.78 -1.016) (xy 17.78 -9.144)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -2.54 -2.54 0)
				(length 5.08)
				(name "A"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.54 -7.62 0)
				(length 5.08)
				(name "K"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "C"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "E"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "PC410L"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "PC410L"
			(at -1.27 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SOP2.54-5"
			(at -2.54 -17.78 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "DUAL-CHANNEL HIGH SPEED-10 MBit/s LOGIC GATE OPTOCOUPLERS"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Note" "*"
			(at -2.54 -20.32 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Part_Number" "PC410L0NIP0F"
			(at -2.54 -22.86 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Package" "SOP-5"
			(at -2.54 -25.4 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -2.54 -30.48 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -2.54 -33.02 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Comment" "PC410L"
			(at 1.27 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(symbol "PC410L_1_1"
			(polyline
				(pts
					(xy 2.54 0) (xy 2.54 -12.7)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0) (xy 17.78 0)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -2.54) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -10.16) (xy 5.08 -10.16)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -12.7) (xy 17.78 -12.7)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.556 -5.08) (xy 6.604 -5.08) (xy 5.08 -7.112) (xy 3.556 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy 5.08 -10.16)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 6.604 -7.366) (xy 6.604 -7.62) (xy 3.556 -7.62) (xy 3.556 -7.366) (xy 6.604 -7.366)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 9.398 -6.35) (xy 9.398 -6.858) (xy 8.89 -6.858) (xy 9.398 -6.35)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 9.398 -6.858) (xy 7.874 -5.334)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 9.398 -7.62) (xy 9.398 -8.128) (xy 8.89 -8.128) (xy 9.398 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 9.398 -8.128) (xy 7.874 -6.604)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 15.748 -5.842) (xy 15.494 -5.842) (xy 15.494 -9.398) (xy 15.748 -9.398) (xy 15.748 -5.842)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 15.748 -8.382) (xy 17.526 -10.16)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 17.272 -5.08) (xy 15.748 -6.604)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 17.272 -9.144) (xy 17.272 -9.906) (xy 16.51 -9.906) (xy 17.272 -9.144)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 17.78 0) (xy 17.78 -12.7)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 17.78 -5.08) (xy 17.272 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -2.54 -2.54 0)
				(length 5.08)
				(name "A"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.54 -10.16 0)
				(length 5.08)
				(name "K"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "VCC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin open_collector line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "VO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "PC457"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "PC457"
			(at -1.27 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SOP2.54-5"
			(at -2.54 -16.51 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "5-Pin Phototransistor Optocoupler,High Speed 1Mb/s, High CMR"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Part_Number" "PC457L0NIP0F"
			(at -2.54 -21.59 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Package" "SOP-5-OP"
			(at -2.54 -24.13 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -2.54 -29.21 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -2.54 -31.75 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Comment" "PC457"
			(at 1.27 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(symbol "PC457_1_1"
			(polyline
				(pts
					(xy 2.54 -1.016) (xy 2.54 -11.43)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -1.016) (xy 17.78 -1.016)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -2.54) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -10.16) (xy 5.08 -10.16)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -11.43) (xy 17.78 -11.43)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.556 -5.08) (xy 6.604 -5.08) (xy 5.08 -7.112) (xy 3.556 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy 5.08 -10.16)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 6.604 -7.366) (xy 6.604 -7.62) (xy 3.556 -7.62) (xy 3.556 -7.366) (xy 6.604 -7.366)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 9.144 -3.81) (xy 7.62 -5.334)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 9.144 -4.318) (xy 9.144 -3.81) (xy 8.636 -3.81) (xy 9.144 -4.318)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 9.144 -5.08) (xy 7.62 -6.604)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 9.144 -5.588) (xy 9.144 -5.08) (xy 8.636 -5.08) (xy 9.144 -5.588)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 10.922 -4.318) (xy 10.922 -4.064) (xy 13.97 -4.064) (xy 13.97 -4.318) (xy 10.922 -4.318)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 12.446 -2.54) (xy 17.78 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 12.446 -7.62) (xy 12.446 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 12.446 -7.62) (xy 14.986 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 13.97 -6.604) (xy 10.922 -6.604) (xy 12.446 -4.572) (xy 13.97 -6.604)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 15.24 -5.842) (xy 14.986 -5.842) (xy 14.986 -9.398) (xy 15.24 -9.398) (xy 15.24 -5.842)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 15.24 -8.382) (xy 17.018 -10.16)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 16.764 -5.08) (xy 15.24 -6.604)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 16.764 -5.08) (xy 17.78 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 16.764 -9.144) (xy 16.764 -9.906) (xy 16.002 -9.906) (xy 16.764 -9.144)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 17.018 -10.16) (xy 17.78 -10.16)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 17.78 -1.016) (xy 17.78 -11.43)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -2.54 -2.54 0)
				(length 5.08)
				(name "A"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.54 -10.16 0)
				(length 5.08)
				(name "K"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "VCC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "Vo"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "PC817"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "PC817"
			(at -1.27 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "DIP-4"
			(at -2.54 -14.224 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Part_Number" "PC817"
			(at -2.54 -16.764 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Note" "*"
			(at -2.54 -19.304 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Package" "DIP-4"
			(at -2.54 -21.844 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -2.54 -26.924 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -2.54 -29.464 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Comment" "PC817"
			(at 1.27 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(symbol "PC817_1_1"
			(polyline
				(pts
					(xy 2.54 -1.016) (xy 2.54 -9.144)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -1.016) (xy 17.78 -1.016)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -2.54) (xy 5.842 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -7.62) (xy 5.842 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -9.144) (xy 17.78 -9.144)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 -3.81) (xy 7.874 -3.81) (xy 5.842 -5.842) (xy 3.81 -3.81)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 5.842 -2.54) (xy 5.842 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.874 -6.096) (xy 7.874 -6.35) (xy 3.81 -6.35) (xy 3.81 -6.096) (xy 7.874 -6.096)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 11.176 -3.302) (xy 9.652 -4.826)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 11.176 -3.81) (xy 11.176 -3.302) (xy 10.668 -3.302) (xy 11.176 -3.81)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 11.176 -4.572) (xy 9.652 -6.096)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 11.176 -5.08) (xy 11.176 -4.572) (xy 10.668 -4.572) (xy 11.176 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 13.462 -3.302) (xy 13.208 -3.302) (xy 13.208 -6.858) (xy 13.462 -6.858) (xy 13.462 -3.302)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 13.462 -5.842) (xy 15.24 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 14.986 -2.54) (xy 13.462 -4.064)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 14.986 -2.54) (xy 17.78 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 14.986 -6.604) (xy 14.986 -7.366) (xy 14.224 -7.366) (xy 14.986 -6.604)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 15.24 -7.62) (xy 17.78 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 17.78 -1.016) (xy 17.78 -9.144)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -2.54 -2.54 0)
				(length 5.08)
				(name "A"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.54 -7.62 0)
				(length 5.08)
				(name "K"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "C"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "E"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "REF3020AIDBZT"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 1.27 0)
			(effects
				(font
					(size 1.397 1.397)
				)
				(justify left bottom)
			)
		)
		(property "Value" "REF3020AIDBZT"
			(at -3.81 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SOT23-3N"
			(at -5.08 -17.78 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "2.048V Voltage Reference, 3-Pin SOT-23, Industrial Temperature, Tape and Reel"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -5.08 -22.86 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -5.08 -25.4 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Manufacturer" "TI"
			(at -5.08 -27.94 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "user" "VSS"
			(at 5.08 -7.112 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Package" "SOT-23"
			(at -5.08 -33.02 0)
			(effects
				(font
					(size 1.397 1.397)
				)
				(justify left bottom)
			)
		)
		(property "Part_Number" "REF3020AIDBZT"
			(at -5.08 -35.56 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Comment" "REF3020"
			(at -1.27 1.27 0)
			(effects
				(font
					(size 1.397 1.397)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Created" "8/05/2006"
			(at -5.08 -38.1 0)
			(effects
				(font
					(size 1.397 1.397)
				)
				(justify left bottom)
			)
		)
		(symbol "REF3020AIDBZT_1_1"
			(rectangle
				(start 0 -7.62)
				(end 15.24 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin power_in line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 7.62 -12.7 90)
				(length 5.08)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "REF3312AIDBZT"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 1.27 0)
			(effects
				(font
					(size 1.397 1.397)
				)
				(justify left bottom)
			)
		)
		(property "Value" "REF3312AIDBZT"
			(at -3.81 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SOT23-3N"
			(at -5.08 -17.78 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "1.25V Voltage Reference, 3-Pin SOT-23, Industrial Temperature, Tape and Reel"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -5.08 -22.86 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -5.08 -25.4 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Manufacturer" "TI"
			(at -5.08 -27.94 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "user" "VSS"
			(at 5.08 -7.112 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Package" "SOT-23"
			(at -5.08 -33.02 0)
			(effects
				(font
					(size 1.397 1.397)
				)
				(justify left bottom)
			)
		)
		(property "Part_Number" "REF3312AIDBZT"
			(at -5.08 -35.56 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Comment" "REF3012"
			(at -1.27 1.27 0)
			(effects
				(font
					(size 1.397 1.397)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Created" "8/05/2006"
			(at -5.08 -38.1 0)
			(effects
				(font
					(size 1.397 1.397)
				)
				(justify left bottom)
			)
		)
		(symbol "REF3312AIDBZT_1_1"
			(rectangle
				(start 0 -7.62)
				(end 15.24 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin power_in line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 7.62 -12.7 90)
				(length 5.08)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F030R8T6"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "STM32F030R8T6"
			(at -6.35 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SQFP50P1200X1200-64M"
			(at -7.62 -114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "STM32 ARM-based 32-bit MCU with 64 Kbytes Flash, 64-pin LQFP, Industrial Temperature"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -7.62 -116.84 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Package" "LQFP64"
			(at -7.62 -121.92 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Part_Number" "STM32F030R8T6"
			(at -7.62 -127 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -7.62 -129.54 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Comment" "STM32F030R8T6"
			(at -3.81 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(symbol "STM32F030R8T6_1_1"
			(rectangle
				(start 0 -109.22)
				(end 45.72 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin bidirectional line
				(at -7.62 -2.54 0)
				(length 7.62)
				(name "PA0-WKUP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -5.08 0)
				(length 7.62)
				(name "PA1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -7.62 0)
				(length 7.62)
				(name "PA2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -10.16 0)
				(length 7.62)
				(name "PA3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -12.7 0)
				(length 7.62)
				(name "PA4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -15.24 0)
				(length 7.62)
				(name "PA5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -17.78 0)
				(length 7.62)
				(name "PA6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -20.32 0)
				(length 7.62)
				(name "PA7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -25.4 0)
				(length 7.62)
				(name "PA8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -27.94 0)
				(length 7.62)
				(name "PA9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -30.48 0)
				(length 7.62)
				(name "PA10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -33.02 0)
				(length 7.62)
				(name "PA11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -35.56 0)
				(length 7.62)
				(name "PA12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -38.1 0)
				(length 7.62)
				(name "PA13/JTMS/SWDIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -40.64 0)
				(length 7.62)
				(name "PA14/JTCK/SWCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "49"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -43.18 0)
				(length 7.62)
				(name "PA15/JTDI"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "50"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -7.62 -48.26 0)
				(length 7.62)
				(name "OSC_IN/PD0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at -7.62 -50.8 0)
				(length 7.62)
				(name "OSC_OUT/PD1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -53.34 0)
				(length 7.62)
				(name "PD2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "54"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -58.42 0)
				(length 7.62)
				(name "PF4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -60.96 0)
				(length 7.62)
				(name "PF5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -63.5 0)
				(length 7.62)
				(name "PF6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -66.04 0)
				(length 7.62)
				(name "PF7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -7.62 -73.66 0)
				(length 7.62)
				(name "BOOT0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "60"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -78.74 0)
				(length 7.62)
				(name "NRST"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 -88.9 0)
				(length 7.62)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 -93.98 0)
				(length 7.62)
				(name "VDD_1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 -99.06 0)
				(length 7.62)
				(name "VDD_3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "64"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 -106.68 0)
				(length 7.62)
				(name "VDDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -2.54 180)
				(length 7.62)
				(name "PB0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -5.08 180)
				(length 7.62)
				(name "PB1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -7.62 180)
				(length 7.62)
				(name "PB2/BOOT1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -10.16 180)
				(length 7.62)
				(name "PB3/JTDO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "55"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -12.7 180)
				(length 7.62)
				(name "PB4/JNTRST"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "56"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -15.24 180)
				(length 7.62)
				(name "PB5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "57"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -17.78 180)
				(length 7.62)
				(name "PB6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "58"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -20.32 180)
				(length 7.62)
				(name "PB7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "59"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -25.4 180)
				(length 7.62)
				(name "PB8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "61"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -27.94 180)
				(length 7.62)
				(name "PB9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "62"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -30.48 180)
				(length 7.62)
				(name "PB10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -33.02 180)
				(length 7.62)
				(name "PB11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -35.56 180)
				(length 7.62)
				(name "PB12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -38.1 180)
				(length 7.62)
				(name "PB13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -40.64 180)
				(length 7.62)
				(name "PB14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -43.18 180)
				(length 7.62)
				(name "PB15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -48.26 180)
				(length 7.62)
				(name "PC0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -50.8 180)
				(length 7.62)
				(name "PC1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -53.34 180)
				(length 7.62)
				(name "PC2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -55.88 180)
				(length 7.62)
				(name "PC3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -58.42 180)
				(length 7.62)
				(name "PC4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -60.96 180)
				(length 7.62)
				(name "PC5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -63.5 180)
				(length 7.62)
				(name "PC6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -66.04 180)
				(length 7.62)
				(name "PC7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -71.12 180)
				(length 7.62)
				(name "PC8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -73.66 180)
				(length 7.62)
				(name "PC9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -76.2 180)
				(length 7.62)
				(name "PC10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "51"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -78.74 180)
				(length 7.62)
				(name "PC11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "52"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -81.28 180)
				(length 7.62)
				(name "PC12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "53"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -83.82 180)
				(length 7.62)
				(name "PC13-TAMPER-RTC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -86.36 180)
				(length 7.62)
				(name "PC14-OSC32_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -88.9 180)
				(length 7.62)
				(name "PC15-OSC32_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 53.34 -93.98 180)
				(length 7.62)
				(name "VSS_1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 53.34 -99.06 180)
				(length 7.62)
				(name "VSS_3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "63"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 53.34 -106.68 180)
				(length 7.62)
				(name "VSSA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F091RCT6"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -48.26 46.99 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Value" "STM32F091RCT6"
			(at -31.75 50.8 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f091rc.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "LQFP64"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "STM32F091RCT6_0_1"
			(pin power_in line
				(at -2.54 52.07 270)
				(length 3.81)
				(name "VDD_1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 3.81)
				(name "VSS_4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 0 52.07 270)
				(length 3.81)
				(name "VDDIO2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 3.81)
				(name "VSS_3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "63"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 52.07 270)
				(length 3.81)
				(name "VDD_3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "64"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 3.81)
				(name "VSS_2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 5.08 52.07 270)
				(length 3.81)
				(name "VDD_4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 5.08 -50.8 90)
				(length 3.81)
				(name "VSS_1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 81.28 -27.94 180)
				(length 3.81)
				(name "VBAT"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 81.28 -35.56 180)
				(length 3.81)
				(name "VDDA"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 81.28 -40.64 180)
				(length 3.81)
				(name "VSSA"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
		)
		(symbol "STM32F091RCT6_1_1"
			(rectangle
				(start 77.47 -46.99)
				(end -49.53 48.26)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin bidirectional line
				(at -53.34 40.64 0)
				(length 3.81)
				(name "PA0/USART2_CTS/TIM2_CH1_ETR/TSC_G1_IO1/USART4_TX_COMP1_OUT/RTC__TAMP2/WKUP1/ADC_IN0/COMP1_INM6"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 38.1 0)
				(length 3.81)
				(name "PA1/USART2_RTS/TIM2_CH2/TIM15_CH1N/TSC_G1_IO2/USART4_RX/ADC_IN1/COMP1_INP"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 35.56 0)
				(length 3.81)
				(name "PA2/USART2_TX/TIM2_CH3/TIM15_CH1/TSC_G1_IO3/COMP2_OUT/ADC_IN2/WKUP4/COMP2_INM6"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 33.02 0)
				(length 3.81)
				(name "PA3/USART2_RX/TIM2_CH4/TIM15_CH2/TSC_G1_IO4/ADC_IN3/COMP2_INP"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 30.48 0)
				(length 3.81)
				(name "PA4/SPI1_NSS/I2S1_WS/TIM14_CH1/TSC_G2_IO1/USART2_CK/USART6_TX/COMP1_INM4/COMP2_INM4/ADC_IN4/DAC_OUT1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 27.94 0)
				(length 3.81)
				(name "PA5/SPI1_SCK/I2S1_CK/CEC/TIM2_CH1_ETR/TSC_G2_IO2/USART6_RX/COMP1_INM5/COMP2_INM5/ADC_IN5/DAC_OUT2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 25.4 0)
				(length 3.81)
				(name "PA6/SPI1_MISO/I2S1_MCK/TIM3_CH1/TIM1_BKIN/TIM16_CH1/COMP1_OUT/TSC_G2_IO3/USART3_CTS/ADC_IN6"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 22.86 0)
				(length 3.81)
				(name "PA7/SPI1_MOSI/I2S1_SD/TIM3_CH2/TIM14_CH1/TIM1_CH1N/TIM17_CH1/COMP2_OUT/TSC_G2_IO4/ADC_IN7"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 20.32 0)
				(length 3.81)
				(name "PA8/USART1_CK/TIM1_CH1/MCO/CRS_SYNC"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 17.78 0)
				(length 3.81)
				(name "PA9/USART1_TX/TIM1_CH2/TIM15_BKIN/MCO/TSC_G4_IO1/I2C1_SCL"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 15.24 0)
				(length 3.81)
				(name "PA10/USART1_RX/TIM1_CH3/TIM17_BKIN/TSC_G4_IO2/I2C1_SDA"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 12.7 0)
				(length 3.81)
				(name "PA11/CAN_RX/USART1_CTS/TIM1_CH4/COMP1_OUT/TSC_G4_IO3/I2C2_SCL"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 10.16 0)
				(length 3.81)
				(name "PA12/CAN_TX/USART1_RTS/TIM1_ETR/COMP2_OUT/TSC_G4_IO4/I2C2_SDA"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 7.62 0)
				(length 3.81)
				(name "PA13/IR_OUT/SWDIO"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 5.08 0)
				(length 3.81)
				(name "PA14/USART2_TX/SWCLK"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "49"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 2.54 0)
				(length 3.81)
				(name "PA15/SPI1_NSS/I2S1_WS/USART2_RX/USART4_RTS/TIM2_CH1_ETR"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "50"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -2.54 0)
				(length 3.81)
				(name "PB0/TIM3_CH3/TIM1_CH2N/TSC_G3_IO2/USART3_CK/ADC_IN8"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -5.08 0)
				(length 3.81)
				(name "PB1/TIM3_CH4/USART3_RTS/TIM14_CH1/TIM1_CH3N/TSC_G3_IO3/ADC_IN9"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -7.62 0)
				(length 3.81)
				(name "PB2/TSC_G3_IO4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -10.16 0)
				(length 3.81)
				(name "PB3/SPI1_SCK/I2S1_CK/TIM2_CH2/TSC_G5_IO1/USART5_TX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "55"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -12.7 0)
				(length 3.81)
				(name "PB4/SPI1_MISO/I2S1_MCK/TIM17_BKIN/TIM3_CH1/TSC_G5_IO2/USART5_RX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "56"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -15.24 0)
				(length 3.81)
				(name "PB5/SPI1_MOSI/I2S1_SD/I2C1_SMBA/TIM16_BKIN/TIM3_CH2/USART5_CK_RTS/WKUP6"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "57"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -17.78 0)
				(length 3.81)
				(name "PB6/I2C1_SCL/USART1_TX/TIM16_CH1N/TSC_G5_I03"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "58"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -20.32 0)
				(length 3.81)
				(name "PB7/I2C1_SDA/USART1_RX/USART4_CTS/TIM17_CH1N/TSC_G5_IO4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "59"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -22.86 0)
				(length 3.81)
				(name "PB8/I2C1_SCL/CEC/TIM16_CH1/TSC_SYNC/CAN_RX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "61"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -25.4 0)
				(length 3.81)
				(name "PB9/SPI2_NSS/I2S2_WS/I2C1_SDA/IR_OUT/TIM17_CH1/CAN_TX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "62"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -27.94 0)
				(length 3.81)
				(name "PB10/SPI2_SCK/I2S2_CK/I2C2_SCL/USART3_TX/CEC/TSC_SYNC/TIM2_CH3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -30.48 0)
				(length 3.81)
				(name "PB11/USART3_RX/TIM2_CH4/TSC_G6_IO1/I2C2_SDA"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -33.02 0)
				(length 3.81)
				(name "PB12/TIM1_BKIN/TIM15_BKIN/SPI2_NSS/I2S2_WS/USART3_CK/TSC_G6_IO2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -35.56 0)
				(length 3.81)
				(name "PB13/SPI2_SCK/I2S2_CK/I2C2_SCL/USART3_CTS/TIM1_CH1N/TSC_G6_IO3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -38.1 0)
				(length 3.81)
				(name "PB14/SPI2_MISO/I2S2_MCK/I2C2_SDA/USART3_RTS/TIM1_CH2N/TIM15_CH1/TSC_G6_IO4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -40.64 0)
				(length 3.81)
				(name "PB15/SPI2_MOSI/I2S2_SD/TIM1_CH3N/TIM15_CH1N/TIM15_CH2/WKUP7/RTC_REFIN"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 81.28 40.64 180)
				(length 3.81)
				(name "PC0/USART6_TX/USART7_TX/ADC_IN10"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 81.28 38.1 180)
				(length 3.81)
				(name "PC1/USART6_RX/USART7_RX/ADC_IN11"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 81.28 35.56 180)
				(length 3.81)
				(name "PC2/SPI2_MISO/I2S2_MCK/USART8_TX/ADC_IN12"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 81.28 33.02 180)
				(length 3.81)
				(name "PC3/SPI2_MOSI/I2S2_SD/USART8_RX/ADC_IN13"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 81.28 30.48 180)
				(length 3.81)
				(name "PC4/USART3_TX/ADC_IN14"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 81.28 27.94 180)
				(length 3.81)
				(name "PC5/TSC_G3_IO1/USART3_RX/ADC_IN15/WKUP5"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 81.28 25.4 180)
				(length 3.81)
				(name "PC6/TIM3_CH1/USART7_TX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 81.28 22.86 180)
				(length 3.81)
				(name "PC7/TIM3_CH2/USART7_RX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 81.28 20.32 180)
				(length 3.81)
				(name "PC8/TIM3_CH3/USART8_TX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 81.28 17.78 180)
				(length 3.81)
				(name "PC9/TIM3_CH4/USART8_RX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 81.28 15.24 180)
				(length 3.81)
				(name "PC10/USART3_TX/USART4_TX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "51"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 81.28 12.7 180)
				(length 3.81)
				(name "PC11/USART3_RX/USART4_RX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "52"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 81.28 10.16 180)
				(length 3.81)
				(name "PC12/USART3_CK/USART4_CK/USART5_TX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "53"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 81.28 7.62 180)
				(length 3.81)
				(name "PC13/WKUP2/RTC_TAMP1/RTC_TS/RTC_OUT"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 81.28 5.08 180)
				(length 3.81)
				(name "PC14/OSC32_IN"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 81.28 2.54 180)
				(length 3.81)
				(name "PC15/OSC32_OUT"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 81.28 -2.54 180)
				(length 3.81)
				(name "PD2/USART3_RTS/TIM3_ETR/USART5_RX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "54"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin input line
				(at 81.28 -7.62 180)
				(length 3.81)
				(name "OSC_IN/PF0/CRS__SYNC/I2C1_SDA"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin output line
				(at 81.28 -10.16 180)
				(length 3.81)
				(name "OSC_OUT/PF1/I2C1_SCL"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 81.28 -17.78 180)
				(length 3.81)
				(name "PF11-BOOT0"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "60"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 81.28 -22.86 180)
				(length 3.81)
				(name "NRST"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103R4T6"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -48.26 46.99 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Value" "STM32F103R4T6"
			(at 1.27 0 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "LQFP64"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "STM32F103R4T6_0_1"
			(pin power_in line
				(at -53.34 -17.78 0)
				(length 3.81)
				(name "VBAT"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at -53.34 -20.32 0)
				(length 3.81)
				(name "VDDA"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at -53.34 -22.86 0)
				(length 3.81)
				(name "VDD_1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at -53.34 -25.4 0)
				(length 3.81)
				(name "VDD_2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at -53.34 -27.94 0)
				(length 3.81)
				(name "VDD_3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "64"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at -53.34 -30.48 0)
				(length 3.81)
				(name "VDD_4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at -53.34 -33.02 0)
				(length 3.81)
				(name "VSSA"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at -53.34 -35.56 0)
				(length 3.81)
				(name "VSS_1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at -53.34 -38.1 0)
				(length 3.81)
				(name "VSS_2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at -53.34 -40.64 0)
				(length 3.81)
				(name "VSS_3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "63"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at -53.34 -43.18 0)
				(length 3.81)
				(name "VSS_4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
		)
		(symbol "STM32F103R4T6_1_1"
			(rectangle
				(start 49.53 -45.72)
				(end -49.53 45.72)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin bidirectional line
				(at -53.34 40.64 0)
				(length 3.81)
				(name "PA0/WKUP/USART2_CTS/ADC12_IN0/TIM2_CH1_ETR"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 38.1 0)
				(length 3.81)
				(name "PA1/USART2_RTS/ADC12_IN1/TIM2_CH2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 35.56 0)
				(length 3.81)
				(name "PA2/USART2_TX/ADC12_IN2/TIM2_CH3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 33.02 0)
				(length 3.81)
				(name "PA3/USART2_RX/ADC12_IN3/TIM2_CH4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 30.48 0)
				(length 3.81)
				(name "PA4/SPI1_NSS/USART2_CK/ADC12_IN4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 27.94 0)
				(length 3.81)
				(name "PA5/SPI1_SCK/ADC12_IN5"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 25.4 0)
				(length 3.81)
				(name "PA6/SPI1_MISO/ADC12_IN6/TIM3_CH1/TIM1_BKIN"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 22.86 0)
				(length 3.81)
				(name "PA7/SPI1_MOSI/ADC12_IN7/TIM3_CH2/TIM1_CH1N"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 20.32 0)
				(length 3.81)
				(name "PA8/USART1_CK/TIM1_CH1/MCO"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 17.78 0)
				(length 3.81)
				(name "PA9/USART1_TX/TIM1_CH2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 15.24 0)
				(length 3.81)
				(name "PA10/USART1_RX/TIM1_CH3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 12.7 0)
				(length 3.81)
				(name "PA11/USART1_CTS/CANRX/USBDM/TIM1_CH4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 10.16 0)
				(length 3.81)
				(name "PA12/USART1_RTS/CANTX/USBDP/TIM1_ETR"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 7.62 0)
				(length 3.81)
				(name "JTMS/SWDIO/PA13"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 5.08 0)
				(length 3.81)
				(name "JTCK/SWCLK/PA14"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "49"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 2.54 0)
				(length 3.81)
				(name "JTDI/TIM2_CH1_ETR/PA15/SPI1_NSS"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "50"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin input line
				(at -53.34 -2.54 0)
				(length 3.81)
				(name "OSC_IN/PD0"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin output line
				(at -53.34 -5.08 0)
				(length 3.81)
				(name "OSC_OUT/PD1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -7.62 0)
				(length 3.81)
				(name "PD2/TIM3_ETR"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "54"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -12.7 0)
				(length 3.81)
				(name "BOOT0"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "60"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -15.24 0)
				(length 3.81)
				(name "NRST"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 40.64 180)
				(length 3.81)
				(name "PB0/ADC12_IN8/TIM3_CH3/TIM1_CH2N"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 38.1 180)
				(length 3.81)
				(name "PB1/ADC12_IN9/TIM3_CH4/TIM1_CH3N"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 35.56 180)
				(length 3.81)
				(name "PB2/BOOT1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 33.02 180)
				(length 3.81)
				(name "JTDO/TIM2_CH2/PB3/TRACESWO/SPI1_SCK"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "55"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 30.48 180)
				(length 3.81)
				(name "JNTRST/TIM3_CH1/PB4/SPI1_MISO"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "56"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 27.94 180)
				(length 3.81)
				(name "PB5/I2C1_SMBA/TIM3_CH2/SPI1_MOSI"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "57"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 25.4 180)
				(length 3.81)
				(name "PB6/I2C1_SCL/USART1_TX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "58"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 22.86 180)
				(length 3.81)
				(name "PB7/I2C1_SDA/USART1_RX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "59"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 20.32 180)
				(length 3.81)
				(name "PB8/I2C1_SCL/CANRX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "61"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 17.78 180)
				(length 3.81)
				(name "PB9/I2C1_SDA/CANTX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "62"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 15.24 180)
				(length 3.81)
				(name "PB10/TIM2_CH3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 12.7 180)
				(length 3.81)
				(name "PB11/TIM2_CH4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 10.16 180)
				(length 3.81)
				(name "PB12/TIM1_BKIN"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 7.62 180)
				(length 3.81)
				(name "PB13/TIM1_CH1N"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 5.08 180)
				(length 3.81)
				(name "PB14/TIM1_CH2N"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 2.54 180)
				(length 3.81)
				(name "PB15/TIM1_CH3N"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -2.54 180)
				(length 3.81)
				(name "PC0/ADC12_IN10"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -5.08 180)
				(length 3.81)
				(name "PC1/ADC12_IN11"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -7.62 180)
				(length 3.81)
				(name "PC2/ADC12_IN12"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -10.16 180)
				(length 3.81)
				(name "PC3/ADC12_IN13"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -12.7 180)
				(length 3.81)
				(name "PC4/ADC12_IN14"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -15.24 180)
				(length 3.81)
				(name "PC5/ADC12_IN15"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -17.78 180)
				(length 3.81)
				(name "PC6/TIM3_CH1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -20.32 180)
				(length 3.81)
				(name "PC7/TIM3_CH2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -22.86 180)
				(length 3.81)
				(name "PC8/TIM3_CH3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -25.4 180)
				(length 3.81)
				(name "PC9/TIM3_CH4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -27.94 180)
				(length 3.81)
				(name "PC10"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "51"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -30.48 180)
				(length 3.81)
				(name "PC11"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "52"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -33.02 180)
				(length 3.81)
				(name "PC12"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "53"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -35.56 180)
				(length 3.81)
				(name "PC13/TMPR/RTC"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -38.1 180)
				(length 3.81)
				(name "PC14/OSC32_IN"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -40.64 180)
				(length 3.81)
				(name "PC15/OSC32_OUT"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103RBT6"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -48.26 46.99 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Value" "STM32F103RBT6"
			(at 1.27 0 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "LQFP64"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "STM32F103RBT6_0_1"
			(pin power_in line
				(at -2.54 52.07 270)
				(length 3.81)
				(name "VDD_1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 3.81)
				(name "VSS_4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 0 52.07 270)
				(length 3.81)
				(name "VDD_2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 3.81)
				(name "VSS_3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "63"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 52.07 270)
				(length 3.81)
				(name "VDD_3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "64"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 3.81)
				(name "VSS_2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 5.08 52.07 270)
				(length 3.81)
				(name "VDD_4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 5.08 -50.8 90)
				(length 3.81)
				(name "VSS_1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 53.34 -29.21 180)
				(length 3.81)
				(name "VBAT"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 53.34 -36.83 180)
				(length 3.81)
				(name "VDDA"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 53.34 -40.64 180)
				(length 3.81)
				(name "VSSA"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
		)
		(symbol "STM32F103RBT6_1_1"
			(rectangle
				(start 49.53 -46.99)
				(end -49.53 48.26)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin bidirectional line
				(at -53.34 40.64 0)
				(length 3.81)
				(name "PA0/WKUP/USART2_CTS/ADC12_IN0/TIM2_CH1_ETR"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 38.1 0)
				(length 3.81)
				(name "PA1/USART2_RTS/ADC12_IN1/TIM2_CH2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 35.56 0)
				(length 3.81)
				(name "PA2/USART2_TX/ADC12_IN2/TIM2_CH3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 33.02 0)
				(length 3.81)
				(name "PA3/USART2_RX/ADC12_IN3/TIM2_CH4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 30.48 0)
				(length 3.81)
				(name "PA4/SPI1_NSS/USART2_CK/ADC12_IN4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 27.94 0)
				(length 3.81)
				(name "PA5/SPI1_SCK/ADC12_IN5"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 25.4 0)
				(length 3.81)
				(name "PA6/SPI1_MISO/ADC12_IN6/TIM3_CH1/TIM1_BKIN"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 22.86 0)
				(length 3.81)
				(name "PA7/SPI1_MOSI/ADC12_IN7/TIM3_CH2/TIM1_CH1N"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 20.32 0)
				(length 3.81)
				(name "PA8/USART1_CK/TIM1_CH1/MCO"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 17.78 0)
				(length 3.81)
				(name "PA9/USART1_TX/TIM1_CH2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 15.24 0)
				(length 3.81)
				(name "PA10/USART1_RX/TIM1_CH3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 12.7 0)
				(length 3.81)
				(name "PA11/USART1_CTS/CANRX/USBDM/TIM1_CH4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 10.16 0)
				(length 3.81)
				(name "PA12/USART1_RTS/CANTX/USBDP/TIM1_ETR"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 7.62 0)
				(length 3.81)
				(name "JTMS/SWDIO/PA13"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 5.08 0)
				(length 3.81)
				(name "JTCK/SWCLK/PA14"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "49"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 2.54 0)
				(length 3.81)
				(name "JTDI/TIM2_CH1_ETR/PA15/SPI1_NSS"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "50"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -2.54 0)
				(length 3.81)
				(name "PB0/ADC12_IN8/TIM3_CH3/TIM1_CH2N"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -5.08 0)
				(length 3.81)
				(name "PB1/ADC12_IN9/TIM3_CH4/TIM1_CH3N"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -7.62 0)
				(length 3.81)
				(name "PB2/BOOT1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -10.16 0)
				(length 3.81)
				(name "JTDO/TIM2_CH2/PB3/TRACESWO/SPI1_SCK"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "55"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -12.7 0)
				(length 3.81)
				(name "JNTRST/TIM3_CH1/PB4/SPI1_MISO"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "56"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -15.24 0)
				(length 3.81)
				(name "PB5/I2C1_SMBAI/TIM3_CH2/SPI1_MOSI"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "57"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -17.78 0)
				(length 3.81)
				(name "PB6/I2C1_SCL/TIM4_CH1/USART1_TX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "58"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -20.32 0)
				(length 3.81)
				(name "PB7/I2C1_SDA/TIM4_CH2/USART1_RX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "59"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -22.86 0)
				(length 3.81)
				(name "PB8/TIM4_CH3/I2C1_SCL/CANRX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "61"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -25.4 0)
				(length 3.81)
				(name "PB9/TIM4_CH4/I2C1_SDA/CANTX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "62"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -27.94 0)
				(length 3.81)
				(name "PB10/I2C2_SCL/USART3_TX/TIM2_CH3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -30.48 0)
				(length 3.81)
				(name "PB11/I2C2_SDA/USART3_RX/TIM2_CH4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -33.02 0)
				(length 3.81)
				(name "PB12/SPI2_NSS/I2C2_SMBAI/USART3_CK/TIM1_BKIN"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -35.56 0)
				(length 3.81)
				(name "PB13/SPI2_SCK/USART3_CTS/TIM1_CH1N"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -38.1 0)
				(length 3.81)
				(name "PB14/SPI2_MISO/USART3_RTS/TIM1_CH2N"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -40.64 0)
				(length 3.81)
				(name "PB15/SPI2_MOSI/TIM1_CH3N"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 40.64 180)
				(length 3.81)
				(name "PC0/ADC12_IN10"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 38.1 180)
				(length 3.81)
				(name "PC1/ADC12_IN11"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 35.56 180)
				(length 3.81)
				(name "PC2/ADC12_IN12"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 33.02 180)
				(length 3.81)
				(name "PC3/ADC12_IN13"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 30.48 180)
				(length 3.81)
				(name "PC4/ADC12_IN14"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 27.94 180)
				(length 3.81)
				(name "PC5/ADC12_IN15"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 25.4 180)
				(length 3.81)
				(name "PC6/TIM3_CH1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 22.86 180)
				(length 3.81)
				(name "PC7/TIM3_CH2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 20.32 180)
				(length 3.81)
				(name "PC8/TIM3_CH3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 17.78 180)
				(length 3.81)
				(name "PC9/TIM3_CH4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 15.24 180)
				(length 3.81)
				(name "PC10/USART3_TX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "51"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 12.7 180)
				(length 3.81)
				(name "PC11/USART3_RX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "52"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 10.16 180)
				(length 3.81)
				(name "PC12/USART3_CK"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "53"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 7.62 180)
				(length 3.81)
				(name "PC13/TMPR/RTC"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 5.08 180)
				(length 3.81)
				(name "PC14/OSC32_IN"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 2.54 180)
				(length 3.81)
				(name "PC15/OSC32_OUT"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -2.54 180)
				(length 3.81)
				(name "PD2/TIM3_ETR"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "54"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin input line
				(at 53.34 -7.62 180)
				(length 3.81)
				(name "OSC_IN/PD0"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin output line
				(at 53.34 -10.16 180)
				(length 3.81)
				(name "OSC_OUT/PD1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -19.05 180)
				(length 3.81)
				(name "BOOT0"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "60"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -24.13 180)
				(length 3.81)
				(name "NRST"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103RCT6"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -48.26 48.26 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Value" "STM32F103RCT6"
			(at -27.94 48.26 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103rc.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "LQFP64"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "STM32F103RCT6_0_1"
			(pin power_in line
				(at -2.54 50.8 270)
				(length 3.81)
				(name "VDD_4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at -2.54 -52.07 90)
				(length 3.81)
				(name "VSS_1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 3.81)
				(name "VDD_3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "64"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -52.07 90)
				(length 3.81)
				(name "VSS_2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 3.81)
				(name "VDD_2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 -52.07 90)
				(length 3.81)
				(name "VSS_3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "63"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 5.08 50.8 270)
				(length 3.81)
				(name "VDD_1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 5.08 -52.07 90)
				(length 3.81)
				(name "VSS_4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 53.34 -30.48 180)
				(length 3.81)
				(name "VBAT"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 53.34 -35.56 180)
				(length 3.81)
				(name "VDDA"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at 53.34 -40.64 180)
				(length 3.81)
				(name "VSSA"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
		)
		(symbol "STM32F103RCT6_1_1"
			(rectangle
				(start 49.53 -48.26)
				(end -49.53 46.99)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin bidirectional line
				(at -53.34 40.64 0)
				(length 3.81)
				(name "PA0/WKUP/USART2_CTS/ADC123_IN0/TIM2_CH1_ETR/TIM5_CH1/TIM8_ETR"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 38.1 0)
				(length 3.81)
				(name "PA1/USART2_RTS/ADC123_IN1/TIM2_CH2/TIM5_CH2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 35.56 0)
				(length 3.81)
				(name "PA2/USART2_TX/ADC123_IN2/TIM2_CH3/TIM5_CH3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 33.02 0)
				(length 3.81)
				(name "PA3/USART2_RX/ADC123_IN3/TIM2_CH4/TIM5_CH4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 30.48 0)
				(length 3.81)
				(name "PA4/SPI1_NSS/USART2_CK/ADC12_IN4/DAC_OUT1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 27.94 0)
				(length 3.81)
				(name "PA5/SPI1_SCK/ADC12_IN5/DAC_OUT2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 25.4 0)
				(length 3.81)
				(name "PA6/SPI1_MISO/ADC12_IN6/TIM3_CH1/TIM1_BKIN/TIM8_BKIN"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 22.86 0)
				(length 3.81)
				(name "PA7/SPI1_MOSI/ADC12_IN7/TIM3_CH2/TIM8_CH1N/TIM1_CH1N"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 20.32 0)
				(length 3.81)
				(name "PA8/USART1_CK/TIM1_CH1/MCO"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 17.78 0)
				(length 3.81)
				(name "PA9/USART1_TX/TIM1_CH2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 15.24 0)
				(length 3.81)
				(name "PA10/USART1_RX/TIM1_CH3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 12.7 0)
				(length 3.81)
				(name "PA11/USART1_CTS/CANRX/USBDM/TIM1_CH4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 10.16 0)
				(length 3.81)
				(name "PA12/USART1_RTS/CANTX/USBDP/TIM1_ETR"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 7.62 0)
				(length 3.81)
				(name "JTMS/SWDIO/PA13"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 5.08 0)
				(length 3.81)
				(name "JTCK/SWCLK/PA14"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "49"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 2.54 0)
				(length 3.81)
				(name "JTDI/SPI3_NSS/I2S3_WS/TIM2_CH1_ETR/PA15/SPI1_NSS"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "50"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -2.54 0)
				(length 3.81)
				(name "PB0/ADC12_IN8/TIM3_CH3/TIM8_CH2N/TIM1_CH2N"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -5.08 0)
				(length 3.81)
				(name "PB1/ADC12_IN9/TIM3_CH4/TIM8_CH3N/TIM1_CH3N"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -7.62 0)
				(length 3.81)
				(name "PB2/BOOT1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -10.16 0)
				(length 3.81)
				(name "JTDO/SPI3_SCK/I2S3_CK/TIM2_CH2/PB3/TRACESWO/SPI1_SCK"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "55"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -12.7 0)
				(length 3.81)
				(name "JNTRST/SPI3_MISO/TIM3_CH1/PB4/SPI1_MISO"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "56"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -15.24 0)
				(length 3.81)
				(name "PB5/I2C1_SMBA/SPI3_MOSI/I2S3_SD/TIM3_CH2/SPI1_MOSI"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "57"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -17.78 0)
				(length 3.81)
				(name "PB6/I2C1_SCL/TIM4_CH1/USART1_TX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "58"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -20.32 0)
				(length 3.81)
				(name "PB7/I2C1_SDA/TIM4_CH2/USART1_RX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "59"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -22.86 0)
				(length 3.81)
				(name "PB8/TIM4_CH3/SDIO_D4/I2C1_SCL/CANRX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "61"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -25.4 0)
				(length 3.81)
				(name "PB9/TIM4_CH4/SDIO_D5//I2C1_SDA/CANTX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "62"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -27.94 0)
				(length 3.81)
				(name "PB10/I2C2_SCL/USART3_TX/TIM2_CH3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -30.48 0)
				(length 3.81)
				(name "PB11/I2C2_SDA/USART3_RX/TIM2_CH4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -33.02 0)
				(length 3.81)
				(name "PB12/SPI2_NSS/I2C2_SMBA/USART3_CK/TIM1_BKIN/I2S2_WS"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -35.56 0)
				(length 3.81)
				(name "PB13/SPI2_SCK/I2S2_CK/USART3_CTS/TIM1_CH1N"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -38.1 0)
				(length 3.81)
				(name "PB14/SPI2_MISO/USART3_RTS/TIM1_CH2N"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -40.64 0)
				(length 3.81)
				(name "PB15/SPI2_MOSI/TIM1_CH3N/I2S2_SD"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 40.64 180)
				(length 3.81)
				(name "PC0/ADC123_IN10"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 38.1 180)
				(length 3.81)
				(name "PC1/ADC123_IN11"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 35.56 180)
				(length 3.81)
				(name "PC2/ADC123_IN12"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 33.02 180)
				(length 3.81)
				(name "PC3/ADC123_IN13"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 30.48 180)
				(length 3.81)
				(name "PC4/ADC12_IN14"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 27.94 180)
				(length 3.81)
				(name "PC5/ADC12_IN15"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 25.4 180)
				(length 3.81)
				(name "PC6/I2S2_MCK/TIM8_CH1/SDIO_D6/TIM3_CH1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 22.86 180)
				(length 3.81)
				(name "PC7/I2S3_MCK/TIM8_CH2/SDIO_D7/TIM3_CH2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 20.32 180)
				(length 3.81)
				(name "PC8/TIM8_CH3/SDIO_D0/TIM3_CH3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 17.78 180)
				(length 3.81)
				(name "PC9/TIM8_CH4/SDIO_D1/TIM3_CH4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 15.24 180)
				(length 3.81)
				(name "PC10/UART4_TX/SDIO_D2/USART3_TX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "51"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 12.7 180)
				(length 3.81)
				(name "PC11/UART4_RX/SDIO_D3/USART3_RX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "52"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 10.16 180)
				(length 3.81)
				(name "PC12/UART5_TX/SDIO_CK/USART3_CK"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "53"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 7.62 180)
				(length 3.81)
				(name "PC13/TMPR/RTC"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 5.08 180)
				(length 3.81)
				(name "PC14/OSC32_IN"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 2.54 180)
				(length 3.81)
				(name "PC15/OSC32_OUT"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -2.54 180)
				(length 3.81)
				(name "PD2/TIM3_ETR/UART5_RX/SDIO_CMD"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "54"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin input line
				(at 53.34 -10.16 180)
				(length 3.81)
				(name "OSC_IN/PD0/CANRX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin output line
				(at 53.34 -12.7 180)
				(length 3.81)
				(name "OSC_OUT/PD1/CANTX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -20.32 180)
				(length 3.81)
				(name "BOOT0"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "60"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -25.4 180)
				(length 3.81)
				(name "NRST"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103RFT6"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -48.26 46.99 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Value" "STM32F103RFT6"
			(at 1.27 0 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "LQFP64"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "STM32F103RFT6_0_1"
			(pin power_in line
				(at -53.34 -17.78 0)
				(length 3.81)
				(name "VBAT"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at -53.34 -20.32 0)
				(length 3.81)
				(name "VDDA"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at -53.34 -22.86 0)
				(length 3.81)
				(name "VDD_1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at -53.34 -25.4 0)
				(length 3.81)
				(name "VDD_2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at -53.34 -27.94 0)
				(length 3.81)
				(name "VDD_3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "64"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at -53.34 -30.48 0)
				(length 3.81)
				(name "VDD_4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at -53.34 -33.02 0)
				(length 3.81)
				(name "VSSA"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at -53.34 -35.56 0)
				(length 3.81)
				(name "VSS_1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at -53.34 -38.1 0)
				(length 3.81)
				(name "VSS_2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at -53.34 -40.64 0)
				(length 3.81)
				(name "VSS_3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "63"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin power_in line
				(at -53.34 -43.18 0)
				(length 3.81)
				(name "VSS_4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
		)
		(symbol "STM32F103RFT6_1_1"
			(rectangle
				(start 49.53 -45.72)
				(end -49.53 45.72)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin bidirectional line
				(at -53.34 40.64 0)
				(length 3.81)
				(name "PA0/WKUP/USART2_CTS/ADC123_IN0/TIM2_CH1_ETR/TIM5_CH1/TIM8_ETR"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 38.1 0)
				(length 3.81)
				(name "PA1/USART2_RTS/ADC123_IN1/TIM2_CH2/TIM5_CH2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 35.56 0)
				(length 3.81)
				(name "PA2/USART2_TX/ADC123_IN2/TIM2_CH3/TIM5_CH3/TIM9_CH1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 33.02 0)
				(length 3.81)
				(name "PA3/USART2_RX/ADC123_IN3/TIM2_CH4/TIM5_CH4/TIM9_CH2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 30.48 0)
				(length 3.81)
				(name "PA4/SPI1_NSS/USART2_CK/ADC12_IN4/DAC_OUT1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 27.94 0)
				(length 3.81)
				(name "PA5/SPI1_SCK/ADC12_IN5/DAC_OUT2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 25.4 0)
				(length 3.81)
				(name "PA6/SPI1_MISO/ADC12_IN6/TIM3_CH1/TIM8_BKIN/TIM13_CH1/TIM1_BKIN"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 22.86 0)
				(length 3.81)
				(name "PA7/SPI1_MOSI/ADC12_IN7/TIM3_CH2/TIM8_CH1N/TIM14_CH1/TIM1_CH1N"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 20.32 0)
				(length 3.81)
				(name "PA8/USART1_CK/TIM1_CH1/MCO"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 17.78 0)
				(length 3.81)
				(name "PA9/USART1_TX/TIM1_CH2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 15.24 0)
				(length 3.81)
				(name "PA10/USART1_RX/TIM1_CH3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 12.7 0)
				(length 3.81)
				(name "PA11/USART1_CTS/CANRX/USBDM/TIM1_CH4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 10.16 0)
				(length 3.81)
				(name "PA12/USART1_RTS/CANTX/USBDP/TIM1_ETR"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 7.62 0)
				(length 3.81)
				(name "JTMS/SWDIO/PA13"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 5.08 0)
				(length 3.81)
				(name "JTCK/SWCLK/PA14"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "49"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 2.54 0)
				(length 3.81)
				(name "JTDI/SPI3_NSS/I2S3_WS/TIM2_CH1_ETR/PA15/SPI1_NSS"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "50"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin input line
				(at -53.34 -2.54 0)
				(length 3.81)
				(name "OSC_IN/PD0"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin output line
				(at -53.34 -5.08 0)
				(length 3.81)
				(name "OSC_OUT/PD1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -7.62 0)
				(length 3.81)
				(name "PD2/TIM3_ETR/UART5_RX/SDIO_CMD"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "54"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -12.7 0)
				(length 3.81)
				(name "BOOT0"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "60"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -15.24 0)
				(length 3.81)
				(name "NRST"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 40.64 180)
				(length 3.81)
				(name "PB0/ADC12_IN8/TIM3_CH3/TIM8_CH2N/TIM1_CH2N"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 38.1 180)
				(length 3.81)
				(name "PB1/ADC12_IN9/TIM3_CH4/TIM8_CH3N/TIM1_CH3N"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 35.56 180)
				(length 3.81)
				(name "PB2/BOOT1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 33.02 180)
				(length 3.81)
				(name "JTDO/SPI3_SCK/I2S3_CK/TIM2_CH2/PB3/TRACESWO/SPI1_SCK"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "55"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 30.48 180)
				(length 3.81)
				(name "JNTRST/SPI3_MISO/TIM3_CH1/PB4/SPI1_MISO"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "56"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 27.94 180)
				(length 3.81)
				(name "PB5/I2C1_SMBA/SPI3_MOSI/I2S3_SD/TIM3_CH2/SPI1_MOSI"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "57"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 25.4 180)
				(length 3.81)
				(name "PB6/I2C1_SCL/TIM4_CH1/USART1_TX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "58"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 22.86 180)
				(length 3.81)
				(name "PB7/I2C1_SDA/TIM4_CH2/USART1_RX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "59"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 20.32 180)
				(length 3.81)
				(name "PB8/TIM4_CH3/SDIO_D4/TIM10_CH1/I2C1_SCL/CANRX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "61"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 17.78 180)
				(length 3.81)
				(name "PB9/TIM4_CH4/SDIO_D5/TIM11_CH1/I2C1_SDA/CANTX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "62"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 15.24 180)
				(length 3.81)
				(name "PB10/I2C2_SCL/USART3_TX/TIM2_CH3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 12.7 180)
				(length 3.81)
				(name "PB11/I2C2_SDA/USART3_RX/TIM2_CH4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 10.16 180)
				(length 3.81)
				(name "PB12/SPI2_NSS/I2C2_SMBA/USART3_CK/TIM1_BKIN/I2S2_WS"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 7.62 180)
				(length 3.81)
				(name "PB13/SPI2_SCK/USART3_CTS/TIM1_CH1N/I2S2_CK"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 5.08 180)
				(length 3.81)
				(name "PB14/SPI2_MISO/USART3_RTS/TIM1_CH2N/TIM12_CH1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 2.54 180)
				(length 3.81)
				(name "PB15/SPI2_MOSI/TIM1_CH3N/I2S2_SD/TIM12_CH2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -2.54 180)
				(length 3.81)
				(name "PC0/ADC123_IN10"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -5.08 180)
				(length 3.81)
				(name "PC1/ADC123_IN11"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -7.62 180)
				(length 3.81)
				(name "PC2/ADC123_IN12"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -10.16 180)
				(length 3.81)
				(name "PC3/ADC123_IN13"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -12.7 180)
				(length 3.81)
				(name "PC4/ADC12_IN14"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -15.24 180)
				(length 3.81)
				(name "PC5/ADC12_IN15"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -17.78 180)
				(length 3.81)
				(name "PC6/I2S2_MCK/TIM8_CH1/SDIO_D6/TIM3_CH1"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -20.32 180)
				(length 3.81)
				(name "PC7/I2S3_MCK/TIM8_CH2/SDIO_D7/TIM3_CH2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -22.86 180)
				(length 3.81)
				(name "PC8/TIM8_CH3/SDIO_D0/TIM3_CH3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -25.4 180)
				(length 3.81)
				(name "PC9/TIM8_CH4/SDIO_D1/TIM3_CH4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -27.94 180)
				(length 3.81)
				(name "PC10/UART4_TX/SDIO_D2/USART3_TX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "51"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -30.48 180)
				(length 3.81)
				(name "PC11/UART4_RX/SDIO_D3/USART3_RX"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "52"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -33.02 180)
				(length 3.81)
				(name "PC12/UART5_TX/SDIO_CK/USART3_CK"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "53"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -35.56 180)
				(length 3.81)
				(name "PC13/TMPR/RTC"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -38.1 180)
				(length 3.81)
				(name "PC14/OSC32_IN"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
			(pin bidirectional line
				(at 53.34 -40.64 180)
				(length 3.81)
				(name "PC15/OSC32_OUT"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 0.9906 0.9906)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103VBT6"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "STM32F103VBT6"
			(at -6.35 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "LQFP100_M"
			(at -7.62 -162.56 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "STM32 ARM-based 32-bit MCU with 64 Kbytes Flash, 100-pin LQFP, Industrial Temperature"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -7.62 -167.64 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Package" "LQFP100"
			(at -7.62 -170.18 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -7.62 -172.72 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Manufacturer" "ST"
			(at -7.62 -175.26 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Part_Number" "STM32F103VBT6"
			(at -7.62 -177.8 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Comment" "STM32F103VBT6"
			(at -3.81 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(symbol "STM32F103VBT6_1_1"
			(rectangle
				(start 0 -157.48)
				(end 83.82 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin bidirectional line
				(at -7.62 -2.54 0)
				(length 7.62)
				(name "PA0-WKUP/USART2_CTS/_ADC12_IN0/_TIM2_CH1_ETR"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -5.08 0)
				(length 7.62)
				(name "PA1/USART2_RTS/ADC12_IN1/TIM2_CH2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -7.62 0)
				(length 7.62)
				(name "PA2/USART2_TX/ADC12_IN2/TIM2_CH3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -10.16 0)
				(length 7.62)
				(name "PA3/USART2_RX/ADC12_IN3/TIM2_CH4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -12.7 0)
				(length 7.62)
				(name "PA4/SPI1_NSS/USART2_CK/ADC12_IN4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -15.24 0)
				(length 7.62)
				(name "PA5/SPI1_SCK/ADC12_IN5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -17.78 0)
				(length 7.62)
				(name "PA6/SPI1_MISO/ADC12_IN6/TIM3_CH1//TIM1_BKIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -20.32 0)
				(length 7.62)
				(name "PA7/SPI1_MOSI/ADC12_IN7/TIM3_CH2//TIM1_CH1N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -25.4 0)
				(length 7.62)
				(name "PA8/USART1_CK/TIM1_CH1/MCO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "67"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -27.94 0)
				(length 7.62)
				(name "PA9/USART1_TX/IM1_CH2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "68"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -30.48 0)
				(length 7.62)
				(name "PA10/USART1_RX/TIM1_CH3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "69"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -33.02 0)
				(length 7.62)
				(name "PA11/USART1_CTS/USBDM/CAN_RX/TIM1_CH4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "70"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -35.56 0)
				(length 7.62)
				(name "PA12/USART1_RTS/USBDP/_CAN_TX/TIM1_ETR"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "71"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -38.1 0)
				(length 7.62)
				(name "PA13/JTMS/SWDIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "72"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -40.64 0)
				(length 7.62)
				(name "PA14/JTCK/SWCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "76"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -43.18 0)
				(length 7.62)
				(name "PA15/JTDI//TIM2_CH1_ETR/PA15/SPI1_NSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "77"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -48.26 0)
				(length 7.62)
				(name "PB0/ADC12_IN8/TIM3_CH3//TIM1_CH2N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -50.8 0)
				(length 7.62)
				(name "PB1/ADC12_IN9/TIM3_CH4//TIM1_CH3N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -53.34 0)
				(length 7.62)
				(name "PB2/BOOT1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -55.88 0)
				(length 7.62)
				(name "PB3/JTDO//PB3/TRACESWO/TIM2_CH2/SPI1_SCK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "89"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -58.42 0)
				(length 7.62)
				(name "PB4/JNTRST//PB4/TIM3_CH1/SPI1_MISO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "90"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -60.96 0)
				(length 7.62)
				(name "PB5/I2C1_SMBAI//TIM3_CH2/_SPI1_MOSI"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "91"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -63.5 0)
				(length 7.62)
				(name "PB6/I2C1_SCL/TIM4_CH1//USART1_TX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "92"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -66.04 0)
				(length 7.62)
				(name "PB7/I2C1_SDA/TIM4_CH2//USART1_RX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "93"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -71.12 0)
				(length 7.62)
				(name "PB8/TIM4_CH3//I2C1_SCL/CAN_RX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "95"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -73.66 0)
				(length 7.62)
				(name "PB9/TIM4_CH4//I2C1_SDA/CAN_TX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "96"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -76.2 0)
				(length 7.62)
				(name "PB10/I2C2_SCL/USART3_TX//TIM2_CH3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -78.74 0)
				(length 7.62)
				(name "PB11/I2C2_SDA/USART3_RX//TIM2_CH4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -83.82 0)
				(length 7.62)
				(name "PB12/SPI2_NSS/I2C2_SMBAI/USART3_CK/TIM1_BKIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "51"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -86.36 0)
				(length 7.62)
				(name "PB13/SPI2_SCK/USART3_CTS/TIM1_CH1N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "52"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -88.9 0)
				(length 7.62)
				(name "PB14/SPI2_MISO/USART3_RTS/TIM1_CH2N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "53"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -91.44 0)
				(length 7.62)
				(name "PB15/SPI2_MOSI/TIM1_CH3N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "54"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input clock
				(at -7.62 -96.52 0)
				(length 7.62)
				(name "OSC_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at -7.62 -99.06 0)
				(length 7.62)
				(name "OSC_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -7.62 -104.14 0)
				(length 7.62)
				(name "BOOT0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "94"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -109.22 0)
				(length 7.62)
				(name "NRST"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 -116.84 0)
				(length 7.62)
				(name "VREF-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 -119.38 0)
				(length 7.62)
				(name "VREF+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 -127 0)
				(length 7.62)
				(name "NC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "73"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 -134.62 0)
				(length 7.62)
				(name "VBAT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 -139.7 0)
				(length 7.62)
				(name "VDD_1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "50"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 -142.24 0)
				(length 7.62)
				(name "VDD_2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "75"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 -144.78 0)
				(length 7.62)
				(name "VDD_3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "100"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 -147.32 0)
				(length 7.62)
				(name "VDD_4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 -149.86 0)
				(length 7.62)
				(name "VDD_5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 -154.94 0)
				(length 7.62)
				(name "VDDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -2.54 180)
				(length 7.62)
				(name "PC0/ADC12_IN10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -5.08 180)
				(length 7.62)
				(name "PC1/ADC12_IN11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -7.62 180)
				(length 7.62)
				(name "PC2/ADC12_IN12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -10.16 180)
				(length 7.62)
				(name "PC3/ADC12_IN13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -12.7 180)
				(length 7.62)
				(name "PC4/ADC12_IN14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -15.24 180)
				(length 7.62)
				(name "PC5/ADC12_IN15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -17.78 180)
				(length 7.62)
				(name "PC6//TIM3_CH1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "63"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -20.32 180)
				(length 7.62)
				(name "PC7//TIM3_CH2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "64"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -25.4 180)
				(length 7.62)
				(name "PC8//TIM3_CH3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "65"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -27.94 180)
				(length 7.62)
				(name "PC9//TIM3_CH4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "66"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -30.48 180)
				(length 7.62)
				(name "PC10//USART3_TX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "78"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -33.02 180)
				(length 7.62)
				(name "PC11//USART3_RX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "79"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -35.56 180)
				(length 7.62)
				(name "PC12//USART3_CK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "80"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -38.1 180)
				(length 7.62)
				(name "PC13-TAMPER-RTC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -40.64 180)
				(length 7.62)
				(name "PC14-OSC32_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -43.18 180)
				(length 7.62)
				(name "PC15-OSC32_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -48.26 180)
				(length 7.62)
				(name "PD0//CAN_RX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "81"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -50.8 180)
				(length 7.62)
				(name "PD1//CAN_TX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "82"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -53.34 180)
				(length 7.62)
				(name "PD2/TIM3_ETR"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "83"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -55.88 180)
				(length 7.62)
				(name "PD3//USART2_CTS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "84"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -58.42 180)
				(length 7.62)
				(name "PD4//USART2_RTS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "85"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -60.96 180)
				(length 7.62)
				(name "PD5//USART2_TX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "86"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -63.5 180)
				(length 7.62)
				(name "PD6//USART2_RX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "87"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -66.04 180)
				(length 7.62)
				(name "PD7//USART2_CK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "88"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -71.12 180)
				(length 7.62)
				(name "PD8//USART3_TX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "55"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -73.66 180)
				(length 7.62)
				(name "PD9//USART3_RX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "56"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -76.2 180)
				(length 7.62)
				(name "PD10//USART3_CK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "57"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -78.74 180)
				(length 7.62)
				(name "PD11//USART3_CTS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "58"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -81.28 180)
				(length 7.62)
				(name "PD12//TIM4_CH1/USART3_RTS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "59"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -83.82 180)
				(length 7.62)
				(name "PD13//TIM4_CH2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "60"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -86.36 180)
				(length 7.62)
				(name "PD14//TIM4_CH3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "61"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -88.9 180)
				(length 7.62)
				(name "PD15//TIM4_CH4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "62"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -93.98 180)
				(length 7.62)
				(name "PE0/TIM4_ETR"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "97"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -96.52 180)
				(length 7.62)
				(name "PE1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "98"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -99.06 180)
				(length 7.62)
				(name "PE2/TRACECK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -101.6 180)
				(length 7.62)
				(name "PE3/TRACED0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -104.14 180)
				(length 7.62)
				(name "PE4/TRACED1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -106.68 180)
				(length 7.62)
				(name "PE5/TRACED2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -109.22 180)
				(length 7.62)
				(name "PE6/TRACED3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -111.76 180)
				(length 7.62)
				(name "PE7//TIM1_ETR"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -116.84 180)
				(length 7.62)
				(name "PE8//TIM1_CH1N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -119.38 180)
				(length 7.62)
				(name "PE9//TIM1_CH1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -121.92 180)
				(length 7.62)
				(name "PE10//TIM1_CH2N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -124.46 180)
				(length 7.62)
				(name "PE11//TIM1_CH2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -127 180)
				(length 7.62)
				(name "PE12//TIM1_CH3N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -129.54 180)
				(length 7.62)
				(name "PE13//TIM1_CH3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -132.08 180)
				(length 7.62)
				(name "PE14//TIM1_CH4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 91.44 -134.62 180)
				(length 7.62)
				(name "PE15//TIM1_BKIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 91.44 -139.7 180)
				(length 7.62)
				(name "VSS_1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "49"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 91.44 -142.24 180)
				(length 7.62)
				(name "VSS_2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "74"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 91.44 -144.78 180)
				(length 7.62)
				(name "VSS_3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "99"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 91.44 -147.32 180)
				(length 7.62)
				(name "VSS_4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 91.44 -149.86 180)
				(length 7.62)
				(name "VSS_5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 91.44 -154.94 180)
				(length 7.62)
				(name "VSSA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F373VxT"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -0.0254 6.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "STM32F373VxT"
			(at 1.2446 8.89 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SQFP50P1600X1600-100M"
			(at -0.0254 -99.06 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Imported"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -0.0254 -101.6 0)
			(effects
				(font
					(size 1.016 1.016)
				)
				(hide yes)
			)
		)
		(property "Value_1" "Value"
			(at -0.0254 -104.14 0)
			(effects
				(font
					(size 1.016 1.016)
				)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -0.0254 -109.22 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Part_Number" "STM32F373VxT"
			(at -0.0254 -116.84 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Comment" "*"
			(at 3.7846 6.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(symbol "STM32F373VxT_1_1"
			(rectangle
				(start 7.62 -93.98)
				(end 215.9 5.08)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin bidirectional line
				(at 0 0 0)
				(length 7.62)
				(name "PA0/USART2_CTS,_TIM2_CH1_ETR,_TIM5_CH1_ETR,_TIM19_CH1,_TSC_G1_IO1,_COMP1_OUT/RTC__TAMPER2,_WKUP1,_ADC_IN0,_COMP1_INM"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -2.54 0)
				(length 7.62)
				(name "PA1/SPI3_SCK/I2S3_CK,_USART2_RTS,_TIM2_CH2,_TIM15_CH1N,_TIM5_CH2,_TIM19_CH2,_TSC_G1_IO2,_RTC_REFIN/ADC_IN1,_COMP1_INP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -5.08 0)
				(length 7.62)
				(name "PA2/COMP2_OUT,_SPI3_MISO/I2S3_MCK,_USART2_TX,_TIM2_CH3,_TIM15_CH1,_TIM5_CH3,_TIM19_CH3,_TSC_G1_IO3/ADC_IN2,_COMP2_INM"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -7.62 0)
				(length 7.62)
				(name "PA3/SPI3_MOSI/I2S3_SD,_USART2_RX,_TIM2_CH4,_TIM15_CH2,_TIM5_CH4,_TIM19_CH4,_TSC_G1_IO4/ADC_IN3,_COMP2_INP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -10.16 0)
				(length 7.62)
				(name "PA4/SPI1_NSS/I2S1_WS,_SPI3_NSS/I2S3_WS,_USART2_CK,_TIM3_CH2,_TIM12_CH1,_TSC_G2_IO1,_ADC_IN4,_DAC1_OUT1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -12.7 0)
				(length 7.62)
				(name "PA5/SPI1_SCK/I2S1_CK,_CEC,_TIM2_CH1_ETR,_TIM14_CH1,_TIM12_CH2,_TSC_G2_IO2_ADC_IN5,_DAC1_OUT2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -15.24 0)
				(length 7.62)
				(name "PA6/SPI1_MISO/I2S1_MCK,_COMP1_OUT,_TIM3_CH1,_TIM13_CH1,_TIM16_CH1,_TSC_G2_IO3_ADC_IN6,_DAC2_OUT1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -17.78 0)
				(length 7.62)
				(name "PA7/TSC_G2_IO4,_TIM14_CH1,_SPI1_MOSI/I2S1_SD,_TIM17_CH1,_TIM3_CH2,_COMP2_OUT_ADC_IN7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -20.32 0)
				(length 7.62)
				(name "PA8/SPI2_SCK/I2S2_CK,_I2C2_SMBA,_USART1_CK,_TIM4_ETR,_TIM5_CH1_ETR,_MCO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "67"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -22.86 0)
				(length 7.62)
				(name "PA9/SPI2_MISO/I2S2_MCK,_I2C2_SCL,_USART1_TX,_TIM2_CH3,_TIM15_BKIN,_TIM13_CH1,_TSC_G4_IO1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "68"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -25.4 0)
				(length 7.62)
				(name "PA10/SPI2_MOSI/I2S2_SD,_I2C2_SDA,_USART1_RX,_TIM2_CH4,_TIM17_BKIN,_TIM14_CH1,_TSC_G4_IO2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "69"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -27.94 0)
				(length 7.62)
				(name "PA11/SPI2_NSS/I2S2_WS,_SPI1_NSS/I2S1_WS,_USART1_CTS,_CAN_RX,_TIM4_CH1,_USB_DM,_TIM5_CH2,_COMP1_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "70"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -30.48 0)
				(length 7.62)
				(name "PA12/SPI1_SCK/I2S1_CK,_USART1_RTS,_CAN_TX,_USB_DP,_TIM16_CH1,_TIM4_CH2,_TIM5_CH3,_COMP2_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "71"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -33.02 0)
				(length 7.62)
				(name "PA13/SPI1_MISO/I2S1_MCK,_USART3_CTS,_IR_OUT,_TIM16_CH1N,_TIM4_CH3,_TIM5_CH4,_TSC_G4_IO3,_SWDIO-JTMS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "72"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -35.56 0)
				(length 7.62)
				(name "PA14/I2C1_SDA,_TIM12_CH1,_TSC_G4_IO4,_SWCLK-JTCK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "76"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -38.1 0)
				(length 7.62)
				(name "PA15/SPI1_NSS/I2S1_WS,_SPI3_NSS/I2S3_WS,_I2C1_SCL,_TIM2_CH1_ETR,_TIM12_CH2,_TSC_SYNC,_JTDI"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "77"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -43.18 0)
				(length 7.62)
				(name "PB3/SPI1_SCK/I2S1_CK,_SPI3_SCK/I2S3_CK,_USART2_TX,_TIM2_CH2,_TIM3_ETR,_TIM4_ETR,_TIM13_CH1,_TSC_G5_IO1,_JTDO-TRACESWO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "89"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -45.72 0)
				(length 7.62)
				(name "PB4/SPI1_MISO/I2S1_MCK,_SPI3_MISO/I2S3_MCK,_USART2_RX,_TIM16_CH1,_TIM3_CH1,_TIM17_BKIN,_TIM15_CH1N,_TSC_G5_IO2,_NJTRST"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "90"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -48.26 0)
				(length 7.62)
				(name "PB5/SPI1_MOSI/I2S1_SD,_SPI3_MOSI/I2S3_SD,_I2C1_SMBAl,_USART2_CK,_TIM16_BKIN,_TIM3_CH2,_TIM17_CH1,_TIM19_ETR"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "91"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -50.8 0)
				(length 7.62)
				(name "PB6/I2C1_SCL,_USART1_TX,_TIM16_CH1N,_TIM3_CH3,_TIM4_CH1,_TIM19_CH1,_TIM15_CH1,_TSC_G5_IO3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "92"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -53.34 0)
				(length 7.62)
				(name "PB7/I2C1_SDA,_USART1_RX,_TIM17_CH1N,_TIM3_CH4,_TIM4_CH2,_TIM19_CH2,_TIM15_CH2,_TSC_G5_IO4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "93"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -55.88 0)
				(length 7.62)
				(name "PB8/SPI2_SCK/I2S2_CK,_I2C1_SCL,_USART3_TX,_CAN_RX,_CEC,_TIM16_CH1,_TIM4_CH3,_TIM19_CH3,_COMP1_OUT,_TSC_SYNC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "95"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -58.42 0)
				(length 7.62)
				(name "PB9/SPI2_NSS/I2S2_WS,_I2C1_SDA,_USART3_RX,_CAN_TX,_IR_OUT,_TIM17_CH1,_TIM4_CH4,_TIM19_CH4,_COMP2_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "96"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -63.5 0)
				(length 7.62)
				(name "PF0-OSC_IN/I2C2_SDA_OSC_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -66.04 0)
				(length 7.62)
				(name "PF1-OSC_OUT/I2C2_SCL_OSC_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -68.58 0)
				(length 7.62)
				(name "PF2/I2C2_SMBA_"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -71.12 0)
				(length 7.62)
				(name "PF4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -73.66 0)
				(length 7.62)
				(name "PF6/SPI1_MOSI/I2S1_SD,_USART3_RTS,_TIM4_CH4,_I2C2_SCL"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "73"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -76.2 0)
				(length 7.62)
				(name "PF9/TIM14_CH1_"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -78.74 0)
				(length 7.62)
				(name "PF10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -83.82 0)
				(length 7.62)
				(name "NRST"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 0 -88.9 0)
				(length 7.62)
				(name "BOOT0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "94"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 0 180)
				(length 7.62)
				(name "PC0/TIM5_CH1_ETR_ADC_IN10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -2.54 180)
				(length 7.62)
				(name "PC1/TIM5_CH2_ADCIN11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -5.08 180)
				(length 7.62)
				(name "PC2/SPI2_MISO/I2S2_MCK,_TIM5_CH3_ADC_IN12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -7.62 180)
				(length 7.62)
				(name "PC3/SPI2_MOSI/I2S2_SD,_TIM5_CH4_ADC_IN13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -10.16 180)
				(length 7.62)
				(name "PC4/TIM13_CH1,_TSC_G3_IO1,_USART1_TX_ADC_IN14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -12.7 180)
				(length 7.62)
				(name "PC5/TSC_G3_IO2,_USART1_RX_ADC_IN15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -15.24 180)
				(length 7.62)
				(name "PC6/TIM3_CH1,_SPI1_NSS/I2S1_WS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "63"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -17.78 180)
				(length 7.62)
				(name "PC7/TIM3_CH2,_SPI1_SCK/I2S1_CK,"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "64"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -20.32 180)
				(length 7.62)
				(name "PC8/SPI1_MISO/I2S1_MCK,_TIM3_CH3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "65"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -22.86 180)
				(length 7.62)
				(name "PC9/SPI1_MOSI/I2S1_SD,_TIM3_CH4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "66"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -25.4 180)
				(length 7.62)
				(name "PC10/SPI3_SCK/I2S3_CK,_USART3_TX,_TIM19_CH1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "78"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -27.94 180)
				(length 7.62)
				(name "PC11/SPI3_MISO/I2S3_MCK,_USART3_RX,_TIM19_CH2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "79"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -30.48 180)
				(length 7.62)
				(name "PC12/SPI3_MOSI/I2S3_SD,_USART3_CK,_TIM19_CH3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "80"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -33.02 180)
				(length 7.62)
				(name "PC13/WKUP2,_ALARM_OUT,_CALIB_OUT,_TIMESTAMP,_RTC_TAMPER1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -35.56 180)
				(length 7.62)
				(name "PC14-OSC32_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -38.1 180)
				(length 7.62)
				(name "PC15-OSC32_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -43.18 180)
				(length 7.62)
				(name "PD0/CAN_RX,_TIM19_CH4_"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "81"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -45.72 180)
				(length 7.62)
				(name "PD1/CAN_TX,_TIM19_ETR_"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "82"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -48.26 180)
				(length 7.62)
				(name "PD2/TIM3_ETR_"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "83"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -50.8 180)
				(length 7.62)
				(name "PD3/SPI2_MISO/I2S2_MCK,_USART2_CTS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "84"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -53.34 180)
				(length 7.62)
				(name "PD4/SPI2_MOSI/I2S2_SD,_USART2_RTS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "85"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -55.88 180)
				(length 7.62)
				(name "PD5/USART2_TX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "86"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -58.42 180)
				(length 7.62)
				(name "PD6/SPI2_NSS/I2S2_WS,_USART2_RX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "87"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -60.96 180)
				(length 7.62)
				(name "PD7/SPI2_SCK/I2S2_CK,_USART2_CK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "88"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -66.04 180)
				(length 7.62)
				(name "PE0/USART1_TX,_TIM4_ETR_"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "97"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -68.58 180)
				(length 7.62)
				(name "PE1/USART1_RX_"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "98"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -71.12 180)
				(length 7.62)
				(name "PE2/TSC_G7_IO1,_TRACECLK_"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -73.66 180)
				(length 7.62)
				(name "PE3/TSC_G7_IO2,_TRACED0_"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -76.2 180)
				(length 7.62)
				(name "PE4/TSC_G7_IO3,_TRACED1_"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -78.74 180)
				(length 7.62)
				(name "PE5/TSC_G7_IO4,_TRACED2_"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 223.52 -81.28 180)
				(length 7.62)
				(name "PE6/TRACED3_WKUP3,_RTC_TAMPER3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "STM32F373VxT_2_1"
			(rectangle
				(start 7.62 -60.96)
				(end 144.78 5.08)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin bidirectional line
				(at 0 0 0)
				(length 7.62)
				(name "PB0/SPI1_MOSI/I2S1_SD,_TIM3_CH3,_TSC_G3_IO3,_TIM3_CH2_ADC_IN8,_SDADC1_AIN6P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -2.54 0)
				(length 7.62)
				(name "PB1/TIM3_CH4,_TSC_G3_IO4_ADC_IN9,_SDADC1_AIN5P,_SDADC1_AIN6M"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -5.08 0)
				(length 7.62)
				(name "PB2/SDADC1_AIN4P,_SDADC2_AIN6P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -7.62 0)
				(length 7.62)
				(name "PE7/SDADC1_AIN3P,_SDADC1_AIN4M,_SDADC2_AIN5P,_SDADC2_AIN6M"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -10.16 0)
				(length 7.62)
				(name "PE8/SDADC1_AIN8P,_SDADC2_AIN8P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -12.7 0)
				(length 7.62)
				(name "PE9/SDADC1_AIN7P,_SDADC1_AIN8M,_SDADC2_AIN7P,_SDADC2_AIN8M"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -15.24 0)
				(length 7.62)
				(name "PE10/SDADC1_AIN2P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -17.78 0)
				(length 7.62)
				(name "PE11/SDADC1_AIN1P,_SDADC1_AIN2M,_SDADC2_AIN4P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -20.32 0)
				(length 7.62)
				(name "PE12/SDADC1_AIN0P,_SDADC2_AIN3P,_SDADC2_AIN4M"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -22.86 0)
				(length 7.62)
				(name "PE13/SDADC1_AIN0M_,_SDADC2_AIN2P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -25.4 0)
				(length 7.62)
				(name "PE14/SDADC2_AIN1P,_SDADC2_AIN2M"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -27.94 0)
				(length 7.62)
				(name "PE15/USART3_RX_SDADC2_AIN0P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -30.48 0)
				(length 7.62)
				(name "PB10/SPI2_SCK/I2S2_CK,_USART3_TX,_CEC,_TSC_SYNC,_TIM2_CH3_SDADC2_AIN0M"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -33.02 0)
				(length 7.62)
				(name "PB14/SPI2_MISO/I2S2_MCK,_USART3_RTS,_TIM15_CH1,_TIM12_CH1,_TSC_G6_IO1_SDADC3_AIN8P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "53"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -35.56 0)
				(length 7.62)
				(name "PB15/SPI2_MOSI/I2S2_SD,_TIM15_CH1N,_TIM15_CH2,_TIM12_CH2,_TSC_G6_IO2,_RTC_REFIN_SDADC3_AIN7P,_SDADC3_AIN8M"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "54"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -38.1 0)
				(length 7.62)
				(name "PD8/SPI2_SCK/I2S2_CK,_USART3_TX,_TSC_G6_IO3_SDADC3_AIN6P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "55"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -40.64 0)
				(length 7.62)
				(name "PD9/USART3_RX,_TSC_G6_IO4_SDADC3_AIN5P,_SDADC3_AIN6M"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "56"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -43.18 0)
				(length 7.62)
				(name "PD10/USART3_CK_SDADC3_AIN4P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "57"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -45.72 0)
				(length 7.62)
				(name "PD11/USART3_CTS_SDADC3_AIN3P,_SDADC3_AIN4M"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "58"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -48.26 0)
				(length 7.62)
				(name "PD12/USART3_RTS,_TIM4_CH1,_TSC_G8_IO1_SDADC3_AIN2P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "59"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -50.8 0)
				(length 7.62)
				(name "PD13/TIM4_CH2,_TSC_G8_IO2_SDADC3_AIN1P,_SDADC3_AIN2M"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "60"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -53.34 0)
				(length 7.62)
				(name "PD14/TIM4_CH3,_TSC_G8_IO3_SDADC3_AIN0P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "61"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -55.88 0)
				(length 7.62)
				(name "PD15/TIM4_CH4,_TSC_G8_IO4_SDADC3_AIN0M"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "62"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "STM32F373VxT_3_1"
			(rectangle
				(start 7.62 -35.56)
				(end 35.56 5.08)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin power_in line
				(at 0 0 0)
				(length 7.62)
				(name "VSS_1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "99"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -2.54 0)
				(length 7.62)
				(name "VSS_3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "74"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -7.62 0)
				(length 7.62)
				(name "VSSSD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "49"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -12.7 0)
				(length 7.62)
				(name "VSSA/VREF-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -17.78 0)
				(length 7.62)
				(name "VBAT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 43.18 0 180)
				(length 7.62)
				(name "VDD_1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "100"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 43.18 -2.54 180)
				(length 7.62)
				(name "VDD_2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 43.18 -5.08 180)
				(length 7.62)
				(name "VDD_3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "75"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 43.18 -10.16 180)
				(length 7.62)
				(name "VDDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 43.18 -15.24 180)
				(length 7.62)
				(name "VDDSD3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "51"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 43.18 -17.78 180)
				(length 7.62)
				(name "VDDSD12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "50"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 43.18 -22.86 180)
				(length 7.62)
				(name "VREFSD+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "52"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 43.18 -25.4 180)
				(length 7.62)
				(name "VREFSD-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 43.18 -30.48 180)
				(length 7.62)
				(name "VREF+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F401RETx"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -55.88 48.895 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "STM32F401RETx"
			(at 55.88 48.895 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right bottom)
			)
		)
		(property "Footprint" "LQFP64"
			(at 38.1 50.8 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right top)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f401re.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "STM32F401RETx_0_1"
			(rectangle
				(start -55.88 -46.99)
				(end 55.88 48.26)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(symbol "STM32F401RETx_1_1"
			(pin bidirectional line
				(at -59.69 40.64 0)
				(length 3.81)
				(name "PA0/USART2_CTS/TIM2_CH1/TIM2_ETR/TIM5_CH1/ADC1_IN0/WKUP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 38.1 0)
				(length 3.81)
				(name "PA1/USART2_RTS/TIM2_CH2/TIM5_CH2/ADC1_IN1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 35.56 0)
				(length 3.81)
				(name "PA2/USART2_TX/TIM2_CH3/TIM5_CH3/TIM9_CH1/ADC1_IN2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 33.02 0)
				(length 3.81)
				(name "PA3/USART2_RX/TIM2_CH4/TIM5_CH4/TIM9_CH2/ADC1_IN3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 30.48 0)
				(length 3.81)
				(name "PA4/SPI1_NSS/SPI3_NSS/I2S3_WS/USART2_CK/ADC1_IN4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 27.94 0)
				(length 3.81)
				(name "PA5/SPI1_SCK/TIM2_CH1/TIM2_ETR/ADC1_IN5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 25.4 0)
				(length 3.81)
				(name "PA6/SPI1_MISO/TIM1_BKIN/TIM3_CH1/ADC1_IN6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 22.86 0)
				(length 3.81)
				(name "PA7/SPI1_MOSI/TIM1_CH1N/TIM3_CH2/ADC1_IN7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 20.32 0)
				(length 3.81)
				(name "PA8/I2C3_SCL/USART1_CK/TIM1_CH1/OTG_FS_SOF/MCO_1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 17.78 0)
				(length 3.81)
				(name "PA9/I2C3_SMBA/USART1_TX/TIM1_CH2/OTG_FS_VBUS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 15.24 0)
				(length 3.81)
				(name "PA10/USART1_RX/TIM1_CH3/OTG_FS_ID"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 12.7 0)
				(length 3.81)
				(name "PA11/USART1_CTS/USART6_TX/TIM1_CH4/OTG_FS_DM"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 10.16 0)
				(length 3.81)
				(name "PA12/USART1_RTS/USART6_RX/TIM1_ETR/OTG_FS_DP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 7.62 0)
				(length 3.81)
				(name "PA13/JTMS-SWDIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 5.08 0)
				(length 3.81)
				(name "PA14/JTCK-SWCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "49"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 2.54 0)
				(length 3.81)
				(name "PA15/JTDI/SPI1_NSS/SPI3_NSS/I2S3_WS/TIM2_CH1/TIM2_ETR/JTDI"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "50"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 -2.54 0)
				(length 3.81)
				(name "PB0/TIM1_CH2N/TIM3_CH3/ADC1_IN8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 -5.08 0)
				(length 3.81)
				(name "PB1/TIM1_CH3N/TIM3_CH4/ADC1_IN9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 -7.62 0)
				(length 3.81)
				(name "PB2/BOOT1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 -10.16 0)
				(length 3.81)
				(name "PB3/JTDO-SWO/SPI1_SCK/SPI3_SCK/I2S3_CK/I2C2_SDA/TIM2_CH2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "55"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 -12.7 0)
				(length 3.81)
				(name "PB4/NJTRST/SPI1_MISO/SPI3_MISO/I2S3ext_SD/I2C3_SDA/TIM3_CH1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "56"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 -15.24 0)
				(length 3.81)
				(name "PB5/SPI1_MOSI/SPI3_MOSI/I2S3_SD/I2C1_SMBA/TIM3_CH2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "57"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 -17.78 0)
				(length 3.81)
				(name "PB6/I2C1_SCL/USART1_TX/TIM4_CH1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "58"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 -20.32 0)
				(length 3.81)
				(name "PB7/I2C1_SDA/USART1_RX/TIM4_CH2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "59"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 -22.86 0)
				(length 3.81)
				(name "PB8/I2C1_SCL/TIM4_CH3/TIM10_CH1/SDIO_D4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "61"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 -25.4 0)
				(length 3.81)
				(name "PB9/SPI2_NSS/I2S2_WS/I2C1_SDA/TIM4_CH4/TIM11_CH1/SDIO_D5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "62"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 -27.94 0)
				(length 3.81)
				(name "PB10/SPI2_SCK/I2S2_CK/I2C2_SCL/TIM2_CH3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 -33.02 0)
				(length 3.81)
				(name "PB12/SPI2_NSS/I2S2_WS/I2C2_SMBA/TIM1_BKIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 -35.56 0)
				(length 3.81)
				(name "PB13/SPI2_SCK/I2S2_CK/TIM1_CH1N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 -38.1 0)
				(length 3.81)
				(name "PB14/SPI2_MISO/I2S2ext_SD/TIM1_CH2N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -59.69 -40.64 0)
				(length 3.81)
				(name "PB15/SPI2_MOSI/I2S2_SD/TIM1_CH3N/RTC_REFIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -2.54 52.07 270)
				(length 3.81)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "64"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 3.81)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "63"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 52.07 270)
				(length 3.81)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 3.81)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 52.07 270)
				(length 3.81)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 3.81)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 5.08 52.07 270)
				(length 3.81)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 5.08 -50.8 90)
				(length 3.81)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin unspecified line
				(at 30.48 -50.8 90)
				(length 3.81)
				(name "VCAP_1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 59.69 40.64 180)
				(length 3.81)
				(name "PC0/ADC1_IN10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 59.69 38.1 180)
				(length 3.81)
				(name "PC1/ADC1_IN11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 59.69 35.56 180)
				(length 3.81)
				(name "PC2/SPI2_MISO/I2S2ext_SD/ADC1_IN12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 59.69 33.02 180)
				(length 3.81)
				(name "PC3/SPI2_MOSI/I2S2_SD/ADC1_IN13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 59.69 30.48 180)
				(length 3.81)
				(name "PC4/ADC1_IN14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 59.69 27.94 180)
				(length 3.81)
				(name "PC5/ADC1_IN15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 59.69 25.4 180)
				(length 3.81)
				(name "PC6/I2S2_MCK/USART6_TX/TIM3_CH1/SDIO_D6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 59.69 22.86 180)
				(length 3.81)
				(name "PC7/I2S3_MCK/USART6_RX/TIM3_CH2/SDIO_D7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 59.69 20.32 180)
				(length 3.81)
				(name "PC8/USART6_CK/TIM3_CH3/SDIO_D0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 59.69 17.78 180)
				(length 3.81)
				(name "PC9/I2S_CKIN/I2C3_SDA/TIM3_CH4/SDIO_D1/MCO_2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 59.69 15.24 180)
				(length 3.81)
				(name "PC10/SPI3_SCK/I2S3_CK/SDIO_D2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "51"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 59.69 12.7 180)
				(length 3.81)
				(name "PC11/I2S3ext_SD/SPI3_MISO/SDIO_D3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "52"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 59.69 10.16 180)
				(length 3.81)
				(name "PC12/SPI3_MOSI/I2S3_SD/SDIO_CK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "53"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 59.69 7.62 180)
				(length 3.81)
				(name "PC13/RTC_TAMP1/RTC_OUT/RTC_TS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 59.69 5.08 180)
				(length 3.81)
				(name "PC14/OSC32_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 59.69 2.54 180)
				(length 3.81)
				(name "PC15/OSC32_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 59.69 -2.54 180)
				(length 3.81)
				(name "PD2/TIM3_ETR/SDIO_CMD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "54"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 59.69 -7.62 180)
				(length 3.81)
				(name "PH0/OSC_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 59.69 -10.16 180)
				(length 3.81)
				(name "PH1/OSC_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 59.69 -17.78 180)
				(length 3.81)
				(name "BOOT0/VPP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "60"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 59.69 -22.86 180)
				(length 3.81)
				(name "NRST"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 59.69 -27.94 180)
				(length 3.81)
				(name "VBAT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 59.69 -35.56 180)
				(length 3.81)
				(name "VDDA/VREF+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 59.69 -40.64 180)
				(length 3.81)
				(name "VSSA/VREF-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F407VETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 26.67 72.39 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "STM32F407VETx"
			(at 25.4 69.85 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 74.93 -69.85 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00037051.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "ARM Cortex-M4 MCU, 512KB flash, 128KB RAM, 168MHz, 1.8-3.6V, 82 GPIO, LQFP-100"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "ARM Cortex-M4 STM32F4 STM32F407/417"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "STM32F407VETx_0_1"
			(rectangle
				(start -77.47 68.58)
				(end 77.47 -68.58)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(symbol "STM32F407VETx_1_1"
			(pin bidirectional line
				(at -80.01 58.42 0)
				(length 2.54)
				(name "PA0/USART2_CTS/UART4_TX/ETH_MII_CRS/TIM2_CH1_ETR/TIM5_CH1/TIM8_ETR/ADC123_IN0/WKUP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 55.88 0)
				(length 2.54)
				(name "PA1/USART2_RTS/UART4_RX/ETH_RMII_REF_CLK/ETH_MII_RX_CLK/TIM5_CH2/TIM2_CH2/ADC123_IN1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 53.34 0)
				(length 2.54)
				(name "PA2/USART2_TX/TIM5_CH3/TIM9_CH1/TIM2_CH3/ETH_MDIO/ADC123_IN2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 50.8 0)
				(length 2.54)
				(name "PA3/USART2_RX/TIM5_CH4/TIM9_CH2/TIM2_CH4/OTG_HS_ULPI_D0/ETH_MII_COL/ADC123_IN3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 48.26 0)
				(length 2.54)
				(name "PA4/SPI1_NSS/SPI3_NSS/USART2_CK/DCMI_HSYNC/OTG_HS_SOF/I2S3_WS/ADC12_IN4/DAC_OUT1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 45.72 0)
				(length 2.54)
				(name "PA5/SPI1_SCK/OTG_HS_ULPI_CK/TIM2_CH1_ETR/TIM8_CH1N/ADC12_IN5/DAC_OUT2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 43.18 0)
				(length 2.54)
				(name "PA6/SPI1_MISO/TIM8_BKIN/TIM13_CH1/DCMI_PIXCLK/TIM3_CH1/TIM1_BKIN/ADC12_IN6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 40.64 0)
				(length 2.54)
				(name "PA7/SPI1_MOSI/TIM8_CH1N/TIM14_CH1/TIM3_CH2/ETH_MII_RX_DV/TIM1_CH1N/ETH_RMII_CRS_DV/ADC12_IN7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 38.1 0)
				(length 2.54)
				(name "PA8/MCO1/USART1_CK/TIM1_CH1/I2C3_SCL/OTG_FS_SOF"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "67"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 35.56 0)
				(length 2.54)
				(name "PA9/USART1_TX/TIM1_CH2/I2C3_SMBA/DCMI_D0/OTG_FS_VBUS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "68"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 33.02 0)
				(length 2.54)
				(name "PA10/USART1_RX/TIM1_CH3/OTG_FS_ID/DCMI_D1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "69"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 30.48 0)
				(length 2.54)
				(name "PA11/USART1_CTS/CAN1_RX/TIM1_CH4/OTG_FS_DM"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "70"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 27.94 0)
				(length 2.54)
				(name "PA12/USART1_RTS/CAN1_TX/TIM1_ETR/OTG_FS_DP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "71"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 25.4 0)
				(length 2.54)
				(name "PA13/JTMS-SWDIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "72"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 22.86 0)
				(length 2.54)
				(name "PA14/JTCK-SWCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "76"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 20.32 0)
				(length 2.54)
				(name "PA15/JTDI/SPI3_NSS/I2S3_WS/TIM2_CH1_ETR/SPI1_NSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "77"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 15.24 0)
				(length 2.54)
				(name "PB0/TIM3_CH3/TIM8_CH2N/OTG_HS_ULPI_D1/ETH_MII_RXD2/TIM1_CH2N/ADC12_IN8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 12.7 0)
				(length 2.54)
				(name "PB1/TIM3_CH4/TIM8_CH3N/OTG_HS_ULPI_D2/ETH_MII_RXD3/TIM1_CH3N/ADC12_IN9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 10.16 0)
				(length 2.54)
				(name "PB2/BOOT1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 7.62 0)
				(length 2.54)
				(name "PB3/JTDO/TRACESWO/SPI3_SCK/I2S3_CK/TIM2_CH2/SPI1_SCK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "89"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 5.08 0)
				(length 2.54)
				(name "PB4/NJTRST/SPI3_MISO/TIM3_CH1/SPI1_MISO/I2S3ext_SD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "90"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 2.54 0)
				(length 2.54)
				(name "PB5/I2C1_SMBA/CAN2_RX/OTG_HS_ULPI_D7/ETH_PPS_OUT/TIM3_CH2/SPI1_MOSI/SPI3_MOSI/DCMI_D10/I2S3_SD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "91"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 0 0)
				(length 2.54)
				(name "PB6/I2C1_SCL/TIM4_CH1/CAN2_TX/DCMI_D5/USART1_TX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "92"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 -2.54 0)
				(length 2.54)
				(name "PB7/I2C1_SDA/FSMC_NL/DCMI_VSYNC/USART1_RX/TIM4_CH2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "93"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 -5.08 0)
				(length 2.54)
				(name "PB8/TIM4_CH3/SDIO_D4/TIM10_CH1/DCMI_D6/ETH_MII_TXD3/I2C1_SCL/CAN1_RX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "95"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 -7.62 0)
				(length 2.54)
				(name "PB9/SPI2_NSS/I2S2_WS/TIM4_CH4/TIM11_CH1/SDIO_D5/DCMI_D7/I2C1_SDA/CAN1_TX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "96"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 -10.16 0)
				(length 2.54)
				(name "PB10/SPI2_SCK/I2S2_CK/I2C2_SCL/USART3_TX/OTG_HS_ULPI_D3/ETH_MII_RX_ER/TIM2_CH3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 -12.7 0)
				(length 2.54)
				(name "PB11/I2C2_SDA/USART3_RX/OTG_HS_ULPI_D4/ETH_RMII_TX_EN/ETH_MII_TX_EN/TIM2_CH4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 -15.24 0)
				(length 2.54)
				(name "PB12/SPI2_NSS/I2S2_WS/I2C2_SMBA/USART3_CK/TIM1_BKIN/CAN2_RX/OTG_HS_ULPI_D5/ETH_RMII_TXD0/ETH_MII_TXD0/OTG_HS_ID"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "51"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 -17.78 0)
				(length 2.54)
				(name "PB13/SPI2_SCK/I2S2_CK/USART3_CTS/TIM1_CH1N/CAN2_TX/OTG_HS_ULPI_D6/ETH_RMII_TXD1/ETH_MII_TXD1/OTG_HS_VBUS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "52"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 -20.32 0)
				(length 2.54)
				(name "PB14/SPI2_MISO/TIM1_CH2N/TIM12_CH1/OTG_HS_DM/USART3_RTS/TIM8_CH2N/I2S2ext_SD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "53"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 -22.86 0)
				(length 2.54)
				(name "PB15/SPI2_MOSI/I2S2_SD/TIM1_CH3N/TIM8_CH3N/TIM12_CH2/OTG_HS_DP/RTC_REFIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "54"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 -27.94 0)
				(length 2.54)
				(name "PC0/OTG_HS_ULPI_STP/ADC123_IN10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 -30.48 0)
				(length 2.54)
				(name "PC1/ETH_MDC/ADC123_IN11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 -33.02 0)
				(length 2.54)
				(name "PC2/SPI2_MISO/OTG_HS_ULPI_DIR/ETH_MII_TXD2/I2S2ext_SD/ADC123_IN12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 -35.56 0)
				(length 2.54)
				(name "PC3/SPI2_MOSI/I2S2_SD/OTG_HS_ULPI_NXT/ETH_MII_TX_CLK/ADC123_IN13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 -38.1 0)
				(length 2.54)
				(name "PC4/ETH_RMII_RX_D0/ETH_MII_RX_D0/ADC12_IN14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 -40.64 0)
				(length 2.54)
				(name "PC5/ETH_RMII_RX_D1/ETH_MII_RX_D1/ADC12_IN15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 -43.18 0)
				(length 2.54)
				(name "PC6/I2S2_MCK/TIM8_CH1/SDIO_D6/USART6_TX/DCMI_D0/TIM3_CH1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "63"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 -45.72 0)
				(length 2.54)
				(name "PC7/I2S3_MCK/TIM8_CH2/SDIO_D7/USART6_RX/DCMI_D1/TIM3_CH2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "64"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 -48.26 0)
				(length 2.54)
				(name "PC8/TIM8_CH3/SDIO_D0/TIM3_CH3/USART6_CK/DCMI_D2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "65"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 -50.8 0)
				(length 2.54)
				(name "PC9/I2S_CKIN/MCO2/TIM8_CH4/SDIO_D1//I2C3_SDA/DCMI_D3/TIM3_CH4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "66"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 -53.34 0)
				(length 2.54)
				(name "PC10/SPI3_SCK/I2S3_CK/UART4_TX/SDIO_D2/DCMI_D8/USART3_TX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "78"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 -55.88 0)
				(length 2.54)
				(name "PC11/UART4_RX/SPI3_MISO/SDIO_D3/DCMI_D4/USART3_RX/I2S3ext_SD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "79"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 -58.42 0)
				(length 2.54)
				(name "PC12/UART5_TX/SDIO_CK/DCMI_D9/SPI3_MOSI/I2S3_SD/USART3_CK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "80"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 -60.96 0)
				(length 2.54)
				(name "PC13/RTC_OUT/RTC_TAMP1/RTC_TS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 -63.5 0)
				(length 2.54)
				(name "PC14/OSC32_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -80.01 -66.04 0)
				(length 2.54)
				(name "PC15/OSC32_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at -29.21 -71.12 90)
				(length 2.54)
				(name "VCAP_1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "49"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at -21.59 -71.12 90)
				(length 2.54)
				(name "VCAP_2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "73"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -8.89 71.12 270)
				(length 2.54)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -6.35 71.12 270)
				(length 2.54)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -3.81 71.12 270)
				(length 2.54)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -2.54 -71.12 90)
				(length 2.54)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "99"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -1.27 71.12 270)
				(length 2.54)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "50"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 2.54)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "74"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 1.27 71.12 270)
				(length 2.54)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "75"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 2.54)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 3.81 71.12 270)
				(length 2.54)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "100"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 5.08 -71.12 90)
				(length 2.54)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 58.42 180)
				(length 2.54)
				(name "PD0/FSMC_D2/CAN1_RX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "81"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 55.88 180)
				(length 2.54)
				(name "PD1/FSMC_D3/CAN1_TX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "82"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 53.34 180)
				(length 2.54)
				(name "PD2/TIM3_ETR/UART5_RX/SDIO_CMD/DCMI_D11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "83"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 50.8 180)
				(length 2.54)
				(name "PD3/FSMC_CLK/USART2_CTS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "84"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 48.26 180)
				(length 2.54)
				(name "PD4/FSMC_NOE/USART2_RTS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "85"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 45.72 180)
				(length 2.54)
				(name "PD5/FSMC_NWE/USART2_TX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "86"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 43.18 180)
				(length 2.54)
				(name "PD6/FSMC_NWAIT/USART2_RX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "87"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 40.64 180)
				(length 2.54)
				(name "PD7/USART2_CK/FSMC_NE1/FSMC_NCE2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "88"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 38.1 180)
				(length 2.54)
				(name "PD8/FSMC_D13/USART3_TX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "55"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 35.56 180)
				(length 2.54)
				(name "PD9/FSMC_D14/USART3_RX"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "56"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 33.02 180)
				(length 2.54)
				(name "PD10/FSMC_D15/USART3_CK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "57"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 30.48 180)
				(length 2.54)
				(name "PD11/FSMC_CLE/FSMC_A16/USART3_CTS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "58"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 27.94 180)
				(length 2.54)
				(name "PD12/FSMC_ALE/FSMC_A17/TIM4_CH1/USART3_RTS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "59"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 25.4 180)
				(length 2.54)
				(name "PD13/FSMC_A18/TIM4_CH2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "60"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 22.86 180)
				(length 2.54)
				(name "PD14/FSMC_D0/TIM4_CH3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "61"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 20.32 180)
				(length 2.54)
				(name "PD15/FSMC_D1/TIM4_CH4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "62"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 15.24 180)
				(length 2.54)
				(name "PE0/TIM4_ETR/FSMC_NBL0/DCMI_D2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "97"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 12.7 180)
				(length 2.54)
				(name "PE1/FSMC_NBL1/DCMI_D3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "98"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 10.16 180)
				(length 2.54)
				(name "PE2/TRACECLK/FSMC_A23/ETH_MII_TXD3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 7.62 180)
				(length 2.54)
				(name "PE3/TRACED0/FSMC_A19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 5.08 180)
				(length 2.54)
				(name "PE4/TRACED1/FSMC_A20/DCMI_D4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 2.54 180)
				(length 2.54)
				(name "PE5/TRACED2/FSMC_A21/TIM9_CH1/DCMI_D6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 0 180)
				(length 2.54)
				(name "PE6/TRACED3/FSMC_A22/TIM9_CH2/DCMI_D7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 -2.54 180)
				(length 2.54)
				(name "PE7/FSMC_D4/TIM1_ETR"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 -5.08 180)
				(length 2.54)
				(name "PE8/FSMC_D5/TIM1_CH1N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 -7.62 180)
				(length 2.54)
				(name "PE9/FSMC_D6/TIM1_CH1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 -10.16 180)
				(length 2.54)
				(name "PE10/FSMC_D7/TIM1_CH2N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 -12.7 180)
				(length 2.54)
				(name "PE11/FSMC_D8/TIM1_CH2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 -15.24 180)
				(length 2.54)
				(name "PE12/FSMC_D9/TIM1_CH3N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 -17.78 180)
				(length 2.54)
				(name "PE13/FSMC_D10/TIM1_CH3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 -20.32 180)
				(length 2.54)
				(name "PE14/FSMC_D11/TIM1_CH4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 -22.86 180)
				(length 2.54)
				(name "PE15/FSMC_D12/TIM1_BKIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 -30.48 180)
				(length 2.54)
				(name "PH0/OSC_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 -33.02 180)
				(length 2.54)
				(name "PH1/OSC_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 80.01 -38.1 180)
				(length 2.54)
				(name "BOOT0/VPP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "94"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 80.01 -40.64 180)
				(length 2.54)
				(name "NRST/RST"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 80.01 -45.72 180)
				(length 2.54)
				(name "VBAT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 80.01 -50.8 180)
				(length 2.54)
				(name "VREF+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 80.01 -55.88 180)
				(length 2.54)
				(name "VDDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 80.01 -63.5 180)
				(length 2.54)
				(name "VSSA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCA505BG"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 36.83 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "TCA505BG"
			(at -3.81 39.37 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SOIC127P600-16N"
			(at -5.08 -10.16 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Part_Number" "TCA505BG"
			(at -5.08 -12.7 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Note" "*"
			(at -5.08 -15.24 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Package" "SO-16"
			(at -5.08 -17.78 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -5.08 -20.32 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -5.08 -22.86 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Manufacturer" "Infineon"
			(at -5.08 -25.4 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(symbol "TCA505BG_1_1"
			(rectangle
				(start 0 0)
				(end 68.58 30.48)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 5.08)
				(name "NC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 5.08)
				(name "VREF"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 5.08)
				(name "B"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 -5.08 90)
				(length 5.08)
				(name "LC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 20.32 -5.08 90)
				(length 5.08)
				(name "RDI"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 30.48 -5.08 90)
				(length 5.08)
				(name "RHY"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 33.02 35.56 270)
				(length 5.08)
				(name "VT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 40.64 -5.08 90)
				(length 5.08)
				(name "CI"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 43.18 35.56 270)
				(length 5.08)
				(name "VS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 53.34 -5.08 90)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 58.42 35.56 270)
				(length 5.08)
				(name "SC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 63.5 -5.08 90)
				(length 5.08)
				(name "CD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 73.66 25.4 180)
				(length 5.08)
				(name "Q1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 73.66 20.32 180)
				(length 5.08)
				(name "Q2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 73.66 15.24 180)
				(length 5.08)
				(name "Q3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 73.66 10.16 180)
				(length 5.08)
				(name "Q4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "TL072ID"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U9"
			(at -5.08 6.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "TL072ID"
			(at -3.81 8.89 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SOIC127P600-8M"
			(at -5.08 -20.32 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Low-Noise J-FET Dual Operational Amplifier"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "user" "B"
			(at 3.048 -6.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Package" "SO-8"
			(at -5.08 -27.94 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -5.08 -33.02 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -5.08 -35.56 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "user_1" "A"
			(at 3.048 -6.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Part_Number" "TL072ID"
			(at -5.08 -40.64 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Comment" "TL072ID"
			(at -1.27 6.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(symbol "TL072ID_0_1"
			(pin power_in line
				(at 5.08 5.08 270)
				(length 5.08)
				(name "V+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 5.08)
				(name "V-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "TL072ID_1_1"
			(polyline
				(pts
					(xy 0 0) (xy 0 -10.16)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 10.16 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -10.16) (xy 10.16 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.016 -2.54) (xy 2.54 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.016 -7.62) (xy 2.54 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.778 -6.858) (xy 1.778 -8.382)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 0) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -7.62) (xy 5.08 -10.16)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(pin input line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "IN-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 -7.62 0)
				(length 5.08)
				(name "IN+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "TL072ID_2_1"
			(polyline
				(pts
					(xy 0 0) (xy 0 -10.16)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 10.16 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -10.16) (xy 10.16 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.016 -2.54) (xy 2.54 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.016 -7.62) (xy 2.54 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.778 -6.858) (xy 1.778 -8.382)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 0) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -7.62) (xy 5.08 -10.16)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(pin input line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "IN-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 -7.62 0)
				(length 5.08)
				(name "IN+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP172G"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "TLP172G"
			(at -3.81 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SOP2.54-4"
			(at -5.08 -17.78 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "HEXFET Power MOSFET"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -5.08 -20.32 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -5.08 -22.86 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Package" "SOP2.54-4"
			(at -5.08 -25.4 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Part_Number" "TLP172G"
			(at -5.08 -27.94 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Note" "*"
			(at -5.08 -30.48 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Manufacturer" "TOSHIBA"
			(at -5.08 -33.02 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Created" "5/07/2006"
			(at -5.08 -35.56 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(symbol "TLP172G_1_1"
			(polyline
				(pts
					(xy 0 -2.54) (xy 2.54 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -10.16) (xy 2.54 -10.16)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start 0 -12.7)
				(end 10.16 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 1.778 -6.858) (xy 3.302 -6.858)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -2.54) (xy 2.54 -5.588)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -6.858) (xy 1.778 -5.588) (xy 3.302 -5.588) (xy 2.54 -6.858)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 2.54 -10.16) (xy 2.54 -6.858)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -6.604) (xy 6.096 -4.572)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -6.604) (xy 4.826 -5.842) (xy 4.064 -7.112)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 6.604 -8.636) (xy 6.604 -4.064)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.366 -4.064) (xy 6.604 -4.064)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.366 -5.334) (xy 7.366 -2.794)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.366 -7.366) (xy 7.366 -9.906)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.366 -8.636) (xy 6.604 -8.636)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.874 -2.794) (xy 7.874 -3.302)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.874 -3.048) (xy 8.636 -3.048)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.874 -3.81) (xy 7.874 -4.318)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.874 -4.064) (xy 8.382 -4.572) (xy 8.382 -3.556) (xy 7.874 -4.064)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 7.874 -4.826) (xy 7.874 -5.334)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.874 -5.08) (xy 8.636 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.874 -7.62) (xy 8.636 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.874 -7.874) (xy 7.874 -7.366)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.874 -8.636) (xy 8.382 -8.128) (xy 8.382 -9.144) (xy 7.874 -8.636)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 7.874 -8.89) (xy 7.874 -8.382)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.874 -9.652) (xy 8.636 -9.652)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.874 -9.906) (xy 7.874 -9.398)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 8.636 -2.54) (xy 10.16 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 8.636 -3.048) (xy 8.636 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 8.636 -4.064) (xy 7.874 -4.064)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 8.636 -5.08) (xy 8.636 -4.064)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 8.636 -5.08) (xy 8.636 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 8.636 -5.08)
				(radius 0.0001)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 8.636 -7.62) (xy 8.636 -8.636)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 8.636 -7.62)
				(radius 0.0001)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 8.636 -8.636) (xy 7.874 -8.636)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 8.636 -9.652) (xy 8.636 -10.16)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 8.636 -10.16) (xy 10.16 -10.16)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 8.89 -3.81) (xy 9.906 -3.81)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 8.89 -4.572) (xy 9.906 -4.572) (xy 9.398 -3.81) (xy 8.89 -4.572)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 8.89 -8.128) (xy 9.906 -8.128) (xy 9.398 -8.89) (xy 8.89 -8.128)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 8.89 -8.89) (xy 9.906 -8.89)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 9.398 -3.81) (xy 9.398 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 9.398 -4.572) (xy 9.398 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 9.398 -5.08) (xy 8.636 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 9.398 -7.62) (xy 8.636 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 9.398 -8.128) (xy 9.398 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 9.398 -8.89) (xy 9.398 -10.16)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "Anode"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 5.08)
				(name "Cathone"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "Drain"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 15.24 -10.16 180)
				(length 5.08)
				(name "Drain"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP2362"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "TLP2362"
			(at -3.81 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SOP2.54-5"
			(at -5.08 -16.51 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "5-Pin Phototransistor Optocoupler,High Speed 10Mb/s, High CMR"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Part_Number" "TLP2362"
			(at -5.08 -21.59 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Package" "SOP1.27-5"
			(at -5.08 -24.13 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -5.08 -29.21 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -5.08 -31.75 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Comment" "TLP2362"
			(at -1.27 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(symbol "TLP2362_1_1"
			(polyline
				(pts
					(xy 0 -1.016) (xy 0 -11.43)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -1.016) (xy 15.24 -1.016)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 2.54 -2.54)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -10.16) (xy 2.54 -10.16)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -11.43) (xy 15.24 -11.43)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.016 -5.08) (xy 4.064 -5.08) (xy 2.54 -7.112) (xy 1.016 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 2.54 -2.54) (xy 2.54 -10.16)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 4.064 -7.366) (xy 4.064 -7.62) (xy 1.016 -7.62) (xy 1.016 -7.366) (xy 4.064 -7.366)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 6.604 -6.604) (xy 6.604 -7.112) (xy 6.096 -7.112) (xy 6.604 -6.604)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 6.604 -7.112) (xy 5.08 -5.588)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 6.604 -7.874) (xy 6.604 -8.382) (xy 6.096 -8.382) (xy 6.604 -7.874)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 6.604 -8.382) (xy 5.08 -6.858)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 11.43 -7.62) (xy 12.7 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 11.43 -7.62) (xy 7.62 -5.08) (xy 7.62 -10.16) (xy 11.43 -7.62)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 12.7 -5.842) (xy 12.446 -5.842) (xy 12.446 -9.398) (xy 12.7 -9.398) (xy 12.7 -5.842)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 12.7 -8.382) (xy 14.478 -10.16)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 14.224 -5.08) (xy 12.7 -6.604)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 14.224 -5.08) (xy 15.24 -5.08)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 14.224 -9.144) (xy 14.224 -9.906) (xy 13.462 -9.906) (xy 14.224 -9.144)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 14.478 -10.16) (xy 15.24 -10.16)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 15.24 -1.016) (xy 15.24 -11.43)
				)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "A"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 5.08)
				(name "K"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "VCC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "Vo"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV803SDBZR"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "TLV803SDBZR"
			(at -3.81 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SOT23-3N"
			(at -5.08 -20.32 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "ON Semiconductor"
			(at -5.08 -22.86 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Part_Number" "TLV803SDBZR"
			(at -5.08 -25.4 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet Link" "http://www.onsemi.com/pub/Collateral/MAX809S-D.PDF"
			(at -5.08 -30.48 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Geometry.Height" "1.11mm"
			(at -5.08 -33.02 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Package" "SOT-23"
			(at -5.08 -35.56 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Comment" "TLV803SDBZR"
			(at -1.27 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(symbol "TLV803SDBZR_1_1"
			(rectangle
				(start 0 -10.16)
				(end 20.32 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin power_in line
				(at -5.08 -5.08 0)
				(length 5.08)
				(name "VCC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 10.16 -15.24 90)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "RESET"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS54331DR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "TPS54331DR"
			(at 3.81 8.89 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 22.86 -8.89 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps54331.pdf"
			(at 25.4 -11.43 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "3.5V to 28V Input, 3A, Synchronous Step-Down Converter with Eco-mode(tm)"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Step-Down DC-DC Switching Regulator"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "SO*8"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "TPS54331DR_1_1"
			(rectangle
				(start -10.16 7.62)
				(end 10.16 -7.62)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "EN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "COMP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "BOOT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "PH"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VSENSE"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS61040DDC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "TPS61040DDC"
			(at 0 6.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 2.54 -6.35 0)
			(effects
				(font
					(size 1.27 1.27)
					(italic yes)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61040.pdf"
			(at -5.08 7.62 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Synchronous Boost Regulator, Adjustable Output up to 28V, SOT-23-5"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Step-Up Boost DC-DC Regulator Adjustable"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "TPS61040DDC_0_1"
			(rectangle
				(start -5.08 5.08)
				(end 5.08 -5.08)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(symbol "TPS61040DDC_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SW"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "FB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS61071DDC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "TPS61071DDC"
			(at 0 6.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 2.54 -6.35 0)
			(effects
				(font
					(size 1.27 1.27)
					(italic yes)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.ti.com/cn/lit/ds/symlink/tps61071.pdf"
			(at -5.08 7.62 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "具有 600mA 开关的 90% 高效同步升压转换器"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Step-Up Boost DC-DC Regulator Adjustable"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "TPS61071DDC_0_0"
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VOUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "TPS61071DDC_0_1"
			(rectangle
				(start -5.08 5.08)
				(end 5.08 -5.08)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(symbol "TPS61071DDC_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VBAT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SW"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "FB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "URA_ZP-6W"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 19.05 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "URA_ZP-6W"
			(at -3.81 21.59 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "Mornsun-ZP-A"
			(at -5.08 -5.1054 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Package" "SIP"
			(at -5.08 -12.7254 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "插件"
			(at -5.08 -17.8054 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -5.08 -20.3454 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Price" "13"
			(at -5.08 -22.8854 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Part_Number" "URA2415ZP-6WR3"
			(at -5.08 -25.4254 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(symbol "URA_ZP-6W_1_1"
			(rectangle
				(start 0 0)
				(end 7.62 17.78)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(rectangle
				(start 8.382 0.254)
				(end 9.398 17.526)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(rectangle
				(start 10.16 0)
				(end 17.78 17.78)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 5.08)
				(name "Vin"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 5.08)
				(name "Vin"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "+Vo"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "0V"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "0V"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "-Vo"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "URB_YMD-6WR3"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 1.27 0)
			(effects
				(font
					(size 1.524 1.524)
				)
				(justify left bottom)
			)
		)
		(property "Value" "URB_YMD-6WR3"
			(at 7.62 -16.51 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "URB_YMD-6WR3_0_1"
			(rectangle
				(start 0 -15.24)
				(end 15.24 0)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 7.62 -0.635) (xy 7.62 -2.54)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.62 -3.175) (xy 7.62 -5.08)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.62 -5.715) (xy 7.62 -7.62)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.62 -8.255) (xy 7.62 -10.16)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.62 -10.795) (xy 7.62 -12.7)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.62 -13.335) (xy 7.62 -14.605)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(pin input line
				(at -2.54 -2.54 0)
				(length 2.54)
				(name "VIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -2.54 -12.7 0)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "+VO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "0V"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "VN5160S-E"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 1.27 0)
			(effects
				(font
					(size 1.397 1.397)
				)
				(justify left bottom)
			)
		)
		(property "Value" "VN5160S-E"
			(at -3.81 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "SOIC127P600-8N"
			(at -5.08 -17.78 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Part_Number" "VN5160STR-E"
			(at -5.08 -20.32 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Package" "SO-8"
			(at -5.08 -22.86 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Note" "*"
			(at -5.08 -25.4 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Manufacturer" "ST"
			(at -5.08 -27.94 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Mount" "贴片"
			(at -5.08 -30.48 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Type" "IC"
			(at -5.08 -33.02 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(symbol "VN5160S-E_1_1"
			(rectangle
				(start 0 -12.7)
				(end 20.32 0)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin input line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "STAT_DIS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin open_collector line
				(at -5.08 -5.08 0)
				(length 5.08)
				(name "STATUS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 -7.62 0)
				(length 5.08)
				(name "IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -5.08 -10.16 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "VCC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "VCC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "VNS3NV04DPTR-E"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0.762 1.143 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "VNS3NV04DPTR-E"
			(at 10.16 -16.51 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/vns3nv04dp-e.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "OMNIFET II fully autoprotected Power MOSFET"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "fully autoprotected Power MOSFET"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "VNS3NV04DPTR-E_0_1"
			(rectangle
				(start 0 -15.24)
				(end 22.86 0)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "SOURCE1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 -5.08 0)
				(length 5.08)
				(name "INPUT1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 5.08)
				(name "SOURCE2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 -12.7 0)
				(length 5.08)
				(name "INPUT2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin open_collector line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "DRAIN1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin open_collector line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "DRAIN1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin open_collector line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "DRAIN2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin open_collector line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "DRAIN2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "VRB2405YMD-10W"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.27 8.89 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "VRB2405YMD-10W"
			(at -8.89 -10.16 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "tj_IC:MORNSUN-VRB_YMD-10W"
			(at -6.35 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.mornsun.cn/html/pdf/VRB2405YMD-10WR3.html"
			(at -6.35 -5.08 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "DC/DC input 24V,10W"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "VRB2405YMD-10W_0_1"
			(polyline
				(pts
					(xy 0 6.985) (xy 0 5.715)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 5.08) (xy 0 3.81)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 3.175) (xy 0 1.905)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 1.27) (xy 0 0)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -0.635) (xy 0 -1.905)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
		)
		(symbol "VRB2405YMD-10W_1_1"
			(rectangle
				(start -7.62 -7.62)
				(end 7.62 7.62)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -3.81)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -4.445) (xy 0 -5.715)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -6.35) (xy 0 -7.62)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "Vin"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "Ctrl"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "+Vo"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "0V"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "VRB_YMD-6W"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.27 6.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "VRB_YMD-6W"
			(at -5.08 -7.62 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "tj_IC:MORNSUN-VRB_YMD-6W"
			(at -6.35 -1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.mornsun.cn/html/pdf/VRB2405YMD-6WR3.html"
			(at -6.35 -5.08 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "DC/DC 6W"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "VRB_YMD-6W_0_1"
			(polyline
				(pts
					(xy 0 4.445) (xy 0 3.175)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 1.27)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0.635) (xy 0 -0.635)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -1.27) (xy 0 -2.54)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -3.175) (xy 0 -4.445)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
		)
		(symbol "VRB_YMD-6W_1_1"
			(rectangle
				(start -7.62 -5.08)
				(end 7.62 5.08)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "Vin"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vo"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "0V"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "W25Q32JVSS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "W25Q32JVSS"
			(at 7.62 8.89 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.23x5.23mm_P1.27mm"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.winbond.com/resource-files/w25q32jv%20revg%2003272018%20plus.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "32Mb Serial Flash Memory, Standard/Dual/Quad SPI, SOIC-8"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "flash memory SPI"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "SOIC*5.23x5.23mm*P1.27mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "W25Q32JVSS_0_1"
			(rectangle
				(start -12.7 7.62)
				(end 12.7 -10.16)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(symbol "W25Q32JVSS_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "~{CS}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "DI(IO0)"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "DO(IO1)"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "~{WP}(IO2)"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{HOLD}/~{RESET}(IO3)"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "WRA_S-3WR2"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 15.24 0)
			(effects
				(font
					(size 1.524 1.524)
				)
				(justify left bottom)
			)
		)
		(property "Value" "WRA_S-3WR2"
			(at 7.62 -2.54 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Footprint" "tj_IC:MORNSUN-S-3W"
			(at 0 0 0)
			(effects
				(font
					(size 1.524 1.524)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.mornsun.cn/html/pdf/WRA2412S-3WR2.html"
			(at 0 0 0)
			(effects
				(font
					(size 1.524 1.524)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "WRA_S-3WR2_0_1"
			(rectangle
				(start 0 0)
				(end 7.62 15.24)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(rectangle
				(start 8.382 0.254)
				(end 9.398 14.986)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(rectangle
				(start 10.16 0)
				(end 17.78 15.24)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 5.08)
				(name "Vin"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 5.08)
				(name "Ctrl"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin no_connect line
				(at 12.7 13.97 180)
				(length 5.08)
				(hide yes)
				(name "NC"
					(effects
						(font
							(size 0.0254 0.0254)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 0.0254 0.0254)
						)
					)
				)
			)
			(pin power_out line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "+Vo"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "0V"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "-Vo"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "WRB_S-3WR2"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 16.51 0)
			(effects
				(font
					(size 1.524 1.524)
				)
				(justify left bottom)
			)
		)
		(property "Value" "WRB_S-3WR2"
			(at 8.89 -1.27 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.524 1.524)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.524 1.524)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "WRB_S-3WR2_0_1"
			(rectangle
				(start 0 0)
				(end 7.62 15.24)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(rectangle
				(start 8.382 0.254)
				(end 9.398 14.986)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(rectangle
				(start 10.16 0)
				(end 17.78 15.24)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 5.08)
				(name "Vin"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 5.08)
				(name "Ctrl"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 15.24 180)
				(length 5.08)
				(hide yes)
				(name "NC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "+Vo"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "CS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "0V"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "doIoT-780E"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at 3.81 -5.08 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "doiot-780E"
			(at 0 -2.54 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "tj_IC:doiot-780E"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 17.78 5.08 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "doIoT-1X"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "doIoT-780E_1_0"
			(rectangle
				(start 0 17.78)
				(end 11.43 0)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type background)
				)
			)
			(pin power_in line
				(at -5.08 15.24 0)
				(length 5.08)
				(name "BAT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 12.7 0)
				(length 5.08)
				(name "EN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 10.16 0)
				(length 5.08)
				(name "RXD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at -5.08 7.62 0)
				(length 5.08)
				(name "TXD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -5.08 5.08 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -5.08 2.54 0)
				(length 5.08)
				(name "VCC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 16.51 15.24 180)
				(length 5.08)
				(name "BOOT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 16.51 12.7 180)
				(length 5.08)
				(name "LED"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 16.51 10.16 180)
				(length 5.08)
				(name "DN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 16.51 7.62 180)
				(length 5.08)
				(name "DP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 16.51 5.08 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 16.51 2.54 180)
				(length 5.08)
				(name "VCC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "74AHC1G08"
		(extends "74LVC1G08")
		(property "Reference" "U"
			(at -2.54 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "74AHC1G08"
			(at 6.35 -3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Single AND Gate, Low-Voltage CMOS"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Single Gate AND LVC CMOS"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
	)
	(symbol "74AHCT1G08"
		(extends "74LVC1G08")
		(property "Reference" "U"
			(at -2.54 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "74AHCT1G08"
			(at 6.35 -3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Single AND Gate, Low-Voltage CMOS"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Single Gate AND LVC CMOS"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
	)
	(symbol "74AUC1G08"
		(extends "74LVC1G08")
		(property "Reference" "U"
			(at -2.54 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "74AUC1G08"
			(at 6.35 -3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Single AND Gate, Low-Voltage CMOS"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Single Gate AND LVC CMOS"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
	)
	(symbol "74AUP1G08"
		(extends "74LVC1G08")
		(property "Reference" "U"
			(at -2.54 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "74AUP1G08"
			(at 6.35 -3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Single AND Gate, Low-Voltage CMOS"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Single Gate AND LVC CMOS"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "SOT* SG-*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
	)
	(symbol "CX7527"
		(extends "CX7527C")
		(property "Reference" "U"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "CX7527"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_SO:SOP-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "http://tj20.top:81/datasheet/CX7527X-60V_Datasheet_ReV1.0.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "高性能多模式 PWM反激式控制器,AC/DC"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "PWM,AC/DC,PWM"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
	)
	(symbol "MAX132CWG"
		(extends "MAX132CNG")
		(property "Reference" "U"
			(at 22.86 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "MAX132CWG"
			(at 25.4 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-24_W7.62mm"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.mouser.cn/datasheet/2/256/MAX132-1514523.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "Package_DIP:DIP-24_W7.62mm Package_SO:SOIC-24W_7.5x15.4mm_P1.27mm"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
	)
	(symbol "MAX13488EESA+"
		(extends "MAX13487EESA+")
		(property "Reference" "U"
			(at -6.096 11.43 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "MAX13488EESA+"
			(at 0.762 11.43 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" ""
			(at 0 -17.78 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX13487E-MAX13488E.pdf"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Half-Duplex RS-485-/RS-422-Compatible Transceiver with AutoDirection Control, SOIC-8"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Half-Duplex RS-485-/RS-422-Compatible Transceiver with AutoDirection Control, SOIC-8"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
	)
	(symbol "MT2492"
		(extends "ME3110AM6G")
		(property "Reference" "U"
			(at -0.127 -1.143 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "MT2492"
			(at 6.35 12.573 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://atta.szlcsc.com/upload/public/pdf/source/20221209/5C81DA9662873D3A116170FFBF63E49D.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "2A,4.5V-16V Input,600kHz,Synchronous Step-Down Converter"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "POWER,dcdc"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
	)
	(symbol "SP3232EEY-L_TR"
		(extends "MAX2323TSSOP")
		(property "Reference" "U"
			(at -10.16 16.51 0)
			(effects
				(font
					(size 1.143 1.143)
				)
				(justify left bottom)
			)
		)
		(property "Value" "SP3232EEY-L_TR"
			(at 3.81 -20.32 0)
			(effects
				(font
					(size 1.143 1.143)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "TSSOP16"
			(at 2.54 22.86 0)
			(effects
				(font
					(size 0.508 0.508)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.maxlinear.com/ds/sp3222e_sp3232e.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.524 1.524)
				)
				(hide yes)
			)
		)
		(property "Description" "True +3.0V to +5.5V RS-232 Transceivers"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "RS232"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "*TSSOP16* *TSSOP-16*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
	)
	(symbol "STM32F103R6T6"
		(extends "STM32F103R4T6")
		(property "Reference" "U"
			(at -48.26 46.99 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Value" "STM32F103R6T6"
			(at 1.27 0 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "LQFP64"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
	)
	(symbol "STM32F103R8T6"
		(extends "STM32F103RBT6")
		(property "Reference" "U"
			(at -48.26 46.99 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Value" "STM32F103R8T6"
			(at 1.27 0 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "LQFP64"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
	)
	(symbol "STM32F103RDT6"
		(extends "STM32F103RCT6")
		(property "Reference" "U"
			(at -48.26 48.26 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Value" "STM32F103RDT6"
			(at -27.94 48.26 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "LQFP64"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
	)
	(symbol "STM32F103RET6"
		(extends "STM32F103RCT6")
		(property "Reference" "U"
			(at -48.26 48.26 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Value" "STM32F103RET6"
			(at -27.94 48.26 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "LQFP64"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
	)
	(symbol "STM32F103RGT6"
		(extends "STM32F103RFT6")
		(property "Reference" "U"
			(at -48.26 46.99 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Value" "STM32F103RGT6"
			(at 1.27 0 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "LQFP64"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
	)
	(symbol "STM32F407VGTx"
		(extends "STM32F407VETx")
		(property "Reference" "U"
			(at 26.67 72.39 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "STM32F407VGTx"
			(at 25.4 69.85 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 74.93 -69.85 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00037051.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "ARM Cortex-M4 MCU, 1024KB flash, 128KB RAM, 168MHz, 1.8-3.6V, 82 GPIO, LQFP-100"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "ARM Cortex-M4 STM32F4 STM32F407/417"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
	)
	(symbol "TPS61040DBV"
		(extends "TPS61040DDC")
		(property "Reference" "U"
			(at -5.08 6.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "TPS61040DBV"
			(at 0 6.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 2.54 -6.35 0)
			(effects
				(font
					(size 1.27 1.27)
					(italic yes)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61040.pdf"
			(at -5.08 7.62 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Synchronous Boost Regulator, Adjustable Output up to 28V, SOT-23-5"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Step-Up Boost DC-DC Regulator Adjustable"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
	)
	(symbol "W25Q128JVS"
		(extends "W25Q32JVSS")
		(property "Reference" "U"
			(at -8.89 8.89 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "W25Q128JVS"
			(at 7.62 8.89 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.23x5.23mm_P1.27mm"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.winbond.com/resource-files/w25q128jv%20revg%2004082019%20plus.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "128Mb Serial Flash Memory, Standard/Dual/Quad SPI, SOIC-8"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "flash memory SPI"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "SOIC*5.23x5.23mm*P1.27mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
	)
)
