(footprint "SXN_SMCM7060" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Sheetfile" "power.kicad_sch")
  (property "Sheetname" "Power")
  (property "lcsc_no" "C381615")
  (attr smd)
  (fp_text reference "T" (at -0.1 -5.025 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 0dc9976c-cb77-415e-b172-93127dad5a62)
  )
  (fp_text value "SMCM7060" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 998b321f-5fb0-4a06-b092-abfc6d2ca2ef)
  )
  (fp_line (start -3 -3.75) (end -3 3.75)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp e30852de-46c9-41f0-a3d9-8ef66086dca2))
  (fp_line (start -3 3.75) (end -2.75 3.75)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 4223c2a6-1e18-449e-b0db-7d5b50dc35f8))
  (fp_line (start -2.75 -3.75) (end -3 -3.75)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 01b02b1d-a148-4b4b-948e-18cefc661921))
  (fp_line (start -0.5 -3.75) (end 0.5 -3.75)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp f7afb3b7-8d8f-4b52-bd1d-a3b4dd204f23))
  (fp_line (start -0.5 3.75) (end 0.5 3.75)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 7ba124e3-fe22-4f69-a67f-e203f053af6f))
  (fp_line (start 3 -3.75) (end 2.75 -3.75)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 493dccf6-d92a-44bb-884f-db0b989b22f6))
  (fp_line (start 3 3.75) (end 2.75 3.75)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 4c582148-65df-43c2-876f-5efdcd86aaf3))
  (fp_line (start 3 3.75) (end 3 -3.75)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 3b9d8230-9e65-4fe0-aee6-a17b8634d913))
  (fp_line (start -3.25 -4.25) (end -3.25 4.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fe30de92-a111-4bdd-b978-5e437d4afc94))
  (fp_line (start -3.25 4.25) (end 3.25 4.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 55d08cb5-567c-4464-9bf5-de8f80222658))
  (fp_line (start 3.25 -4.25) (end -3.25 -4.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp aff6f1bc-d74b-4d4f-adc9-5617126e1b14))
  (fp_line (start 3.25 4.25) (end 3.25 -4.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp cd6c71fd-3ca9-4427-8c3b-ef26b3871295))
  (fp_line (start -3 -3.75) (end -3 3.75)
    (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp adb1773b-eca6-48ec-9a80-57b128d9b7b7))
  (fp_line (start -3 3.75) (end 3 3.75)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3d4b4c58-7a60-4eb8-a6e9-fcc8c4b12f27))
  (fp_line (start 2.25 -3.75) (end -3 -3.75)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b52e36e6-0d95-4294-8ac9-c26b2b134f71))
  (fp_line (start 3 -3) (end 2.25 -3.75)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4881435c-66bc-4751-8db2-515f78b03b6a))
  (fp_line (start 3 3.75) (end 3 -3)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 534998f0-fe39-42b1-b945-a200779bf9dd))
  (pad "1" smd roundrect (at 1.625 -2.75) (size 1.75 2.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 3f95a2f9-f126-4f12-9a10-750a89c1f5ff))
  (pad "2" smd roundrect (at -1.625 -2.75) (size 1.75 2.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 40dea0d2-46d2-456a-b951-36d94e5da07b))
  (pad "3" smd roundrect (at -1.625 2.75) (size 1.75 2.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 2eba5251-c7e3-4105-9639-654b9d2e0a83))
  (pad "4" smd roundrect (at 1.625 2.75) (size 1.75 2.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 27da5741-8de0-4edb-808e-f59fb1fd1c73))
  (model "${TJ_LIB}/3d/ACM7060.STEP"
    (offset (xyz 3 -3.5 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 -90))
  )
)
