(module SuperCap_V_Type_d11.5mm_p4.5mm (layer F.Cu) (tedit 5D4E16C8)
  (fp_text reference REF** (at -0.25 -7) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SuperCap_V_Type_d11.5mm_p4.5mm (at 0 -0.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.25 -6) (end 2.25 -6) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.25 -6) (end 2.25 -1.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.25 -6) (end -2.25 -1.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.25 6) (end -2.25 6) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.25 6) (end -2.25 1.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.25 6) (end 2.25 1.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.8 -5.4) (end -2.8 -4.6) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.2 -5) (end -2.4 -5) (layer F.SilkS) (width 0.12))
  (pad 1 thru_hole circle (at -2.25 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 2.25 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask))
)
