(module Fuse_L8.5mm_W4.0mm_P5.08mm (layer F.Cu) (tedit 5E9442E1)
  (descr "Fuse, 2010 Series / 8.5x8.5x4mm (Square) / Time-Lag Type,http://www.walterfuse.com/pdf/subminiature/subminiature_2010.pdf")
  (tags "2010 Series ,8.5x8.5x4mm (Square) / Time-Lag Type,walterfuse")
  (fp_text reference REF** (at 0 -3.34) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Fuse_L8.5mm_W4.0mm_P5.08mm (at 2.45 3.25) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -4.4 2.15) (end 4.42 2.15) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.42 -2.15) (end 4.42 2.15) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.4 -2.15) (end -4.4 2.15) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.4 -2.15) (end 4.42 -2.15) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.5 2.25) (end 4.52 2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.52 -2.25) (end 4.52 2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.5 -2.25) (end -4.5 2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.5 -2.25) (end 4.52 -2.25) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -4.25 -2) (end 4.27 -2) (layer F.Fab) (width 0.1))
  (fp_line (start -4.25 2) (end 4.27 2) (layer F.Fab) (width 0.1))
  (fp_line (start -4.25 -2) (end -4.25 2) (layer F.Fab) (width 0.1))
  (fp_line (start 4.27 -2) (end 4.27 2) (layer F.Fab) (width 0.1))
  (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -2.54 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_BelFuse_0ZRE_0ZRE0012FF_L8.3mm_W3.8mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
