(module SuperCap_V_Type_d18.7mm_p5mm (layer F.Cu) (tedit 5D4E157C)
  (fp_text reference REF** (at -0.5 -10.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SuperCap_V_Type_d18.7mm_p5mm (at 0 -0.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3.7 -8) (end -2.9 -8) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.3 -8.4) (end -3.3 -7.6) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.5 -9.5) (end -2.5 -2) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.5 -9.5) (end 2.5 -2) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.5 -9.5) (end 2.5 -9.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.5 9.5) (end -2.5 9.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.5 9.5) (end -2.5 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.5 9.5) (end 2.5 2) (layer F.SilkS) (width 0.12))
  (pad 2 thru_hole circle (at 2.5 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -2.5 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
)
