(module MORNSUN-VRB_YMD-6W (layer F.Cu) (tedit 5F1AC013)
  (descr "(https://www.mornsun.cn/html/pdf/VRB2405YMD-6WR3.html)")
  (fp_text reference REF** (at 0 0.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value MORNSUN-VRB_YMD-6W (at 0 -0.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -13.208 13.208) (end -13.208 -13.208) (layer F.Fab) (width 0.12))
  (fp_line (start 13.208 13.208) (end -13.208 13.208) (layer F.Fab) (width 0.12))
  (fp_line (start 13.208 -13.208) (end 13.208 13.208) (layer F.Fab) (width 0.12))
  (fp_line (start -13.208 -13.208) (end 13.208 -13.208) (layer F.Fab) (width 0.12))
  (fp_line (start -12.7 12.7) (end -12.7 -12.7) (layer F.CrtYd) (width 0.12))
  (fp_line (start 12.7 12.7) (end -12.7 12.7) (layer F.CrtYd) (width 0.12))
  (fp_line (start 12.7 -12.7) (end 12.7 12.7) (layer F.CrtYd) (width 0.12))
  (fp_line (start 4.064 -12.7) (end 12.7 -12.7) (layer F.CrtYd) (width 0.12))
  (fp_line (start 2.54 -11.176) (end 4.064 -12.7) (layer F.CrtYd) (width 0.12))
  (fp_line (start 1.016 -12.7) (end 2.54 -11.176) (layer F.CrtYd) (width 0.12))
  (fp_line (start -12.7 -12.7) (end 1.016 -12.7) (layer F.CrtYd) (width 0.12))
  (fp_line (start -12.7 12.7) (end -12.7 -12.7) (layer F.SilkS) (width 0.12))
  (fp_line (start -12.7 -12.7) (end 12.7 -12.7) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.7 -12.7) (end 12.7 12.7) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.7 12.7) (end -12.7 12.7) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.16 -12.954) (end 12.954 -12.954) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.954 -12.954) (end 12.954 -10.16) (layer F.SilkS) (width 0.12))
  (pad 1 thru_hole circle (at 2.54 -10.16) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -2.54 -10.16) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -10.16 10.16) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 0 10.16) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 10.16 10.16) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
)
