(module MountingHole_3.2x4.3mm_S5.0x6.0mm (layer F.Cu) (tedit 5E7F6AFE)
  (descr "Mounting Hole 3.2x4.3mm, no annular, M3,silk 5.0x6.0mm")
  (tags "mounting hole 3.2x4.3mm no annular m3")
  (attr virtual)
  (fp_text reference REF** (at 0 -4.2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value MountingHole_3.2x4.3mm_S5.0x6.0mm (at 0 4.2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0.3 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_arc (start -0.5 0) (end -0.5 -2.5) (angle -180) (layer F.SilkS) (width 0.15))
  (fp_arc (start 0.5 0) (end 0.5 2.5) (angle -180) (layer F.SilkS) (width 0.15))
  (fp_arc (start -0.5 0) (end -0.5 -2.6) (angle -180) (layer F.CrtYd) (width 0.05))
  (fp_arc (start 0.5 0) (end 0.5 2.6) (angle -180) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.5 -2.6) (end 0.5 -2.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.5 2.6) (end -0.5 2.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.5 -2.5) (end 0.5 -2.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.5 2.5) (end -0.5 2.5) (layer F.SilkS) (width 0.15))
  (pad "" np_thru_hole oval (at 0 0) (size 4.3 3.2) (drill oval 4.3 3.2) (layers *.Cu *.Mask))
)
