(module FUSE-TH_BD4.0-L11.0-P15.00-D0.6 (layer F.Cu) (tedit 5E6F4342)
  (descr "SunFuse Ceramic Slow Blow Fuse 6H_6HP.PDF")
  (tags "UL/CSA 6x32mm Ceramic Slow Blow Fuse")
  (fp_text reference REF** (at -0.3 3.2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value FUSE-TH_BD4.0-L11.0-P15.00-D0.6 (at 0.3 -0.3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -5.6 2.1) (end 5.6 2.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 5.6 2.1) (end 5.6 -2.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -5.6 -2.1) (end -5.6 2.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -5.6 -2.1) (end 5.6 -2.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -8.8 2.3) (end 8.8 2.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 8.8 2.3) (end 8.8 -2.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start -8.8 -2.3) (end -8.8 2.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start -8.8 -2.3) (end 8.8 -2.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.6 -2.1) (end -5.6 2.1) (layer F.Fab) (width 0.1))
  (fp_line (start -5.6 -2.1) (end -4 -2.1) (layer F.Fab) (width 0.1))
  (fp_line (start -5.6 2.1) (end -4 2.1) (layer F.Fab) (width 0.1))
  (fp_text user %R (at 0 0.2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -4 -2.1) (end -4 2.1) (layer F.Fab) (width 0.1))
  (fp_line (start 4 -1.8) (end -4 -1.8) (layer F.Fab) (width 0.1))
  (fp_line (start 4 1.8) (end -4 1.8) (layer F.Fab) (width 0.1))
  (fp_line (start -6.1 0) (end -3.5 0) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.5 0) (end 6.2 0) (layer F.SilkS) (width 0.15))
  (fp_line (start -7.5 0) (end -5.6 0) (layer F.Fab) (width 0.1))
  (fp_line (start 5.6 2.1) (end 4 2.1) (layer F.Fab) (width 0.1))
  (fp_line (start 4 2.1) (end 4 -2.1) (layer F.Fab) (width 0.1))
  (fp_line (start 5.6 2.1) (end 5.6 -2.1) (layer F.Fab) (width 0.1))
  (fp_line (start 7.5 0) (end 5.6 0) (layer F.Fab) (width 0.1))
  (fp_line (start 5.6 -2.1) (end 4 -2.1) (layer F.Fab) (width 0.1))
  (fp_arc (start -1.75 0) (end 0 0) (angle -180) (layer F.SilkS) (width 0.15))
  (fp_arc (start 1.75 0) (end 0 0) (angle -180) (layer F.SilkS) (width 0.15))
  (pad 2 thru_hole circle (at 7.5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -7.5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_SunFuse-6HP.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
