(footprint "Jushuo_AFC07-S45FCA-00"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "FFC / FPC 插座，间距:0.5mm P数:45P 抽屉式 下接")
	(property "Reference" "REF**"
		(at 0 -4.65 0)
		(layer "F.SilkS")
		(uuid "94e9c6ab-eb69-4817-944d-1e91f3b57f1e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Jushuo_AFC07-S45FCA-00"
		(at 0 3.45 0)
		(layer "F.Fab")
		(uuid "ffe1923f-dbfd-46a8-bfa8-274438652b81")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://item.szlcsc.com/datasheet/AFC07-S45FCA-00/253882.html"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "b1f924bd-bbfa-4a8b-a317-6315dc075bf6")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "70afc52a-d408-46d2-b136-275f65b4f7cd")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -14.45 0.64)
		(end -14 0.64)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0c14e3ef-90d2-4b95-b823-05a6be8fbb02")
	)
	(fp_line
		(start -14.45 2.36)
		(end -14.45 0.64)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9e349ab6-eb6c-414d-8515-d3bbd86ee12e")
	)
	(fp_line
		(start -14 -3.01)
		(end -12.41 -3.01)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0fc0adbb-6757-4e19-a743-3504d0b5f707")
	)
	(fp_line
		(start -14 0.64)
		(end -14 -3.01)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "73fbf7c6-2379-4a32-be19-6206beede0d9")
	)
	(fp_line
		(start 11.41 -3.01)
		(end 14 -3.01)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "51fbdab3-9c90-4862-8a6c-8a3e6f21e062")
	)
	(fp_line
		(start 14 -3.01)
		(end 14 0.64)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1aa3ee39-d1c7-4193-ac6b-5e5b7760aac8")
	)
	(fp_line
		(start 14 0.64)
		(end 14.45 0.64)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "20f37b9e-fa95-4317-b737-240dd9b2834b")
	)
	(fp_line
		(start 14.45 0.64)
		(end 14.45 2.36)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1dd8ff09-8832-4416-8c0a-6c4d760bd714")
	)
	(fp_line
		(start 14.45 2.36)
		(end -14.45 2.36)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "cc99c54f-2622-4af2-94a3-12f7acbc36e0")
	)
	(fp_poly
		(pts
			(xy -11.47 -2.9) (xy -11.8 -2.66) (xy -11.8 -3.14)
		)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill yes)
		(layer "F.SilkS")
		(uuid "002fbe14-656e-4b80-9470-3bc51b728ed0")
	)
	(fp_rect
		(start -14.7 -3.95)
		(end 14.7 2.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "3ee5a316-4867-4748-a52d-a50900cd445b")
	)
	(fp_line
		(start -14.05 0.75)
		(end -13.65 0.75)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "09bd0c43-9fab-4949-8841-9f66958cf4ad")
	)
	(fp_line
		(start -14.05 2.25)
		(end -14.05 0.75)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "09fc26c0-0522-43ec-8b69-44b809cb6151")
	)
	(fp_line
		(start -13.65 -2.25)
		(end 13.65 -2.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "132b4cd9-4a90-4b31-9f08-98d2d27c5b43")
	)
	(fp_line
		(start -13.65 0.75)
		(end -13.65 -2.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5b08fc63-f6d2-42fd-b1c2-b11d09a47c1f")
	)
	(fp_line
		(start -11.5 -2.25)
		(end -11 -1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b138b15d-f6a3-4c71-8879-a2a3d23b8b8d")
	)
	(fp_line
		(start -11 -1.25)
		(end -10.5 -2.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "39e61045-4e7d-4cb9-a080-0cc6a39447bc")
	)
	(fp_line
		(start 13.65 -2.25)
		(end 13.65 0.75)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ca5d6618-f168-44d9-a693-b785b1d87257")
	)
	(fp_line
		(start 13.65 0.75)
		(end 14.05 0.75)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d58692e0-b246-4886-9bcb-25a22e333a26")
	)
	(fp_line
		(start 14.05 0.75)
		(end 14.05 2.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f12ddc43-7d2a-4185-8f43-9eb4689fa308")
	)
	(fp_line
		(start 14.05 2.25)
		(end -14.05 2.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "de75c26f-734f-4330-882f-f3020765e5d9")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "7889d1cc-47da-47d9-970c-3df7b16951fe")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -11 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "9e2b04dd-6246-43f5-aabe-d35fddc50417")
	)
	(pad "2" smd roundrect
		(at -10.5 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "a07d0c94-100f-4af1-81ad-dd43d95fc82f")
	)
	(pad "3" smd roundrect
		(at -10 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "facd41a3-4d67-4fd9-aa7f-400a454df548")
	)
	(pad "4" smd roundrect
		(at -9.5 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "952a6fb6-b02b-41f3-b18a-56cd667d05d8")
	)
	(pad "5" smd roundrect
		(at -9 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "5171b022-fca2-46d0-b815-87fd4b9f33e4")
	)
	(pad "6" smd roundrect
		(at -8.5 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "92329735-988c-4779-9340-0655354c54c9")
	)
	(pad "7" smd roundrect
		(at -8 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "b7bcf03a-8448-4d2d-999e-a08eb3640f75")
	)
	(pad "8" smd roundrect
		(at -7.5 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "7e6d47fe-c943-4ade-8bf3-f66f456aef8d")
	)
	(pad "9" smd roundrect
		(at -7 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "707c52ce-d238-4bd1-9d90-efa1364ce3b9")
	)
	(pad "10" smd roundrect
		(at -6.5 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "6a032803-d745-467b-a414-b2f1526fc82e")
	)
	(pad "11" smd roundrect
		(at -6 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "01971479-3732-48ed-b0a0-e9eb8d256490")
	)
	(pad "12" smd roundrect
		(at -5.5 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "d367e415-e037-4276-b133-ac7ada63f078")
	)
	(pad "13" smd roundrect
		(at -5 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "a449bad7-065a-4ff6-a3d1-10f71cb8478f")
	)
	(pad "14" smd roundrect
		(at -4.5 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "0a626766-8d49-4f3f-8b26-a024687264a5")
	)
	(pad "15" smd roundrect
		(at -4 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "b124ed2e-7a73-42dd-9000-5f8e4794f829")
	)
	(pad "16" smd roundrect
		(at -3.5 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "fefd7b88-898e-41e7-b2b8-ab09d64dd534")
	)
	(pad "17" smd roundrect
		(at -3 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "360c7b52-305b-4a3c-9002-2d7f565c42ae")
	)
	(pad "18" smd roundrect
		(at -2.5 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "f7fe5804-4334-436b-80d9-f1a2b4fa5ae9")
	)
	(pad "19" smd roundrect
		(at -2 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "666f2862-3ab5-4d4e-8834-01bfe5011612")
	)
	(pad "20" smd roundrect
		(at -1.5 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "e05c1ca8-10a3-485e-9154-24af6117bbf0")
	)
	(pad "21" smd roundrect
		(at -1 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "68318562-0ce5-450f-b7a0-4e0ad51e0ba1")
	)
	(pad "22" smd roundrect
		(at -0.5 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "56e28a30-c89d-409b-97ae-2bdfe9450f25")
	)
	(pad "23" smd roundrect
		(at 0 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "13c26369-5bc0-4abb-befa-4304a20a2149")
	)
	(pad "24" smd roundrect
		(at 0.5 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "71661a78-f9c9-4bb3-95f8-7445d5bc0aac")
	)
	(pad "25" smd roundrect
		(at 1 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "4be4a3e9-bc2e-4dc9-8ce7-5f0cc5ef6f0e")
	)
	(pad "26" smd roundrect
		(at 1.5 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "a6972418-a854-49ad-93c8-0ca86d3c8320")
	)
	(pad "27" smd roundrect
		(at 2 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "40c94e13-06c8-48e1-857c-dd5c7413fb2e")
	)
	(pad "28" smd roundrect
		(at 2.5 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "e209a0b6-b4b7-4f87-a890-60c55d018287")
	)
	(pad "29" smd roundrect
		(at 3 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "59c38c32-f72c-420a-80db-3e011d5dc0be")
	)
	(pad "30" smd roundrect
		(at 3.5 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "bc9f247f-7706-45d5-b131-d2f7452979a3")
	)
	(pad "31" smd roundrect
		(at 4 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "27df7cdc-d4ce-4f84-8761-eac9ed1eb740")
	)
	(pad "32" smd roundrect
		(at 4.5 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "d6fdb309-45f9-4197-90cd-734a5e0d42e2")
	)
	(pad "33" smd roundrect
		(at 5 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "ec172afd-bd0c-484c-90d5-1ff1522c99e1")
	)
	(pad "34" smd roundrect
		(at 5.5 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "09fe2395-b353-4246-a44e-51a0910e0553")
	)
	(pad "35" smd roundrect
		(at 6 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "6a1e96d4-00ff-4fbd-86e8-f1e86ca69aac")
	)
	(pad "36" smd roundrect
		(at 6.5 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "b48dab5d-5e1f-4f2d-8a36-239edcd30427")
	)
	(pad "37" smd roundrect
		(at 7 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "33d6f6c5-492a-4b73-a98b-fec9514f8e22")
	)
	(pad "38" smd roundrect
		(at 7.5 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "a7c15968-0993-4023-81ea-4eba385aa927")
	)
	(pad "39" smd roundrect
		(at 8 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "329ee6af-50b4-46e4-92e6-ea3016b8aac2")
	)
	(pad "40" smd roundrect
		(at 8.5 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "c8aa531e-c2b4-4111-b1b0-6689d3cd8b0a")
	)
	(pad "41" smd roundrect
		(at 9 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "657ee377-f823-49c5-98d3-4301cfdbed95")
	)
	(pad "42" smd roundrect
		(at 9.5 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "61058b07-5685-4757-ba1c-11ebe2bfff87")
	)
	(pad "43" smd roundrect
		(at 10 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "f0a26661-7f6b-4056-ad59-ad5650001274")
	)
	(pad "44" smd roundrect
		(at 10.5 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "939738e5-16c3-446a-b0f9-1fd481e6621b")
	)
	(pad "45" smd roundrect
		(at 11 -2.9)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "e18602d6-80c2-4c4f-8e1c-bc7f5ed548fd")
	)
	(pad "MP" smd roundrect
		(at -12.6 -0.73)
		(size 2.2 3.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "5ecfb845-fc7e-4550-9bc4-52a839813135")
	)
	(pad "MP" smd roundrect
		(at 12.6 -0.73)
		(size 2.2 3.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "66f4663f-19e6-4c5a-a7cd-c0dc69953733")
	)
	(embedded_fonts no)
)
