(footprint "Relay_SPST_YongNeng_YX201T"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Miniature PCB Relay, PCH Series, 1 Form A (NO), SPST ")
	(tags "Relay SPST NO")
	(property "Reference" "REF**"
		(at 9.5 -2 0)
		(layer "F.SilkS")
		(uuid "6278444c-2ac2-43f3-a816-212ed23bcdae")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Relay_SPST_YongNeng_YX201T"
		(at 9 10 0)
		(layer "F.Fab")
		(uuid "3d535d40-e297-40d4-b704-73a0e4313d9c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://www.ynjdq.com/uploadfiles/2021/07/20210707094927697.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3fb95db5-ab78-4199-b904-f50f5951e97b")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9a006ef1-5e49-44bb-849f-c72a7d1c9167")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -1.17 1.35)
		(end -1.17 6.9)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "70c934e2-2d84-44bd-8c80-4a209700ba90")
	)
	(fp_line
		(start -1.17 8.29)
		(end -1.17 8.92)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6fc56aef-b49f-497d-8dda-e327aa76e2be")
	)
	(fp_line
		(start -0.33 8.92)
		(end -1.17 8.92)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d4c30d84-3866-4cb5-b645-69dedc9d00a7")
	)
	(fp_line
		(start 2.44 0)
		(end 3.71 0)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f2df18db-cf5f-4a33-8b5d-a738d520b856")
	)
	(fp_line
		(start 2.44 1.27)
		(end 3.71 1.27)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "10bf774a-7c40-4087-8764-5bbba7b1964f")
	)
	(fp_line
		(start 2.44 2.54)
		(end 4.98 3.81)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4c10f05f-da42-4b28-99bf-8d9535c3c059")
	)
	(fp_line
		(start 2.44 6.35)
		(end 2.44 1.27)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7a547e06-d47d-402f-985a-8d54eb8ed98e")
	)
	(fp_line
		(start 3.71 0)
		(end 3.71 1.27)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "853abb48-f197-459f-8ca9-e607173fb498")
	)
	(fp_line
		(start 3.71 1.27)
		(end 4.98 1.27)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7f363e14-d1ff-491b-a7e8-8945dcac1d66")
	)
	(fp_line
		(start 3.71 6.35)
		(end 3.71 7.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1d1a4b7d-6e82-4200-afa4-f6f16b72c1f9")
	)
	(fp_line
		(start 3.71 7.6)
		(end 2.44 7.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d8503f4b-4286-443a-b340-478654cc37a7")
	)
	(fp_line
		(start 4.98 1.27)
		(end 4.98 6.35)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "892b0312-91dd-4bdc-a73b-c2d50e211a15")
	)
	(fp_line
		(start 4.98 6.35)
		(end 2.44 6.35)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4e70e83f-e0ec-42a1-b0f4-a3067b094338")
	)
	(fp_line
		(start 9.46 8.92)
		(end -0.33 8.92)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e892c8ae-7235-4493-be49-d559c346bb6b")
	)
	(fp_line
		(start 12.4 2.9)
		(end 12.7 2.9)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "5b78eefb-9950-47cb-b780-45036b68cd6f")
	)
	(fp_line
		(start 12.7 0)
		(end 13.7 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "8da06410-d548-480c-b9c1-0cf06bb762a9")
	)
	(fp_line
		(start 12.7 2.9)
		(end 12.7 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "38f4a0bf-7dbe-4bd6-be3c-853b183925b0")
	)
	(fp_line
		(start 12.7 5.1)
		(end 11.8 2.7)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "ead6f06e-4103-43dc-814a-4b5616e6ae4c")
	)
	(fp_line
		(start 12.7 5.8)
		(end 12.7 5.1)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "57067341-bb4a-45f1-8c22-8d1acef0c131")
	)
	(fp_line
		(start 17.3 -1.32)
		(end -1.17 -1.32)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "382da467-8c1e-47e7-b15d-0b28081146fc")
	)
	(fp_line
		(start 17.3 -1.32)
		(end 17.3 8.92)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "557392ae-14b5-4707-924e-1ff685de833e")
	)
	(fp_line
		(start 17.3 8.92)
		(end 9.5 8.92)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "29a9de27-220f-4e3c-9b99-81262e511cf4")
	)
	(fp_line
		(start -1.35 -1.45)
		(end 17.5 -1.45)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "6f7bb853-e93b-43f7-bc1b-178e623c7098")
	)
	(fp_line
		(start -1.35 9.1)
		(end -1.35 -1.45)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ad3408c5-d077-456a-b5ba-e95da64d05e4")
	)
	(fp_line
		(start 17.5 -1.45)
		(end 17.5 9.1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ee089f5a-9c29-462b-8d27-b28c9fa91192")
	)
	(fp_line
		(start 17.5 9.1)
		(end -1.35 9.1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c9fa0f50-83c8-4c03-a6fb-282cd7cf6893")
	)
	(fp_line
		(start -1.05 8.8)
		(end -1.05 -0.2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3d0f65f6-4c22-42f3-a603-f8fc6b93cce0")
	)
	(fp_line
		(start -0.05 -1.2)
		(end -1.05 -0.2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2a5867b7-6ce2-4c61-9295-0699da857abc")
	)
	(fp_line
		(start -0.05 -1.2)
		(end 17.2 -1.2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b6e1a717-83a8-47fa-b0fd-0fc2bc5c1cdb")
	)
	(fp_line
		(start 0 1.8)
		(end 0 5.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "cd1e1b39-e5db-4bb2-9cec-e27d76e12ce5")
	)
	(fp_line
		(start 17.2 -1.2)
		(end 17.2 8.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e090d89d-22fe-4a8f-8db0-109f24e60c45")
	)
	(fp_line
		(start 17.2 8.8)
		(end -1.05 8.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6feeefac-4c40-4e99-aae7-be290fce5f2a")
	)
	(fp_text user "${REFERENCE}"
		(at 8.95 3.8 0)
		(layer "F.Fab")
		(uuid "61598fb1-e511-4268-a57a-7236839ef7f6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 7.6)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "dd8d7e61-c042-49e3-8eda-fb2c2f7346b1")
	)
	(pad "2" thru_hole circle
		(at 12.7 7.3)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5b67e6c2-6d5a-4e20-a775-5e62450aafbd")
	)
	(pad "3" thru_hole circle
		(at 15.24 0)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8a5b1e18-9694-4626-9492-809c689120d0")
	)
	(pad "4" thru_hole roundrect
		(at 0 0)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.155)
		(uuid "ed08de31-a85c-40ff-94d5-f449711a5ec2")
	)
	(embedded_fonts no)
	(model "${KICAD8_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPST_TE_PCH-1xxx2M.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
