(footprint "FuseClip-D5xL20mm_PAD6.5x5.7mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Fuseholder Clips, 5x20mm Cylinder Fuse, Pins Inline, Horizontal, Eaton 1A5601-01, https://www.eaton.com/content/dam/eaton/products/electronic-components/resources/data-sheet/eaton-1axxxx-pcb-fuse-clips-atc-atm-blade-data-sheet.pdf")
	(tags "fuse clip open")
	(property "Reference" "REF**"
		(at 0.42 4.5 180)
		(layer "F.SilkS")
		(uuid "b9e0ba15-f372-4a9e-a627-d594778258ac")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "FuseClip-D5xL20mm_PAD6.5x5.7mm"
		(at 0.9 4.7 0)
		(layer "F.Fab")
		(uuid "d28c26df-aeff-4f6a-a1dc-f734efaf55cb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://item.szlcsc.com/datasheet/XF-003/757626.html"
		(at 10.7 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6721f08a-e021-4861-9d54-a3f07c0c146b")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "FuseClip,保险丝夹,单位: 对"
		(at 10.7 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3850200d-4883-4e4b-bdb0-7c9df0e1288b")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -10.5 -3.6)
		(end -10.5 -1.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5df2425f-8567-4048-bb60-d1dff0435978")
	)
	(fp_line
		(start -10.5 3.6)
		(end -10.5 1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "22a2b377-b7c4-4175-9181-bb2eb268c635")
	)
	(fp_line
		(start -5.3 -3.6)
		(end -10.5 -3.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "640c939a-8ffb-4030-be52-a3c55dc2504d")
	)
	(fp_line
		(start -5.3 -3.6)
		(end -5.3 -1.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3b89d3a4-2a7d-44c8-9def-f40efe39b408")
	)
	(fp_line
		(start -5.3 -2.5)
		(end 5.3 -2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "16cf57f1-17a7-4e92-bfd1-4ac233a7ec47")
	)
	(fp_line
		(start -5.3 2.5)
		(end 5.3 2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9ffb66cc-9603-4475-aa59-43d92d592c9a")
	)
	(fp_line
		(start -5.3 3.6)
		(end -10.5 3.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "de8b5861-f67f-45f2-aac3-be9ea77d2473")
	)
	(fp_line
		(start -5.3 3.6)
		(end -5.3 1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "320335e2-ef03-47a9-9aac-87ad9f7cdc71")
	)
	(fp_line
		(start -3.5 0)
		(end 3.5 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "f9d7a98f-8617-4aa8-b6f6-cce6f6e59b7a")
	)
	(fp_line
		(start 5.3 -3.6)
		(end 5.3 -1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9256f7aa-4f1a-4001-bdef-7fbb32e451e0")
	)
	(fp_line
		(start 5.3 -3.6)
		(end 10.5 -3.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7eebb937-5634-42da-bd7e-2e0260369d0e")
	)
	(fp_line
		(start 5.3 3.6)
		(end 5.3 1.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "106f01f3-bf47-4150-bb7b-1a3318a6eb3d")
	)
	(fp_line
		(start 5.3 3.6)
		(end 10.5 3.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "537c2196-fe60-48a5-847c-84653e479b38")
	)
	(fp_line
		(start 10.5 -3.6)
		(end 10.5 -1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "be0c7a50-2d41-4fd6-8c28-37a4cf00d900")
	)
	(fp_line
		(start 10.5 3.6)
		(end 10.5 1.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "10ddf54c-6d59-4755-8fb8-43466141a83a")
	)
	(fp_line
		(start -12.2 -3.8)
		(end -12.2 3.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "128b5646-b490-4a46-92e6-dc9019afc845")
	)
	(fp_line
		(start -12.2 -3.8)
		(end 12.2 -3.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "bb074203-ccaa-438b-8d34-1fcc6b4329dd")
	)
	(fp_line
		(start -12.2 3.8)
		(end 12.2 3.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "7eb44f52-f1c4-4f72-82e3-95857a1deb48")
	)
	(fp_line
		(start 12.2 3.8)
		(end 12.2 -3.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "57e128ae-5e07-4818-9f5a-1cee0e65c680")
	)
	(fp_line
		(start -10.5 -3.6)
		(end -5.3 -3.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "305223db-b8da-41f0-95bc-5cbc190042f9")
	)
	(fp_line
		(start -10.5 3.6)
		(end -10.5 -3.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "cf98d80d-88c0-49bf-9255-0bae3b0226e5")
	)
	(fp_line
		(start -5.3 -3.6)
		(end -5.3 3.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "aec430eb-8777-4493-afb6-cb21a2aec738")
	)
	(fp_line
		(start -5.3 -2.5)
		(end 5.3 -2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f6725402-316f-4351-badd-26f7d17d7385")
	)
	(fp_line
		(start -5.3 2.5)
		(end 5.3 2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "cfbe7435-202f-4ad8-a192-7655ca678c5b")
	)
	(fp_line
		(start -5.3 3.6)
		(end -10.5 3.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "90f88726-4cd8-4616-8da9-81b053b7a2c3")
	)
	(fp_line
		(start 5.3 -3.6)
		(end 10.5 -3.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "bc2b91cd-dad2-489e-a5a6-c25b0772eb90")
	)
	(fp_line
		(start 5.3 3.6)
		(end 5.3 -3.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a64a7c06-7057-47f9-be64-f537af3193b4")
	)
	(fp_line
		(start 10.5 -3.6)
		(end 10.5 3.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9ade8aaa-dfca-436d-be8a-be74784ef565")
	)
	(fp_line
		(start 10.5 3.6)
		(end 5.3 3.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c884feb5-afbc-4baf-9f12-868c0ed27bc9")
	)
	(fp_text user "${REFERENCE}"
		(at 10.4 0 0)
		(layer "F.Fab")
		(uuid "006bc43b-d3a8-4a38-a8dc-5a24da3f9b4d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole roundrect
		(at -10.5 0)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
		(uuid "d2cd873e-b7e4-4462-907f-8566e0148f34")
	)
	(pad "1" thru_hole roundrect
		(at -5.3 0)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
		(uuid "b58f977f-0c3d-4fc2-9fb8-ea33924b39a1")
	)
	(pad "2" thru_hole roundrect
		(at 5.3 0 180)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
		(uuid "6c55033c-55b9-4835-9ab8-f334f8a3ffed")
	)
	(pad "2" thru_hole roundrect
		(at 10.5 0 180)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
		(uuid "f0d59009-bdb6-4150-8249-d2a9c5928391")
	)
	(embedded_fonts no)
	(model "${KICAD8_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Clip-5x20mm_Eaton_1A5601-01_Inline_P20.80x6.76mm_D1.70mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
