(footprint "FuseClip-D6.0xL30mm_PAD8.0x7.7mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Fuseholder Clips, 6.0x30mm Cylinder Fuse,")
	(tags "fuse clip open")
	(property "Reference" "REF**"
		(at 0.42 4.5 180)
		(layer "F.SilkS")
		(uuid "b9e0ba15-f372-4a9e-a627-d594778258ac")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "FuseClip-D6.0xL30mm_PAD8.0x7.7mm"
		(at 2.5 1.8 0)
		(layer "F.Fab")
		(uuid "d28c26df-aeff-4f6a-a1dc-f734efaf55cb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://item.szlcsc.com/datasheet/XF-007/757627.html"
		(at 10.7 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6721f08a-e021-4861-9d54-a3f07c0c146b")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 10.7 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3850200d-4883-4e4b-bdb0-7c9df0e1288b")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -16.3 -2)
		(end -16.3 -4.1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "42ac6b07-7c05-4b38-8778-6cc6048983ec")
	)
	(fp_line
		(start -16.3 4.1)
		(end -16.3 2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7e618d3c-669f-4521-b0f6-41cc0e49b7d9")
	)
	(fp_line
		(start -9.1 -4.1)
		(end -16.3 -4.1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6411d096-017c-455a-a4f3-1e489e7c44ad")
	)
	(fp_line
		(start -9.1 -2)
		(end -9.1 -4.1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a7bb5773-6009-4749-bb68-766c6ebe8c3f")
	)
	(fp_line
		(start -9.1 4.1)
		(end -16.3 4.1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0632a49e-3116-4f64-a587-64b928435e5b")
	)
	(fp_line
		(start -9.1 4.1)
		(end -9.1 2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f185921b-0c12-48dc-8340-be03be1c6910")
	)
	(fp_line
		(start -7 0)
		(end 0 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "df57b108-4e91-4486-b57f-d037d000a8bf")
	)
	(fp_line
		(start 0 -3)
		(end -9.1 -3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7d5c4cfd-83bb-446f-ae03-b1cd31abc953")
	)
	(fp_line
		(start 0 -3)
		(end 9.1 -3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ed265626-f6f5-4029-beb9-f6ad275e86b5")
	)
	(fp_line
		(start 0 3)
		(end -9.1 3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c2aa0d9a-ee05-49af-ab0f-4b8ccb42a51b")
	)
	(fp_line
		(start 0 3)
		(end 9.1 3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "26769327-3160-41f1-82e7-11d5d542abde")
	)
	(fp_line
		(start 8 0)
		(end 0 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "8280c306-c9f1-42ce-b369-a4f9d2d7874b")
	)
	(fp_line
		(start 9.1 -4.1)
		(end 9.1 -2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9256f7aa-4f1a-4001-bdef-7fbb32e451e0")
	)
	(fp_line
		(start 9.1 -4.1)
		(end 16.3 -4.1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7eebb937-5634-42da-bd7e-2e0260369d0e")
	)
	(fp_line
		(start 9.1 2)
		(end 9.1 4.1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "106f01f3-bf47-4150-bb7b-1a3318a6eb3d")
	)
	(fp_line
		(start 9.1 4.1)
		(end 16.3 4.1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "537c2196-fe60-48a5-847c-84653e479b38")
	)
	(fp_line
		(start 16.3 -4.1)
		(end 16.3 -2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "be0c7a50-2d41-4fd6-8c28-37a4cf00d900")
	)
	(fp_line
		(start 16.3 2)
		(end 16.3 4.1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "10ddf54c-6d59-4755-8fb8-43466141a83a")
	)
	(fp_line
		(start -18.3 -4.4)
		(end -18.3 4.4)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "89e45c3f-92d8-468f-926e-956f2941bf2a")
	)
	(fp_line
		(start -18.3 -4.4)
		(end 0 -4.4)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "562f3826-c367-4afe-b7d8-c023b3899790")
	)
	(fp_line
		(start 0 -4.4)
		(end 18.3 -4.4)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "83fee08f-7316-4ff9-a4fd-e9a9372f4d8f")
	)
	(fp_line
		(start 0 4.4)
		(end -18.3 4.4)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d1545d95-dfed-4b27-8261-02ac144d64d7")
	)
	(fp_line
		(start 18.3 4.4)
		(end 0 4.4)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "e9862dd4-26d2-4ddd-91fc-972d848045f5")
	)
	(fp_line
		(start 18.3 4.4)
		(end 18.3 -4.4)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "57e128ae-5e07-4818-9f5a-1cee0e65c680")
	)
	(fp_line
		(start -16.3 4.1)
		(end -16.3 -4.1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "82cd9dee-6043-447b-adb3-542a442b07b8")
	)
	(fp_line
		(start -9.1 -4.1)
		(end -16.3 -4.1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "288bc800-1d5d-40e9-9cf9-ab58819ea583")
	)
	(fp_line
		(start -9.1 4.1)
		(end -16.3 4.1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "62c5b827-e2b2-4b71-8759-a284666cf692")
	)
	(fp_line
		(start -9.1 4.1)
		(end -9.1 -4.1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9a80a0f8-fdcd-41ca-ac55-a37175bcff31")
	)
	(fp_line
		(start 0 -3)
		(end -9.1 -3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "17a94511-a143-451f-b63e-35a8e42f75f2")
	)
	(fp_line
		(start 0 -3)
		(end 9.1 -3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "434de308-3c0f-471e-b2ea-4b1db61e07dc")
	)
	(fp_line
		(start 0 3)
		(end -9.1 3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a95d6a73-1cf8-48ec-b38c-387512b4e288")
	)
	(fp_line
		(start 0 3)
		(end 9.1 3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "11b49d13-b047-4242-be65-9a9b1c80ec58")
	)
	(fp_line
		(start 9.1 -4.1)
		(end 9.1 4.1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a64a7c06-7057-47f9-be64-f537af3193b4")
	)
	(fp_line
		(start 9.1 -4.1)
		(end 16.3 -4.1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "bc2b91cd-dad2-489e-a5a6-c25b0772eb90")
	)
	(fp_line
		(start 9.1 4.1)
		(end 16.3 4.1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c884feb5-afbc-4baf-9f12-868c0ed27bc9")
	)
	(fp_line
		(start 16.3 -4.1)
		(end 16.3 4.1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9ade8aaa-dfca-436d-be8a-be74784ef565")
	)
	(fp_text user "${REFERENCE}"
		(at 10.4 0 0)
		(layer "F.Fab")
		(uuid "006bc43b-d3a8-4a38-a8dc-5a24da3f9b4d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "${REFERENCE}"
		(at -10.4 0 180)
		(layer "F.Fab")
		(uuid "4f3a47cf-d409-4d6f-aebb-de65e1e470fe")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole roundrect
		(at -16.3 0)
		(size 3.5 3.5)
		(drill 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
		(uuid "43f0c683-c1ff-4ab6-8867-8a4769323ce6")
	)
	(pad "1" thru_hole roundrect
		(at -9.1 0)
		(size 3.5 3.5)
		(drill 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
		(uuid "b32e55f3-ecaa-4f51-9f63-9b4b0f015dc0")
	)
	(pad "2" thru_hole roundrect
		(at 9.1 0 180)
		(size 3.5 3.5)
		(drill 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
		(uuid "6c55033c-55b9-4835-9ab8-f334f8a3ffed")
	)
	(pad "2" thru_hole roundrect
		(at 16.3 0 180)
		(size 3.5 3.5)
		(drill 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
		(uuid "f0d59009-bdb6-4150-8249-d2a9c5928391")
	)
	(embedded_fonts no)
	(model "${KICAD8_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Clip-5x20mm_Eaton_1A5601-01_Inline_P20.80x6.76mm_D1.70mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
